From 03b83828e452418c18ba506e3e02b5deadbb53fa Mon Sep 17 00:00:00 2001
From: Jens Kuske <jenskuske@gmail.com>
Date: Tue, 27 Oct 2015 17:50:23 +0100
Subject: [PATCH] pinctrl: sunxi: Add H3 PIO controller support

The H3 uses the same pin controller as previous SoC's from Allwinner.
Add support for the pins controlled by the main PIO controller.

Signed-off-by: Jens Kuske <jenskuske@gmail.com>
Acked-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 .../bindings/pinctrl/allwinner,sunxi-pinctrl.txt   |   1 +
 drivers/pinctrl/sunxi/Kconfig                      |   4 +
 drivers/pinctrl/sunxi/Makefile                     |   1 +
 drivers/pinctrl/sunxi/pinctrl-sun8i-h3.c           | 516 +++++++++++++++++++++
 4 files changed, 522 insertions(+)
 create mode 100644 drivers/pinctrl/sunxi/pinctrl-sun8i-h3.c

--- a/Documentation/devicetree/bindings/pinctrl/allwinner,sunxi-pinctrl.txt
+++ b/Documentation/devicetree/bindings/pinctrl/allwinner,sunxi-pinctrl.txt
@@ -18,6 +18,7 @@ Required properties:
   "allwinner,sun8i-a23-r-pinctrl"
   "allwinner,sun8i-a33-pinctrl"
   "allwinner,sun8i-a83t-pinctrl"
+  "allwinner,sun8i-h3-pinctrl"
 
 - reg: Should contain the register physical address and length for the
   pin controller.
--- a/drivers/pinctrl/sunxi/Kconfig
+++ b/drivers/pinctrl/sunxi/Kconfig
@@ -51,6 +51,10 @@ config PINCTRL_SUN8I_A23_R
 	depends on RESET_CONTROLLER
 	select PINCTRL_SUNXI_COMMON
 
+config PINCTRL_SUN8I_H3
+	def_bool MACH_SUN8I
+	select PINCTRL_SUNXI_COMMON
+
 config PINCTRL_SUN9I_A80
 	def_bool MACH_SUN9I
 	select PINCTRL_SUNXI_COMMON
--- a/drivers/pinctrl/sunxi/Makefile
+++ b/drivers/pinctrl/sunxi/Makefile
@@ -13,4 +13,5 @@ obj-$(CONFIG_PINCTRL_SUN8I_A23)		+= pinc
 obj-$(CONFIG_PINCTRL_SUN8I_A23_R)	+= pinctrl-sun8i-a23-r.o
 obj-$(CONFIG_PINCTRL_SUN8I_A33)		+= pinctrl-sun8i-a33.o
 obj-$(CONFIG_PINCTRL_SUN8I_A83T)	+= pinctrl-sun8i-a83t.o
+obj-$(CONFIG_PINCTRL_SUN8I_H3)		+= pinctrl-sun8i-h3.o
 obj-$(CONFIG_PINCTRL_SUN9I_A80)		+= pinctrl-sun9i-a80.o
--- /dev/null
+++ b/drivers/pinctrl/sunxi/pinctrl-sun8i-h3.c
@@ -0,0 +1,516 @@
+/*
+ * Allwinner H3 SoCs pinctrl driver.
+ *
+ * Copyright (C) 2015 Jens Kuske <jenskuske@gmail.com>
+ *
+ * Based on pinctrl-sun8i-a23.c, which is:
+ * Copyright (C) 2014 Chen-Yu Tsai <wens@csie.org>
+ * Copyright (C) 2014 Maxime Ripard <maxime.ripard@free-electrons.com>
+ *
+ * This file is licensed under the terms of the GNU General Public
+ * License version 2.  This program is licensed "as is" without any
+ * warranty of any kind, whether express or implied.
+ */
+
+#include <linux/module.h>
+#include <linux/platform_device.h>
+#include <linux/of.h>
+#include <linux/of_device.h>
+#include <linux/pinctrl/pinctrl.h>
+
+#include "pinctrl-sunxi.h"
+
+static const struct sunxi_desc_pin sun8i_h3_pins[] = {
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 0),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "uart2"),		/* TX */
+		  SUNXI_FUNCTION(0x3, "jtag"),		/* MS */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 0)),	/* PA_EINT0 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 1),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "uart2"),		/* RX */
+		  SUNXI_FUNCTION(0x3, "jtag"),		/* CK */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 1)),	/* PA_EINT1 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 2),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "uart2"),		/* RTS */
+		  SUNXI_FUNCTION(0x3, "jtag"),		/* DO */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 2)),	/* PA_EINT2 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 3),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "uart2"),		/* CTS */
+		  SUNXI_FUNCTION(0x3, "jtag"),		/* DI */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 3)),	/* PA_EINT3 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 4),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "uart0"),		/* TX */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 4)),	/* PA_EINT4 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 5),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "uart0"),		/* RX */
+		  SUNXI_FUNCTION(0x3, "pwm0"),
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 5)),	/* PA_EINT5 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 6),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "sim"),		/* PWREN */
+		  SUNXI_FUNCTION(0x3, "pwm1"),
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 6)),	/* PA_EINT6 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 7),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "sim"),		/* CLK */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 7)),	/* PA_EINT7 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 8),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "sim"),		/* DATA */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 8)),	/* PA_EINT8 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 9),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "sim"),		/* RST */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 9)),	/* PA_EINT9 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 10),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "sim"),		/* DET */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 10)),	/* PA_EINT10 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 11),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "i2c0"),		/* SCK */
+		  SUNXI_FUNCTION(0x3, "di"),		/* TX */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 11)),	/* PA_EINT11 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 12),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "i2c0"),		/* SDA */
+		  SUNXI_FUNCTION(0x3, "di"),		/* RX */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 12)),	/* PA_EINT12 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 13),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "spi1"),		/* CS */
+		  SUNXI_FUNCTION(0x3, "uart3"),		/* TX */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 13)),	/* PA_EINT13 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 14),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "spi1"),		/* CLK */
+		  SUNXI_FUNCTION(0x3, "uart3"),		/* RX */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 14)),	/* PA_EINT14 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 15),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "spi1"),		/* MOSI */
+		  SUNXI_FUNCTION(0x3, "uart3"),		/* RTS */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 15)),	/* PA_EINT15 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 16),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "spi1"),		/* MISO */
+		  SUNXI_FUNCTION(0x3, "uart3"),		/* CTS */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 16)),	/* PA_EINT16 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 17),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "spdif"),		/* OUT */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 17)),	/* PA_EINT17 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 18),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "i2s0"),		/* SYNC */
+		  SUNXI_FUNCTION(0x3, "i2c1"),		/* SCK */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 18)),	/* PA_EINT18 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 19),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "i2s0"),		/* CLK */
+		  SUNXI_FUNCTION(0x3, "i2c1"),		/* SDA */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 19)),	/* PA_EINT19 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 20),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "i2s0"),		/* DOUT */
+		  SUNXI_FUNCTION(0x3, "sim"),		/* VPPEN */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 20)),	/* PA_EINT20 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(A, 21),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "i2s0"),		/* DIN */
+		  SUNXI_FUNCTION(0x3, "sim"),		/* VPPPP */
+		  SUNXI_FUNCTION_IRQ_BANK(0x6, 0, 21)),	/* PA_EINT21 */
+	/* Hole */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 0),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0"),		/* WE */
+		  SUNXI_FUNCTION(0x3, "spi0")),		/* MOSI */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 1),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0"),		/* ALE */
+		  SUNXI_FUNCTION(0x3, "spi0")),		/* MISO */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 2),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0"),		/* CLE */
+		  SUNXI_FUNCTION(0x3, "spi0")),		/* CLK */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 3),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0"),		/* CE1 */
+		  SUNXI_FUNCTION(0x3, "spi0")),		/* CS */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 4),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0")),	/* CE0 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 5),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0"),		/* RE */
+		  SUNXI_FUNCTION(0x3, "mmc2")),		/* CLK */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 6),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0"),		/* RB0 */
+		  SUNXI_FUNCTION(0x3, "mmc2")),		/* CMD */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 7),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0")),	/* RB1 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 8),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0"),		/* DQ0 */
+		  SUNXI_FUNCTION(0x3, "mmc2")),		/* D0 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 9),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0"),		/* DQ1 */
+		  SUNXI_FUNCTION(0x3, "mmc2")),		/* D1 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 10),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0"),		/* DQ2 */
+		  SUNXI_FUNCTION(0x3, "mmc2")),		/* D2 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 11),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0"),		/* DQ3 */
+		  SUNXI_FUNCTION(0x3, "mmc2")),		/* D3 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 12),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0"),		/* DQ4 */
+		  SUNXI_FUNCTION(0x3, "mmc2")),		/* D4 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 13),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand0"),		/* DQ5 */
+		  SUNXI_FUNCTION(0x3, "mmc2")),		/* D5 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 14),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand"),		/* DQ6 */
+		  SUNXI_FUNCTION(0x3, "mmc2")),		/* D6 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 15),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand"),		/* DQ7 */
+		  SUNXI_FUNCTION(0x3, "mmc2")),		/* D7 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(C, 16),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "nand"),		/* DQS */
+		  SUNXI_FUNCTION(0x3, "mmc2")),		/* RST */
+	/* Hole */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 0),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* RXD3 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 1),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* RXD2 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 2),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* RXD1 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 3),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* RXD0 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 4),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* RXCK */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 5),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* RXCTL/RCDV */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 6),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* RXERR */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 7),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* TXD3 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 8),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* TXD2L */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 9),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* TXD1 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 10),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* TXD0 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 11),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* CRS */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 12),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* TXCK */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 13),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* TXCTL/TXEN */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 14),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* TXERR */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 15),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* CLKIN/COL */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 16),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* MDC */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(D, 17),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "emac")),		/* MDIO */
+	/* Hole */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 0),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* PCLK */
+		  SUNXI_FUNCTION(0x3, "ts")),		/* CLK */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 1),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* MCLK */
+		  SUNXI_FUNCTION(0x3, "ts")),		/* ERR */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 2),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* HSYNC */
+		  SUNXI_FUNCTION(0x3, "ts")),		/* SYNC */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 3),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* VSYNC */
+		  SUNXI_FUNCTION(0x3, "ts")),		/* DVLD */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 4),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* D0 */
+		  SUNXI_FUNCTION(0x3, "ts")),		/* D0 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 5),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* D1 */
+		  SUNXI_FUNCTION(0x3, "ts")),		/* D1 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 6),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* D2 */
+		  SUNXI_FUNCTION(0x3, "ts")),		/* D2 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 7),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* D3 */
+		  SUNXI_FUNCTION(0x3, "ts")),		/* D3 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 8),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* D4 */
+		  SUNXI_FUNCTION(0x3, "ts")),		/* D4 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 9),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* D5 */
+		  SUNXI_FUNCTION(0x3, "ts")),		/* D5 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 10),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* D6 */
+		  SUNXI_FUNCTION(0x3, "ts")),		/* D6 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 11),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* D7 */
+		  SUNXI_FUNCTION(0x3, "ts")),		/* D7 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 12),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* SCK */
+		  SUNXI_FUNCTION(0x3, "i2c2")),		/* SCK */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 13),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "csi"),		/* SDA */
+		  SUNXI_FUNCTION(0x3, "i2c2")),		/* SDA */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 14),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out")),
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(E, 15),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out")),
+	/* Hole */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(F, 0),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc0"),		/* D1 */
+		  SUNXI_FUNCTION(0x3, "jtag")),		/* MS */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(F, 1),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc0"),		/* D0 */
+		  SUNXI_FUNCTION(0x3, "jtag")),		/* DI */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(F, 2),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc0"),		/* CLK */
+		  SUNXI_FUNCTION(0x3, "uart0")),	/* TX */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(F, 3),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc0"),		/* CMD */
+		  SUNXI_FUNCTION(0x3, "jtag")),		/* DO */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(F, 4),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc0"),		/* D3 */
+		  SUNXI_FUNCTION(0x3, "uart0")),	/* RX */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(F, 5),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc0"),		/* D2 */
+		  SUNXI_FUNCTION(0x3, "jtag")),		/* CK */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(F, 6),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc0")),		/* DET */
+	/* Hole */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 0),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc1"),		/* CLK */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 0)),	/* PG_EINT0 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 1),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc1"),		/* CMD */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 1)),	/* PG_EINT1 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 2),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc1"),		/* D0 */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 2)),	/* PG_EINT2 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 3),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc1"),		/* D1 */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 3)),	/* PG_EINT3 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 4),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc1"),		/* D2 */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 4)),	/* PG_EINT4 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 5),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "mmc1"),		/* D3 */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 5)),	/* PG_EINT5 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 6),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "uart1"),		/* TX */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 6)),	/* PG_EINT6 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 7),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "uart1"),		/* RX */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 7)),	/* PG_EINT7 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 8),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "uart1"),		/* RTS */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 8)),	/* PG_EINT8 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 9),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "uart1"),		/* CTS */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 9)),	/* PG_EINT9 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 10),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "i2s1"),		/* SYNC */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 10)),	/* PG_EINT10 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 11),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "i2s1"),		/* CLK */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 11)),	/* PG_EINT11 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 12),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "i2s1"),		/* DOUT */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 12)),	/* PG_EINT12 */
+	SUNXI_PIN(SUNXI_PINCTRL_PIN(G, 13),
+		  SUNXI_FUNCTION(0x0, "gpio_in"),
+		  SUNXI_FUNCTION(0x1, "gpio_out"),
+		  SUNXI_FUNCTION(0x2, "i2s1"),		/* DIN */
+		  SUNXI_FUNCTION_IRQ_BANK(0x4, 1, 13)),	/* PG_EINT13 */
+};
+
+static const struct sunxi_pinctrl_desc sun8i_h3_pinctrl_data = {
+	.pins = sun8i_h3_pins,
+	.npins = ARRAY_SIZE(sun8i_h3_pins),
+	.irq_banks = 2,
+};
+
+static int sun8i_h3_pinctrl_probe(struct platform_device *pdev)
+{
+	return sunxi_pinctrl_init(pdev,
+				  &sun8i_h3_pinctrl_data);
+}
+
+static const struct of_device_id sun8i_h3_pinctrl_match[] = {
+	{ .compatible = "allwinner,sun8i-h3-pinctrl", },
+	{}
+};
+
+static struct platform_driver sun8i_h3_pinctrl_driver = {
+	.probe	= sun8i_h3_pinctrl_probe,
+	.driver	= {
+		.name		= "sun8i-h3-pinctrl",
+		.of_match_table	= sun8i_h3_pinctrl_match,
+	},
+};
+builtin_platform_driver(sun8i_h3_pinctrl_driver);
