/dts-v1/;

#include "rt3883.dtsi"

#include <dt-bindings/input/input.h>

/ {
	compatible = "TEW-691GR", "ralink,rt3883-soc";
	model = "TRENDnet TEW-691GR";

	nor-flash@1c000000 {
		compatible = "cfi-flash";
		reg = <0x1c000000 0x800000>;
		bank-width = <2>;
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			reg = <0x0 0x0030000>;
			label = "u-boot";
			read-only;
		};

		partition@30000 {
			reg = <0x00030000 0x00010000>;
			label = "u-boot-env";
			read-only;
		};

		factory: partition@40000 {
			reg = <0x00040000 0x00010000>;
			label = "factory";
			read-only;
		};

		partition@50000 {
			reg = <0x00050000 0x007b0000>;
			label = "firmware";
		};
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;

		reset {
			label = "reset";
			gpios = <&gpio0 10 1>;
			linux,code = <KEY_RESTART>;
		};

		wps {
			label = "wps";
			gpios = <&gpio1 2 1>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		rfkill {
			label = "rfkill";
			gpios = <&gpio0 0 1>;
			linux,code = <KEY_RFKILL>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		wps {
			label = "tew-691gr:green:wps";
			gpios = <&gpio0 9 1>;
		};
	};
};

&gpio1 {
	status = "okay";
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "spi", "i2c", "jtag", "uartf";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	mtd-mac-address = <&factory 0x4>;

	port@0 {
		phy-handle = <&phy0>;
		phy-mode = "rgmii";
	};

	mdio-bus {
		status = "okay";

		phy0: ethernet-phy@0 {
			reg = <0>;
			phy-mode = "rgmii";
		};
	};
};

&wmac {
	status = "okay";
	ralink,mtd-eeprom = <&factory 0x0>;
	ralink,5ghz = <0>;
	mtd-mac-address = <&factory 0x4>;
	mtd-mac-address-increment = <1>;
};
