From 2b436a351803f38d0c8ca9c26103472c8aaeb599 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?=C3=81lvaro=20Fern=C3=A1ndez=20Rojas?= <noltari@gmail.com>
Date: Thu, 19 May 2016 22:07:36 +0200
Subject: [PATCH] MIPS: ralink: add MT7628 EPHY LEDs pinmux support
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: Álvaro Fernández Rojas <noltari@gmail.com>
Cc: john@phrozen.org
Cc: linux-mips@linux-mips.org
Cc: linux-kernel@vger.kernel.org
Patchwork: https://patchwork.linux-mips.org/patch/13308/
Signed-off-by: Ralf Baechle <ralf@linux-mips.org>
---
 arch/mips/ralink/mt7620.c | 100 ++++++++++++++++++++++++++++++++++++++++++++++
 1 file changed, 100 insertions(+)

--- a/arch/mips/ralink/mt7620.c
+++ b/arch/mips/ralink/mt7620.c
@@ -188,6 +188,41 @@ static struct rt2880_pmx_func gpio_grp_m
 	FUNC("gpio", 0, 11, 1),
 };
 
+static struct rt2880_pmx_func p4led_kn_grp_mt7628[] = {
+	FUNC("jtag", 3, 30, 1),
+	FUNC("util", 2, 30, 1),
+	FUNC("gpio", 1, 30, 1),
+	FUNC("p4led_kn", 0, 30, 1),
+};
+
+static struct rt2880_pmx_func p3led_kn_grp_mt7628[] = {
+	FUNC("jtag", 3, 31, 1),
+	FUNC("util", 2, 31, 1),
+	FUNC("gpio", 1, 31, 1),
+	FUNC("p3led_kn", 0, 31, 1),
+};
+
+static struct rt2880_pmx_func p2led_kn_grp_mt7628[] = {
+	FUNC("jtag", 3, 32, 1),
+	FUNC("util", 2, 32, 1),
+	FUNC("gpio", 1, 32, 1),
+	FUNC("p2led_kn", 0, 32, 1),
+};
+
+static struct rt2880_pmx_func p1led_kn_grp_mt7628[] = {
+	FUNC("jtag", 3, 33, 1),
+	FUNC("util", 2, 33, 1),
+	FUNC("gpio", 1, 33, 1),
+	FUNC("p1led_kn", 0, 33, 1),
+};
+
+static struct rt2880_pmx_func p0led_kn_grp_mt7628[] = {
+	FUNC("jtag", 3, 34, 1),
+	FUNC("rsvd", 2, 34, 1),
+	FUNC("gpio", 1, 34, 1),
+	FUNC("p0led_kn", 0, 34, 1),
+};
+
 static struct rt2880_pmx_func wled_kn_grp_mt7628[] = {
 	FUNC("rsvd", 3, 35, 1),
 	FUNC("rsvd", 2, 35, 1),
@@ -195,6 +230,41 @@ static struct rt2880_pmx_func wled_kn_gr
 	FUNC("wled_kn", 0, 35, 1),
 };
 
+static struct rt2880_pmx_func p4led_an_grp_mt7628[] = {
+	FUNC("jtag", 3, 39, 1),
+	FUNC("util", 2, 39, 1),
+	FUNC("gpio", 1, 39, 1),
+	FUNC("p4led_an", 0, 39, 1),
+};
+
+static struct rt2880_pmx_func p3led_an_grp_mt7628[] = {
+	FUNC("jtag", 3, 40, 1),
+	FUNC("util", 2, 40, 1),
+	FUNC("gpio", 1, 40, 1),
+	FUNC("p3led_an", 0, 40, 1),
+};
+
+static struct rt2880_pmx_func p2led_an_grp_mt7628[] = {
+	FUNC("jtag", 3, 41, 1),
+	FUNC("util", 2, 41, 1),
+	FUNC("gpio", 1, 41, 1),
+	FUNC("p2led_an", 0, 41, 1),
+};
+
+static struct rt2880_pmx_func p1led_an_grp_mt7628[] = {
+	FUNC("jtag", 3, 42, 1),
+	FUNC("util", 2, 42, 1),
+	FUNC("gpio", 1, 42, 1),
+	FUNC("p1led_an", 0, 42, 1),
+};
+
+static struct rt2880_pmx_func p0led_an_grp_mt7628[] = {
+	FUNC("jtag", 3, 43, 1),
+	FUNC("rsvd", 2, 43, 1),
+	FUNC("gpio", 1, 43, 1),
+	FUNC("p0led_an", 0, 43, 1),
+};
+
 static struct rt2880_pmx_func wled_an_grp_mt7628[] = {
 	FUNC("rsvd", 3, 44, 1),
 	FUNC("rsvd", 2, 44, 1),
@@ -204,7 +274,17 @@ static struct rt2880_pmx_func wled_an_gr
 
 #define MT7628_GPIO_MODE_MASK		0x3
 
+#define MT7628_GPIO_MODE_P4LED_KN	58
+#define MT7628_GPIO_MODE_P3LED_KN	56
+#define MT7628_GPIO_MODE_P2LED_KN	54
+#define MT7628_GPIO_MODE_P1LED_KN	52
+#define MT7628_GPIO_MODE_P0LED_KN	50
 #define MT7628_GPIO_MODE_WLED_KN	48
+#define MT7628_GPIO_MODE_P4LED_AN	42
+#define MT7628_GPIO_MODE_P3LED_AN	40
+#define MT7628_GPIO_MODE_P2LED_AN	38
+#define MT7628_GPIO_MODE_P1LED_AN	36
+#define MT7628_GPIO_MODE_P0LED_AN	34
 #define MT7628_GPIO_MODE_WLED_AN	32
 #define MT7628_GPIO_MODE_PWM1		30
 #define MT7628_GPIO_MODE_PWM0		28
@@ -251,8 +331,28 @@ static struct rt2880_pmx_group mt7628an_
 				1, MT7628_GPIO_MODE_GPIO),
 	GRP_G("wled_an", wled_an_grp_mt7628, MT7628_GPIO_MODE_MASK,
 				1, MT7628_GPIO_MODE_WLED_AN),
+	GRP_G("p0led_an", p0led_an_grp_mt7628, MT7628_GPIO_MODE_MASK,
+				1, MT7628_GPIO_MODE_P0LED_AN),
+	GRP_G("p1led_an", p1led_an_grp_mt7628, MT7628_GPIO_MODE_MASK,
+				1, MT7628_GPIO_MODE_P1LED_AN),
+	GRP_G("p2led_an", p2led_an_grp_mt7628, MT7628_GPIO_MODE_MASK,
+				1, MT7628_GPIO_MODE_P2LED_AN),
+	GRP_G("p3led_an", p3led_an_grp_mt7628, MT7628_GPIO_MODE_MASK,
+				1, MT7628_GPIO_MODE_P3LED_AN),
+	GRP_G("p4led_an", p4led_an_grp_mt7628, MT7628_GPIO_MODE_MASK,
+				1, MT7628_GPIO_MODE_P4LED_AN),
 	GRP_G("wled_kn", wled_kn_grp_mt7628, MT7628_GPIO_MODE_MASK,
 				1, MT7628_GPIO_MODE_WLED_KN),
+	GRP_G("p0led_kn", p0led_kn_grp_mt7628, MT7628_GPIO_MODE_MASK,
+				1, MT7628_GPIO_MODE_P0LED_KN),
+	GRP_G("p1led_kn", p1led_kn_grp_mt7628, MT7628_GPIO_MODE_MASK,
+				1, MT7628_GPIO_MODE_P1LED_KN),
+	GRP_G("p2led_kn", p2led_kn_grp_mt7628, MT7628_GPIO_MODE_MASK,
+				1, MT7628_GPIO_MODE_P2LED_KN),
+	GRP_G("p3led_kn", p3led_kn_grp_mt7628, MT7628_GPIO_MODE_MASK,
+				1, MT7628_GPIO_MODE_P3LED_KN),
+	GRP_G("p4led_kn", p4led_kn_grp_mt7628, MT7628_GPIO_MODE_MASK,
+				1, MT7628_GPIO_MODE_P4LED_KN),
 	{ 0 }
 };
 
