From 80a97eae304631f57ff8560f87c0b18b95321443 Mon Sep 17 00:00:00 2001
From: Stanislaw Gruszka <sgruszka@redhat.com>
Date: Wed, 8 Feb 2017 13:51:29 +0100
Subject: [PATCH 04/19] rt61pci: use entry directly

Signed-off-by: Stanislaw Gruszka <sgruszka@redhat.com>
Signed-off-by: Kalle Valo <kvalo@codeaurora.org>
---
 drivers/net/wireless/ralink/rt2x00/rt61pci.c | 3 +--
 1 file changed, 1 insertion(+), 2 deletions(-)

diff --git a/drivers/net/wireless/ralink/rt2x00/rt61pci.c b/drivers/net/wireless/ralink/rt2x00/rt61pci.c
index 5306a3b2622d..8adb5f3abe15 100644
--- a/drivers/net/wireless/ralink/rt2x00/rt61pci.c
+++ b/drivers/net/wireless/ralink/rt2x00/rt61pci.c
@@ -1903,8 +1903,7 @@ static void rt61pci_write_tx_desc(struct queue_entry *entry,
 
 	rt2x00_desc_read(txd, 5, &word);
 	rt2x00_set_field32(&word, TXD_W5_PID_TYPE, entry->queue->qid);
-	rt2x00_set_field32(&word, TXD_W5_PID_SUBTYPE,
-			   skbdesc->entry->entry_idx);
+	rt2x00_set_field32(&word, TXD_W5_PID_SUBTYPE, entry->entry_idx);
 	rt2x00_set_field32(&word, TXD_W5_TX_POWER,
 			   TXPOWER_TO_DEV(entry->queue->rt2x00dev->tx_power));
 	rt2x00_set_field32(&word, TXD_W5_WAITING_DMA_DONE_INT, 1);
-- 
2.12.1

