<MSGENTRY>
<MSG>
<MSGMAIN>
<MSGTEXT>
<PARA>Auto removal: Token-ring lobe
</PARA>
</MSGTEXT>
</MSGMAIN>
<MSGSUB>
<TITLE>Failure
</TITLE>
<MSGTEXT>
<PARA>Local token-ring adapter
</PARA>
<PARA>Local access unit
</PARA>
<PARA>Local lobe cables
</PARA>
</MSGTEXT>
</MSGSUB>
<MSGREL>
<TITLE>NetWare message:
</TITLE>
<MSGTEXT>
<PARA>TOKEN-NW-237-Adapter <REPLACEABLE>number</REPLACEABLE&
gt; -board <REPLACEABLE>number</REPLACEABLE> : The adapter
is beaconing.
</PARA>
<PARA>Ring status = <REPLACEABLE>code</REPLACEABLE>
 .
</PARA>
</MSGTEXT>
</MSGREL>
     </MSG>
<MSGINFO>
<MSGORIG>NetView for NetWare
</MSGORIG>
<MSGLEVEL>Informative
</MSGLEVEL>
     </MSGINFO>
<MSGEXPLAN>
<TITLE>Explanation:
</TITLE>
<PARA>Adapter left the ring as part of the beacon automatic
recovery process.
</PARA>
</MSGEXPLAN>
<MSGEXPLAN>
<TITLE>Action:
</TITLE>
<PARA>Ask the LAN administrator to review the link data.
</PARA>
</MSGEXPLAN>
</MSGENTRY>
