/*
 * Copyright (c) 2020-2023, Arm Limited. All rights reserved.
 *
 * SPDX-License-Identifier: BSD-3-Clause
 */

#include <dt-bindings/interrupt-controller/arm-gic.h>

/ {
	compatible = "arm,morello";

	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	aliases {
		serial0 = &soc_uart0;
	};

	gic: interrupt-controller@2c010000 {
		compatible = "arm,gic-v3";
		#address-cells = <2>;
		#interrupt-cells = <3>;
		#size-cells = <2>;
		ranges;
		interrupt-controller;
	};

	pmu {
		compatible = "arm,armv8-pmuv3";
		interrupts = <GIC_PPI 7 IRQ_TYPE_LEVEL_HIGH>;
	};

	spe-pmu {
		compatible = "arm,statistical-profiling-extension-v1";
		interrupts = <GIC_PPI 5 IRQ_TYPE_LEVEL_HIGH>;
	};

	psci {
		compatible = "arm,psci-0.2";
		method = "smc";
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupts = <GIC_PPI 13 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_PPI 14 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_PPI 11 IRQ_TYPE_LEVEL_LOW>,
			     <GIC_PPI 10 IRQ_TYPE_LEVEL_LOW>;
	};

	mailbox: mhu@45000000 {
		compatible = "arm,mhu-doorbell", "arm,primecell";
		reg = <0x0 0x45000000 0x0 0x1000>;
		interrupts = <GIC_SPI 318 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 316 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "mhu_lpri_rx",
				  "mhu_hpri_rx";
		#mbox-cells = <2>;
		mbox-name = "ARM-MHU";
		clocks = <&soc_refclk50mhz>;
		clock-names = "apb_pclk";
	};

	sram: sram@45200000 {
		compatible = "mmio-sram";
		reg = <0x0 0x06000000 0x0 0x8000>;

		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0x0 0x06000000 0x8000>;

		cpu_scp_hpri0: scp-sram@0 {
			compatible = "arm,scmi-shmem";
			reg = <0x0 0x80>;
		};

		cpu_scp_hpri1: scp-sram@80 {
			compatible = "arm,scmi-shmem";
			reg = <0x80 0x80>;
		};
	};

	soc_refclk50mhz: refclk50mhz {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <50000000>;
		clock-output-names = "apb_pclk";
	};

	soc_refclk85mhz: refclk85mhz {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <85000000>;
		clock-output-names = "iofpga:aclk";
	};

	soc_uartclk:  uartclk {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <50000000>;
		clock-output-names = "uartclk";
	};

	soc_uart0: serial@2a400000 {
		compatible = "arm,pl011", "arm,primecell";
		reg = <0x0 0x2a400000 0x0 0x1000>;
		interrupts = <GIC_SPI 63 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&soc_uartclk>, <&soc_refclk50mhz>;
		clock-names = "uartclk", "apb_pclk";
		status = "okay";
	};
};
