// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/dts-v1/;

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

#include "ar7241.dtsi"

/ {
	compatible = "ubnt,unifi", "qca,ar7241";
	model = "Ubiquiti UniFi AP";

	aliases {
		led-boot = &dome_green;
		led-failsafe = &dome_green;
		led-running = &dome_green;
		led-upgrade = &dome_green;
	};

	extosc: ref {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <40000000>;
	};

	keys {
		compatible = "gpio-keys-polled";
		poll-interval = <20>;
		reset {
			linux,code = <KEY_RESTART>;
			gpios = <&gpio 12 GPIO_ACTIVE_LOW>;
			debounce-interval = <60>;
		};
	};

	leds {
		compatible = "gpio-leds";
		dome_green: dome-green {
			label = "ubnt:green:dome";
			gpios = <&gpio 0 GPIO_ACTIVE_HIGH>;
		};

		dome-orange {
			label = "ubnt:orange:dome";
			gpios = <&gpio 1 GPIO_ACTIVE_HIGH>;
		};
	};
};

&uart {
	status = "okay";
};

&pll {
	clocks = <&extosc>;
};

&spi {
	status = "okay";
	num-cs = <1>;

	flash@0 {
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <25000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@0 {
				label = "u-boot";
				reg = <0x000000 0x040000>;
				read-only;
			};

			partition@1 {
				label = "u-boot-env";
				reg = <0x040000 0x010000>;
			};

			partition@2 {
				compatible = "denx,uimage";
				label = "firmware";
				reg = <0x050000 0x750000>;
			};

			partition@3 {
				label = "board_config";
				reg = <0x7a0000 0x010000>;
				read-only;
			};

			partition@4 {
				label = "cfg";
				reg = <0x7b0000 0x040000>;
				read-only;
			};

			art: partition@5 {
				label = "art";
				reg = <0x7f0000 0x010000>;
				read-only;
			};
		};
	};
};

&pcie {
	status = "okay";

	wifi@0,0 {
		reg = <0x0000 0 0 0 0>;
		qca,no-eeprom;
	};
};

&eth0 {
	status = "okay";

	mtd-mac-address = <&art 0x0>;
};

&eth1 {
	status = "okay";

	compatible = "syscon", "simple-mfd";
};
