#!/bin/sh

ath10kcal_die() {
	echo "ath10cal: " "$*"
	exit 1
}

ath10kcal_from_file() {
	local source=$1
	local offset=$2
	local count=$3

	dd if=$source of=/lib/firmware/$FIRMWARE bs=1 skip=$offset count=$count 2>/dev/null || \
		ath10kcal_die "failed to extract calibration data from $source"
}

ath10kcal_extract() {
	local part=$1
	local offset=$2
	local count=$3
	local mtd cal_size

	mtd=$(find_mtd_chardev $part)
	[ -n "$mtd" ] || \
		ath10kcal_die "no mtd device found for partition $part"

	# Check that the calibration data size in header equals the desired size
	cal_size=$(dd if=$mtd bs=2 count=1 skip=$(( $offset / 2 )) conv=swab 2>/dev/null | hexdump -ve '1/2 "%d"')

	[ "$count" = "$cal_size" ] || \
		ath10kcal_die "no calibration data found in $part"

	dd if=$mtd of=/lib/firmware/$FIRMWARE bs=1 skip=$offset count=$count 2>/dev/null || \
		ath10kcal_die "failed to extract calibration data from $mtd"
}

ath10kcal_patch_mac() {
	local mac=$1

	[ -z "$mac" ] && return

	macaddr_2bin $mac | dd of=/lib/firmware/$FIRMWARE conv=notrunc bs=1 seek=6 count=6
}

[ -e /lib/firmware/$FIRMWARE ] && exit 0

. /lib/functions.sh
. /lib/functions/system.sh

board=$(board_name)

case "$FIRMWARE" in
"ath10k/cal-pci-0000:00:00.0.bin")
	case $board in
	a40|\
	a60|\
	mr1750|\
	mr1750v2|\
	om5p-acv2)
		ath10kcal_extract "ART" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(cat /sys/class/net/eth0/address) +16)
		;;
	archer-c25-v1|\
	tl-wdr6500-v2)
		ath10kcal_extract "art" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(cat /sys/class/net/eth1/address) -2)
		;;
	archer-c7-v4|\
	archer-c7-v5)
		ath10kcal_extract "art" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(cat /sys/class/net/eth0/address) -1)
		;;
	cf-e355ac-v1|\
	cf-e380ac-v1|\
	cf-e380ac-v2|\
	dlan-pro-1200-ac|\
	e1700ac-v2|\
	e600gac-v2|\
	minibox-v3.2|\
	oolite-v5.2|\
	oolite-v5.2-dev|\
	sr3200|\
	xd3200)
		ath10kcal_extract "art" 20480 2116
		;;
	dap-2695-a1)
		ath10kcal_extract "radiocfg" 20480 2116
		ath10kcal_patch_mac $(mtd_get_mac_ascii bdcfg wlanmac_a)
		;;
	dir-869-a1|\
	qihoo-c301)
		ath10kcal_extract "radiocfg" 20480 2116
		ath10kcal_patch_mac $(mtd_get_mac_ascii devdata wlan5mac)
		;;
	dw33d)
		ath10kcal_extract "art" 20480 2116
		ath10kcal_patch_mac $(mtd_get_mac_binary art 18)
		;;
	epg5000|\
	esr1750)
		ath10kcal_extract "caldata" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(cat /sys/class/net/eth0/address) +1)
		;;
	gl-ar750s|\
	gl-ar750|\
	tl-wpa8630)
		ath10kcal_extract "art" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(cat /sys/class/net/eth0/address) +1)
		;;
	koala)
		ath10kcal_extract "art" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(mtd_get_mac_binary art 12) +0)
		;;
	mc-mac1200r)
		ath10kcal_extract "art" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(cat /sys/class/net/eth1/address) -1)
		;;
	r6100)
		ath10kcal_extract "caldata" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(cat /sys/class/net/eth1/address) +2)
		;;
	rb-952ui-5ac2nd|\
	rb-wapg-5hact2hnd)
		ath10kcal_from_file "/sys/firmware/routerboot/ext_wlan_data" 20480 2116
		;;
	re355|\
	re450|\
	tl-wr902ac-v1)
		ath10kcal_extract "art" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(cat /sys/class/net/eth0/address) -2)
		;;
	unifiac-lite|\
	unifiac-pro)
		ath10kcal_extract "EEPROM" 20480 2116
		;;
	wi2a-ac200i)
		ath10kcal_extract "ART" 20480 2116
		;;
	esac
	;;
"ath10k/cal-pci-0000:01:00.0.bin")
	case $board in
	archer-c5|\
	archer-c7)
		ath10kcal_extract "art" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(cat /sys/class/net/eth1/address) -2)
		;;
	nbg6616|\
	nbg6716)
		ath10kcal_extract "RFdata" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(cat /sys/class/net/eth1/address) -2)
		;;
	om5p-ac)
		ath10kcal_extract "ART" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(cat /sys/class/net/eth0/address) +16)
		;;
	rb-911g-5hpacd|\
	rb-921gs-5hpacd-r2|\
	rb-962uigs-5hact2hnt)
		ath10kcal_from_file "/sys/firmware/routerboot/ext_wlan_data" 20480 2116
		;;
	wlr8100)
		ath10kcal_extract "art" 20480 2116
		ath10kcal_patch_mac $(macaddr_add $(mtd_get_mac_ascii u-boot-env ethaddr) +1)
		;;
	esac
	;;
"ath10k/pre-cal-pci-0000:00:00.0.bin")
	case $board in
	archer-c58-v1|\
	archer-c59-v1|\
	archer-c59-v2|\
	archer-c60-v1|\
	archer-c60-v2|\
	cf-e355ac-v2|\
	cf-e375ac)
		ath10kcal_extract "art" 20480 12064
		ln -sf /lib/firmware/ath10k/pre-cal-pci-0000\:00\:00.0.bin \
			/lib/firmware/ath10k/QCA9888/hw2.0/board.bin
		;;
	cf-e385ac)
		ath10kcal_extract "art" 20480 12064
		;;
	esac
	;;
*)
	exit 1
	;;
esac
