From: Felix Fietkau <nbd@nbd.name>
Subject: kernel: adjust mips highmem offset to avoid the need for -mlong-calls on systems with >256M RAM

Signed-off-by: Felix Fietkau <nbd@nbd.name>
---
 arch/mips/include/asm/mach-generic/spaces.h | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/mips/include/asm/mach-generic/spaces.h
+++ b/arch/mips/include/asm/mach-generic/spaces.h
@@ -50,7 +50,7 @@
  * Memory above this physical address will be considered highmem.
  */
 #ifndef HIGHMEM_START
-#define HIGHMEM_START		_AC(0x20000000, UL)
+#define HIGHMEM_START		_AC(0x10000000, UL)
 #endif
 
 #endif /* CONFIG_32BIT */
