From: Felix Fietkau <nbd@nbd.name>
Date: Sun, 15 May 2016 13:09:20 +0200
Subject: [PATCH] MIPS: ath79: fix regression in PCI window initialization

ath79_ddr_pci_win_base has the type void __iomem *, so register offsets
need to be a multiple of 4.

Cc: Alban Bedel <albeu@free.fr>
Fixes: 24b0e3e84fbf ("MIPS: ath79: Improve the DDR controller interface")
Signed-off-by: Felix Fietkau <nbd@nbd.name>
---

--- a/arch/mips/ath79/common.c
+++ b/arch/mips/ath79/common.c
@@ -76,14 +76,14 @@ void ath79_ddr_set_pci_windows(void)
 {
 	BUG_ON(!ath79_ddr_pci_win_base);
 
-	__raw_writel(AR71XX_PCI_WIN0_OFFS, ath79_ddr_pci_win_base + 0);
-	__raw_writel(AR71XX_PCI_WIN1_OFFS, ath79_ddr_pci_win_base + 1);
-	__raw_writel(AR71XX_PCI_WIN2_OFFS, ath79_ddr_pci_win_base + 2);
-	__raw_writel(AR71XX_PCI_WIN3_OFFS, ath79_ddr_pci_win_base + 3);
-	__raw_writel(AR71XX_PCI_WIN4_OFFS, ath79_ddr_pci_win_base + 4);
-	__raw_writel(AR71XX_PCI_WIN5_OFFS, ath79_ddr_pci_win_base + 5);
-	__raw_writel(AR71XX_PCI_WIN6_OFFS, ath79_ddr_pci_win_base + 6);
-	__raw_writel(AR71XX_PCI_WIN7_OFFS, ath79_ddr_pci_win_base + 7);
+	__raw_writel(AR71XX_PCI_WIN0_OFFS, ath79_ddr_pci_win_base + 0x0);
+	__raw_writel(AR71XX_PCI_WIN1_OFFS, ath79_ddr_pci_win_base + 0x4);
+	__raw_writel(AR71XX_PCI_WIN2_OFFS, ath79_ddr_pci_win_base + 0x8);
+	__raw_writel(AR71XX_PCI_WIN3_OFFS, ath79_ddr_pci_win_base + 0xc);
+	__raw_writel(AR71XX_PCI_WIN4_OFFS, ath79_ddr_pci_win_base + 0x10);
+	__raw_writel(AR71XX_PCI_WIN5_OFFS, ath79_ddr_pci_win_base + 0x14);
+	__raw_writel(AR71XX_PCI_WIN6_OFFS, ath79_ddr_pci_win_base + 0x18);
+	__raw_writel(AR71XX_PCI_WIN7_OFFS, ath79_ddr_pci_win_base + 0x1c);
 }
 EXPORT_SYMBOL_GPL(ath79_ddr_set_pci_windows);
 
