From b7c6d2675899cfff0180412c63fc9cbd5bacdb4d Mon Sep 17 00:00:00 2001
From: Eric Dumazet <edumazet@google.com>
Date: Wed, 19 Apr 2017 09:59:21 -0700
Subject: [PATCH] smsc75xx: use skb_cow_head() to deal with cloned skbs

We need to ensure there is enough headroom to push extra header,
but we also need to check if we are allowed to change headers.

skb_cow_head() is the proper helper to deal with this.

Fixes: d0cad871703b ("smsc75xx: SMSC LAN75xx USB gigabit ethernet adapter driver")
Signed-off-by: Eric Dumazet <edumazet@google.com>
Cc: James Hughes <james.hughes@raspberrypi.org>
Signed-off-by: David S. Miller <davem@davemloft.net>
---
 drivers/net/usb/smsc75xx.c | 8 ++------
 1 file changed, 2 insertions(+), 6 deletions(-)

--- a/drivers/net/usb/smsc75xx.c
+++ b/drivers/net/usb/smsc75xx.c
@@ -2193,13 +2193,9 @@ static struct sk_buff *smsc75xx_tx_fixup
 {
 	u32 tx_cmd_a, tx_cmd_b;
 
-	if (skb_headroom(skb) < SMSC75XX_TX_OVERHEAD) {
-		struct sk_buff *skb2 =
-			skb_copy_expand(skb, SMSC75XX_TX_OVERHEAD, 0, flags);
+	if (skb_cow_head(skb, SMSC75XX_TX_OVERHEAD)) {
 		dev_kfree_skb_any(skb);
-		skb = skb2;
-		if (!skb)
-			return NULL;
+		return NULL;
 	}
 
 	tx_cmd_a = (u32)(skb->len & TX_CMD_A_LEN) | TX_CMD_A_FCS;
