/dts-v1/;

#include "rt2880.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>

/ {
	#address-cells = <1>;
	#size-cells = <1>;
	compatible = "F5D8235_V1", "ralink,rt2880-soc";
	model = "Belkin F5D8235 v1";

	pci@440000 {
		status = "ok";
	};

	cfi@1f000000 {
		compatible = "cfi-flash";
		reg = <0xbc400000 0x800000>;
		bank-width = <2>;
		device-width = <2>;
		#address-cells = <1>;
		#size-cells = <1>;

		partition@0 {
			label = "uboot";
			reg = <0x0 0x30000>;
			read-only;
		};

		partition@30000 {
			label = "uboot-env";
			reg = <0x30000 0x10000>;
			read-only;
		};

		factory: partition@40000 {
			label = "factory";
			reg = <0x40000 0x10000>;
			read-only;
		};

		partition@50000 {
			label = "firmware";
			reg = <0x50000 0x7b0000>;
		};
	};

	rtl8366s {
		compatible = "realtek,rtl8366s";
		gpio-sda = <&gpio0 1 GPIO_ACTIVE_HIGH>;
		gpio-sck = <&gpio0 2 GPIO_ACTIVE_HIGH>;
	};

	gpio-keys-polled {
		compatible = "gpio-keys-polled";
		#address-cells = <1>;
		#size-cells = <0>;
		poll-interval = <100>;

		wps {
			label = "wps";
			gpios = <&gpio0 0 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_WPS_BUTTON>;
		};

		reset {
			label = "reset";
			gpios = <&gpio0 9 GPIO_ACTIVE_LOW>;
			linux,code = <KEY_RESTART>;
		};
	};

	gpio-leds {
		compatible = "gpio-leds";

		internet {
			label = "f5d8235-v1:blue:internet";
			gpios = <&gpio0 17 GPIO_ACTIVE_LOW>;
		};

		internet2 {
			label = "f5d8235-v1:amber:internet";
			gpios = <&gpio0 18 GPIO_ACTIVE_LOW>;
		};

		modem {
			label = "f5d8235-v1:blue:modem";
			gpios = <&gpio0 13 GPIO_ACTIVE_LOW>;
		};

		modem2 {
			label = "f5d8235-v1:amber:modem";
			gpios = <&gpio0 21 GPIO_ACTIVE_LOW>;
		};

		router {
			label = "f5d8235-v1:blue:router";
			gpios = <&gpio0 14 GPIO_ACTIVE_HIGH>;
		};

		storage {
			label = "f5d8235-v1:blue:storage";
			gpios = <&gpio0 7 GPIO_ACTIVE_LOW>;
		};

		storage2 {
			label = "f5d8235-v1:amber:storage";
			gpios = <&gpio0 8 GPIO_ACTIVE_LOW>;
		};

		security {
			label = "f5d8235-v1:blue:security";
			gpios = <&gpio0 10 GPIO_ACTIVE_LOW>;
		};

		security2 {
			label = "f5d8235-v1:amber:security";
			gpios = <&gpio0 12 GPIO_ACTIVE_LOW>;
		};

		wired {
			label = "f5d8235-v1:blue:wired";
			gpios = <&gpio0 5 GPIO_ACTIVE_LOW>;
		};

		wired2 {
			label = "f5d8235-v1:amber:wired";
			gpios = <&gpio0 20 GPIO_ACTIVE_LOW>;
		};

		wireless {
			label = "f5d8235-v1:blue:wireless";
			gpios = <&gpio0 6 GPIO_ACTIVE_LOW>;
		};

		wireless2 {
			label = "f5d8235-v1:amber:wireless";
			gpios = <&gpio0 19 GPIO_ACTIVE_LOW>;
		};
	};
};

&gpio0 {
	status = "okay";
};

&pinctrl {
	state_default: pinctrl0 {
		gpio {
			ralink,group = "spi", "i2c", "jtag", "mdio", "uartlite";
			ralink,function = "gpio";
		};
	};
};

&ethernet {
	status = "okay";
	mtd-mac-address = <&factory 0x4>;

	port@0 {
		mediatek,fixed-link = <1000 1 1 1>;
	};
};

&wmac {
	status = "okay";
	ralink,mtd-eeprom = <&factory 0x0>;
};
