From a3bddfdd19c49f0bde7aa2ff496773c575763d07 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?David=20Lanzend=C3=B6rfer?= <david.lanzendoerfer@o2s.ch>
Date: Sat, 15 Feb 2014 14:02:01 +0100
Subject: [PATCH] ARM: dts: sun7i: Add support for mmc
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: David Lanzendörfer <david.lanzendoerfer@o2s.ch>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun7i-a20-cubieboard2.dts     |  8 ++++
 arch/arm/boot/dts/sun7i-a20-cubietruck.dts      |  8 ++++
 arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts | 23 ++++++++++
 arch/arm/boot/dts/sun7i-a20.dtsi                | 61 +++++++++++++++++++++++++
 4 files changed, 100 insertions(+)

diff --git a/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts b/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
index 07823c2..a8186f5 100644
--- a/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
@@ -20,6 +20,14 @@
 	compatible = "cubietech,cubieboard2", "allwinner,sun7i-a20";
 
 	soc@01c00000 {
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_reference_design>;
+			cd-gpios = <&pio 7 1 0>; /* PH1 */
+			status = "okay";
+		};
+
 		ahci: sata@01c18000 {
 			target-supply = <&reg_ahci_5v>;
 			status = "okay";
diff --git a/arch/arm/boot/dts/sun7i-a20-cubietruck.dts b/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
index 403bd2e..6cd7cca 100644
diff --git a/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts b/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts
index d5c6799..d4e2355 100644
--- a/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts
+++ b/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts
@@ -20,12 +20,35 @@
 	compatible = "olimex,a20-olinuxino-micro", "allwinner,sun7i-a20";
 
 	soc@01c00000 {
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_reference_design>;
+			cd-gpios = <&pio 7 1 0>; /* PH1 */
+			status = "okay";
+		};
+
+		mmc3: mmc@01c12000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc3_pins_a>;
+			pinctrl-1 = <&mmc3_cd_pin_olinuxinom>;
+			cd-gpios = <&pio 7 11 0>; /* PH11 */
+			status = "okay";
+		};
+
 		ahci: sata@01c18000 {
 			target-supply = <&reg_ahci_5v>;
 			status = "okay";
 		};
 
 		pinctrl@01c20800 {
+			mmc3_cd_pin_olinuxinom: mmc3_cd_pin@0 {
+				allwinner,pins = "PH11";
+				allwinner,function = "gpio_in";
+				allwinner,drive = <0>;
+				allwinner,pull = <1>;
+			};
+
 			led_pins_olinuxino: led_pins@0 {
 				allwinner,pins = "PH2";
 				allwinner,function = "gpio_out";
diff --git a/arch/arm/boot/dts/sun7i-a20.dtsi b/arch/arm/boot/dts/sun7i-a20.dtsi
index 3385994..3bc6ac5 100644
--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -392,6 +392,46 @@
 			#size-cells = <0>;
 		};
 
+		mmc0: mmc@01c0f000 {
+			compatible = "allwinner,sun5i-a13-mmc";
+			reg = <0x01c0f000 0x1000>;
+			clocks = <&ahb_gates 8>, <&mmc0_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <0 32 4>;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
+		mmc1: mmc@01c10000 {
+			compatible = "allwinner,sun5i-a13-mmc";
+			reg = <0x01c10000 0x1000>;
+			clocks = <&ahb_gates 9>, <&mmc1_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <0 33 4>;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
+		mmc2: mmc@01c11000 {
+			compatible = "allwinner,sun5i-a13-mmc";
+			reg = <0x01c11000 0x1000>;
+			clocks = <&ahb_gates 10>, <&mmc2_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <0 34 4>;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
+		mmc3: mmc@01c12000 {
+			compatible = "allwinner,sun5i-a13-mmc";
+			reg = <0x01c12000 0x1000>;
+			clocks = <&ahb_gates 11>, <&mmc3_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <0 35 4>;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
 		ahci: sata@01c18000 {
 			compatible = "allwinner,sun4i-a10-ahci";
 			reg = <0x01c18000 0x1000>;
@@ -510,6 +550,27 @@
 				allwinner,drive = <3>;
 				allwinner,pull = <0>;
 			};
+
+			mmc0_pins_a: mmc0@0 {
+				allwinner,pins = "PF0","PF1","PF2","PF3","PF4","PF5";
+				allwinner,function = "mmc0";
+				allwinner,drive = <3>;
+				allwinner,pull = <0>;
+			};
+
+			mmc0_cd_pin_reference_design: mmc0_cd_pin@0 {
+				allwinner,pins = "PH1";
+				allwinner,function = "gpio_in";
+				allwinner,drive = <0>;
+				allwinner,pull = <1>;
+			};
+
+			mmc3_pins_a: mmc3@0 {
+				allwinner,pins = "PI4","PI5","PI6","PI7","PI8","PI9";
+				allwinner,function = "mmc3";
+				allwinner,drive = <3>;
+				allwinner,pull = <0>;
+			};
 		};
 
 		timer@01c20c00 {
-- 
1.8.5.5

