From abc12cd5c39556824cc9022db6eddc64e8e8dbe9 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Wed, 23 Oct 2013 17:54:39 +0100
Subject: [PATCH] clockevent: sun4i: Fill the irq field in the clockevent
 structure

The clock event structure irq field was not filled previously to the
interrupt we're using.

This was resulting in the timer not being used at all when using a
configuration with SMP enabled on a system with several CPUs, and with
the cpumask set to the cpu_possible_mask.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 drivers/clocksource/sun4i_timer.c | 1 +
 1 file changed, 1 insertion(+)

--- a/drivers/clocksource/sun4i_timer.c
+++ b/drivers/clocksource/sun4i_timer.c
@@ -191,6 +191,7 @@ static void __init sun4i_timer_init(stru
 	writel(val | TIMER_IRQ_EN(0), timer_base + TIMER_IRQ_EN_REG);
 
 	sun4i_clockevent.cpumask = cpumask_of(0);
+	sun4i_clockevent.irq = irq;
 
 	clockevents_config_and_register(&sun4i_clockevent, rate,
 					TIMER_SYNC_TICKS, 0xffffffff);
