From d3861805e84e1b54073e20dc499b9380b38bb7ab Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Sun, 3 Nov 2013 10:30:12 +0100
Subject: [PATCH] ARM: sun6i: dt: Add IP needed to bring up the additional
 cores

Add the PRCM and CPU configuration units needed for SMP in the A31 DTSI.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun6i-a31.dtsi | 10 ++++++++++
 1 file changed, 10 insertions(+)

--- a/arch/arm/boot/dts/sun6i-a31.dtsi
+++ b/arch/arm/boot/dts/sun6i-a31.dtsi
@@ -322,5 +322,15 @@
 			#interrupt-cells = <3>;
 			interrupts = <1 9 0xf04>;
 		};
+
+		cpucfg@01f01c00 {
+			compatible = "allwinner,sun6i-a31-cpuconfig";
+			reg = <0x01f01c00 0x300>;
+		};
+
+		prcm@01f01c00 {
+			compatible = "allwinner,sun6i-a31-prcm";
+			reg = <0x01f01400 0x200>;
+		};
 	};
 };
