From 5bfbb46a8685de4c67f084aea983fc9a50c882ad Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?David=20Lanzend=C3=B6rfer?= <david.lanzendoerfer@o2s.ch>
Date: Sat, 15 Feb 2014 14:02:29 +0100
Subject: [PATCH] ARM: dts: sun5i: Add support for mmc
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: David Lanzendörfer <david.lanzendoerfer@o2s.ch>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun5i-a10s-olinuxino-micro.dts | 30 ++++++++++++++++
 arch/arm/boot/dts/sun5i-a10s.dtsi                | 44 ++++++++++++++++++++++++
 arch/arm/boot/dts/sun5i-a13-olinuxino-micro.dts  | 15 ++++++++
 arch/arm/boot/dts/sun5i-a13-olinuxino.dts        | 15 ++++++++
 arch/arm/boot/dts/sun5i-a13.dtsi                 | 37 ++++++++++++++++++++
 5 files changed, 141 insertions(+)

diff --git a/arch/arm/boot/dts/sun5i-a10s-olinuxino-micro.dts b/arch/arm/boot/dts/sun5i-a10s-olinuxino-micro.dts
index 3c9f8b3..5c7b454 100644
--- a/arch/arm/boot/dts/sun5i-a10s-olinuxino-micro.dts
+++ b/arch/arm/boot/dts/sun5i-a10s-olinuxino-micro.dts
@@ -34,7 +34,37 @@
 			};
 		};
 
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_olinuxino_micro>;
+			cd-gpios = <&pio 6 1 0>; /* PG1 */
+			status = "okay";
+		};
+
+		mmc1: mmc@01c10000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc1_pins_a>;
+			pinctrl-1 = <&mmc1_cd_pin_olinuxino_micro>;
+			cd-gpios = <&pio 6 13 0>; /* PG13 */
+			status = "okay";
+		};
+
 		pinctrl@01c20800 {
+			mmc0_cd_pin_olinuxino_micro: mmc0_cd_pin@0 {
+				allwinner,pins = "PG1";
+				allwinner,function = "gpio_in";
+				allwinner,drive = <0>;
+				allwinner,pull = <1>;
+			};
+
+			mmc1_cd_pin_olinuxino_micro: mmc1_cd_pin@0 {
+				allwinner,pins = "PG13";
+				allwinner,function = "gpio_in";
+				allwinner,drive = <0>;
+				allwinner,pull = <1>;
+			};
+
 			led_pins_olinuxino: led_pins@0 {
 				allwinner,pins = "PE3";
 				allwinner,function = "gpio_out";
diff --git a/arch/arm/boot/dts/sun5i-a10s.dtsi b/arch/arm/boot/dts/sun5i-a10s.dtsi
index 3a9b33d..3a7039e 100644
--- a/arch/arm/boot/dts/sun5i-a10s.dtsi
+++ b/arch/arm/boot/dts/sun5i-a10s.dtsi
@@ -299,6 +299,36 @@
 			#size-cells = <0>;
 		};
 
+		mmc0: mmc@01c0f000 {
+			compatible = "allwinner,sun5i-a13-mmc";
+			reg = <0x01c0f000 0x1000>;
+			clocks = <&ahb_gates 8>, <&mmc0_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <32>;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
+		mmc1: mmc@01c10000 {
+			compatible = "allwinner,sun5i-a13-mmc";
+			reg = <0x01c10000 0x1000>;
+			clocks = <&ahb_gates 9>, <&mmc1_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <33>;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
+		mmc2: mmc@01c11000 {
+			compatible = "allwinner,sun5i-a13-mmc";
+			reg = <0x01c11000 0x1000>;
+			clocks = <&ahb_gates 10>, <&mmc2_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <34>;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
 		intc: interrupt-controller@01c20400 {
 			compatible = "allwinner,sun4i-ic";
 			reg = <0x01c20400 0x400>;
@@ -369,6 +399,20 @@
 				allwinner,drive = <0>;
 				allwinner,pull = <0>;
 			};
+
+			mmc0_pins_a: mmc0@0 {
+				allwinner,pins = "PF0","PF1","PF2","PF3","PF4","PF5";
+				allwinner,function = "mmc0";
+				allwinner,drive = <3>;
+				allwinner,pull = <0>;
+			};
+
+			mmc1_pins_a: mmc1@0 {
+				allwinner,pins = "PG3","PG4","PG5","PG6","PG7","PG8";
+				allwinner,function = "mmc1";
+				allwinner,drive = <3>;
+				allwinner,pull = <0>;
+			};
 		};
 
 		timer@01c20c00 {
diff --git a/arch/arm/boot/dts/sun5i-a13-olinuxino-micro.dts b/arch/arm/boot/dts/sun5i-a13-olinuxino-micro.dts
index fe2ce0a..2f08bb2 100644
--- a/arch/arm/boot/dts/sun5i-a13-olinuxino-micro.dts
+++ b/arch/arm/boot/dts/sun5i-a13-olinuxino-micro.dts
@@ -20,7 +20,22 @@
 	compatible = "olimex,a13-olinuxino-micro", "allwinner,sun5i-a13";
 
 	soc@01c00000 {
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_olinuxinom>;
+			cd-gpios = <&pio 6 0 0>; /* PG0 */
+			status = "okay";
+		};
+
 		pinctrl@01c20800 {
+			mmc0_cd_pin_olinuxinom: mmc0_cd_pin@0 {
+				allwinner,pins = "PG0";
+				allwinner,function = "gpio_in";
+				allwinner,drive = <0>;
+				allwinner,pull = <1>;
+			};
+
 			led_pins_olinuxinom: led_pins@0 {
 				allwinner,pins = "PG9";
 				allwinner,function = "gpio_out";
diff --git a/arch/arm/boot/dts/sun5i-a13-olinuxino.dts b/arch/arm/boot/dts/sun5i-a13-olinuxino.dts
index a4ba5ff..a7280f5 100644
--- a/arch/arm/boot/dts/sun5i-a13-olinuxino.dts
+++ b/arch/arm/boot/dts/sun5i-a13-olinuxino.dts
@@ -19,7 +19,22 @@
 	compatible = "olimex,a13-olinuxino", "allwinner,sun5i-a13";
 
 	soc@01c00000 {
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_olinuxino>;
+			cd-gpios = <&pio 6 0 0>; /* PG0 */
+			status = "okay";
+		};
+
 		pinctrl@01c20800 {
+			mmc0_cd_pin_olinuxino: mmc0_cd_pin@0 {
+				allwinner,pins = "PG0";
+				allwinner,function = "gpio_in";
+				allwinner,drive = <0>;
+				allwinner,pull = <1>;
+			};
+
 			led_pins_olinuxino: led_pins@0 {
 				allwinner,pins = "PG9";
 				allwinner,function = "gpio_out";
diff --git a/arch/arm/boot/dts/sun5i-a13.dtsi b/arch/arm/boot/dts/sun5i-a13.dtsi
index 9612c52..63a35b8 100644
--- a/arch/arm/boot/dts/sun5i-a13.dtsi
+++ b/arch/arm/boot/dts/sun5i-a13.dtsi
@@ -281,6 +281,36 @@
 		#size-cells = <1>;
 		ranges;
 
+		mmc0: mmc@01c0f000 {
+			compatible = "allwinner,sun5i-a13-mmc";
+			reg = <0x01c0f000 0x1000>;
+			clocks = <&ahb_gates 8>, <&mmc0_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <32>;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
+		mmc1: mmc@01c10000 {
+			compatible = "allwinner,sun5i-a13-mmc";
+			reg = <0x01c10000 0x1000>;
+			clocks = <&ahb_gates 9>, <&mmc1_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <33>;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
+		mmc2: mmc@01c11000 {
+			compatible = "allwinner,sun5i-a13-mmc";
+			reg = <0x01c11000 0x1000>;
+			clocks = <&ahb_gates 10>, <&mmc2_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <34>;
+			bus-width = <4>;
+			status = "disabled";
+		};
+
 		intc: interrupt-controller@01c20400 {
 			compatible = "allwinner,sun4i-ic";
 			reg = <0x01c20400 0x400>;
@@ -333,6 +363,13 @@
 				allwinner,drive = <0>;
 				allwinner,pull = <0>;
 			};
+
+			mmc0_pins_a: mmc0@0 {
+				allwinner,pins = "PF0","PF1","PF2","PF3","PF4","PF5";
+				allwinner,function = "mmc0";
+				allwinner,drive = <3>;
+				allwinner,pull = <0>;
+			};
 		};
 
 		timer@01c20c00 {
-- 
1.8.5.5

