From a4eb936767bd6a63d54734b9ce48932609ce58eb Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Thu, 7 Nov 2013 12:01:48 +0100
Subject: [PATCH] clocksource: sun4i: Increase a bit the clock event and
 sources rating
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

We want to keep this driver as the default provider of the clock events
and source, yet some other driver might fit in the "desired" category of
ratings. Hence, we need to increase a bit the rating so that we can have
more flexibility in the ratings we choose.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
Tested-by: Emilio López <emilio@elopez.com.ar>
Signed-off-by: Daniel Lezcano <daniel.lezcano@linaro.org>
---
 drivers/clocksource/sun4i_timer.c | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/clocksource/sun4i_timer.c
+++ b/drivers/clocksource/sun4i_timer.c
@@ -114,7 +114,7 @@ static int sun4i_clkevt_next_event(unsig
 
 static struct clock_event_device sun4i_clockevent = {
 	.name = "sun4i_tick",
-	.rating = 300,
+	.rating = 350,
 	.features = CLOCK_EVT_FEAT_PERIODIC | CLOCK_EVT_FEAT_ONESHOT,
 	.set_mode = sun4i_clkevt_mode,
 	.set_next_event = sun4i_clkevt_next_event,
@@ -172,7 +172,7 @@ static void __init sun4i_timer_init(stru
 
 	setup_sched_clock(sun4i_timer_sched_read, 32, rate);
 	clocksource_mmio_init(timer_base + TIMER_CNTVAL_REG(1), node->name,
-			      rate, 300, 32, clocksource_mmio_readl_down);
+			      rate, 350, 32, clocksource_mmio_readl_down);
 
 	ticks_per_jiffy = DIV_ROUND_UP(rate, HZ);
 
