From 54b9b9ab635ed8e643784402096524768f490f5d Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Sat, 11 Jan 2014 04:33:23 +0100
Subject: [PATCH] ARM: sun4i: dt: Add mmc node to a few more boards

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun4i-a10-hackberry.dts  | 9 +++++++++
 arch/arm/boot/dts/sun4i-a10-mini-xplus.dts | 8 ++++++++
 arch/arm/boot/dts/sun4i-a10-pcduino.dts    | 8 ++++++++
 3 files changed, 25 insertions(+)

diff --git a/arch/arm/boot/dts/sun4i-a10-hackberry.dts b/arch/arm/boot/dts/sun4i-a10-hackberry.dts
index 6692d336..2eb30d0 100644
--- a/arch/arm/boot/dts/sun4i-a10-hackberry.dts
+++ b/arch/arm/boot/dts/sun4i-a10-hackberry.dts
@@ -35,6 +35,15 @@
 			};
 		};
 
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_reference_design>;
+			cd-gpios = <&pio 7 1 0>; /* PH1 */
+			cd-mode = <1>;
+			status = "okay";
+		};
+
 		pio: pinctrl@01c20800 {
 			pinctrl-names = "default";
 			pinctrl-0 = <&hackberry_hogs>;
diff --git a/arch/arm/boot/dts/sun4i-a10-mini-xplus.dts b/arch/arm/boot/dts/sun4i-a10-mini-xplus.dts
index 70b3323..6dbe53c 100644
--- a/arch/arm/boot/dts/sun4i-a10-mini-xplus.dts
+++ b/arch/arm/boot/dts/sun4i-a10-mini-xplus.dts
@@ -19,6 +19,14 @@
 	compatible = "pineriver,mini-xplus", "allwinner,sun4i-a10";
 
 	soc@01c00000 {
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_reference_design>;
+			cd-gpios = <&pio 7 1 0>; /* PH1 */
+			status = "okay";
+		};
+
 		uart0: serial@01c28000 {
 			pinctrl-names = "default";
 			pinctrl-0 = <&uart0_pins_a>;
diff --git a/arch/arm/boot/dts/sun4i-a10-pcduino.dts b/arch/arm/boot/dts/sun4i-a10-pcduino.dts
index f5692a3..87f7742 100644
--- a/arch/arm/boot/dts/sun4i-a10-pcduino.dts
+++ b/arch/arm/boot/dts/sun4i-a10-pcduino.dts
@@ -33,6 +33,14 @@
 			};
 		};
 
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_reference_design>;
+			cd-gpios = <&pio 7 1 0>; /* PH1 */
+			status = "okay";
+		};
+
 		uart0: serial@01c28000 {
 			pinctrl-names = "default";
 			pinctrl-0 = <&uart0_pins_a>;
-- 
1.8.5.5

