From 2f2ffd5ea0174434c8214722127e5e977dcecf32 Mon Sep 17 00:00:00 2001
From: Zalan Blenessy <zalan.blenessy@gmail.com>
Date: Sun, 22 Dec 2013 17:08:10 +0100
Subject: [PATCH] ARM: sun7i: dt: Add USB host nodes to a20-olinuxino-micro dts

Add nodes for the usb-phy and ehci- and ohci-usb-host controllers.

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts | 23 +++++++++++++++++++++++
 1 file changed, 23 insertions(+)

diff --git a/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts b/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts
index aef289f..824ce0a 100644
--- a/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts
+++ b/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts
@@ -14,6 +14,7 @@
 /dts-v1/;
 /include/ "sun7i-a20.dtsi"
 /include/ "sunxi-ahci-reg.dtsi"
+/include/ "sun4i-a10-usb-vbus-reg.dtsi"
 #include <dt-bindings/input/input.h>
 
 / {
@@ -37,11 +38,33 @@
 			status = "okay";
 		};
 
+		usbphy: phy@01c13400 {
+			usb1_vbus-supply = <&reg_usb1_vbus>;
+			usb2_vbus-supply = <&reg_usb2_vbus>;
+			status = "okay";
+		};
+
+		ehci0: usb@01c14000 {
+			status = "okay";
+		};
+
+		ohci0: usb@01c14400 {
+			status = "okay";
+		};
+
 		ahci: sata@01c18000 {
 			target-supply = <&reg_ahci_5v>;
 			status = "okay";
 		};
 
+		ehci1: usb@01c1c000 {
+			status = "okay";
+		};
+
+		ohci1: usb@01c1c400 {
+			status = "okay";
+		};
+
 		pinctrl@01c20800 {
 			mmc3_cd_pin_olinuxinom: mmc3_cd_pin@0 {
 				allwinner,pins = "PH11";
-- 
1.8.5.5

