From 5b820d3062a436cf36ddf2fecc88524b9adf7b6e Mon Sep 17 00:00:00 2001
From: Roman Byshko <rbyshko@gmail.com>
Date: Thu, 19 Sep 2013 21:29:45 +0200
Subject: [PATCH] ARM: sun7i: dt: Add USB host nodes to cubieboard2 dts

Add nodes for the usb-phy and ehci- and ohci-usb-host controllers.

Signed-off-by: Roman Byshko <rbyshko@gmail.com>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun7i-a20-cubieboard2.dts | 23 +++++++++++++++++++++++
 1 file changed, 23 insertions(+)

diff --git a/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts b/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
index a8186f5..9fa1d85 100644
--- a/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
@@ -14,6 +14,7 @@
 /dts-v1/;
 /include/ "sun7i-a20.dtsi"
 /include/ "sunxi-ahci-reg.dtsi"
+/include/ "sun4i-a10-usb-vbus-reg.dtsi"
 
 / {
 	model = "Cubietech Cubieboard2";
@@ -28,11 +29,33 @@
 			status = "okay";
 		};
 
+		usbphy: phy@01c13400 {
+			usb1_vbus-supply = <&reg_usb1_vbus>;
+			usb2_vbus-supply = <&reg_usb2_vbus>;
+			status = "okay";
+		};
+
+		ehci0: usb@01c14000 {
+			status = "okay";
+		};
+
+		ohci0: usb@01c14400 {
+			status = "okay";
+		};
+
 		ahci: sata@01c18000 {
 			target-supply = <&reg_ahci_5v>;
 			status = "okay";
 		};
 
+		ehci1: usb@01c1c000 {
+			status = "okay";
+		};
+
+		ohci1: usb@01c1c400 {
+			status = "okay";
+		};
+
 		pinctrl@01c20800 {
 			led_pins_cubieboard2: led_pins@0 {
 				allwinner,pins = "PH20", "PH21";
-- 
1.8.5.5

