From b15b9f68606134222f7aff5120c8ef70ffab92b8 Mon Sep 17 00:00:00 2001
From: Carlo Caione <carlo.caione@gmail.com>
Date: Wed, 16 Oct 2013 20:30:26 +0200
Subject: [PATCH] ARM: dts: sun4i/sun7i: add RTC node

Add the RTC node to DTS for Allwinner A10 and Allwinner A20.

Signed-off-by: Carlo Caione <carlo.caione@gmail.com>
Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun4i-a10.dtsi | 6 ++++++
 arch/arm/boot/dts/sun7i-a20.dtsi | 6 ++++++
 2 files changed, 12 insertions(+)

--- a/arch/arm/boot/dts/sun4i-a10.dtsi
+++ b/arch/arm/boot/dts/sun4i-a10.dtsi
@@ -412,6 +412,12 @@
 			reg = <0x01c20c90 0x10>;
 		};
 
+		rtc: rtc@01c20d00 {
+			compatible = "allwinner,sun4i-rtc";
+			reg = <0x01c20d00 0x20>;
+			interrupts = <24>;
+		};
+
 		sid: eeprom@01c23800 {
 			compatible = "allwinner,sun4i-sid";
 			reg = <0x01c23800 0x10>;
--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -416,6 +416,12 @@
 			reg = <0x01c20c90 0x10>;
 		};
 
+		rtc: rtc@01c20d00 {
+			compatible = "allwinner,sun7i-a20-rtc";
+			reg = <0x01c20d00 0x20>;
+			interrupts = <0 24 1>;
+		};
+
 		sid: eeprom@01c23800 {
 			compatible = "allwinner,sun7i-a20-sid";
 			reg = <0x01c23800 0x200>;
