From c997a1da25fe7c717ed099888b8eb35d4e139e70 Mon Sep 17 00:00:00 2001
From: Felix Fietkau <nbd@openwrt.org>
Date: Sun, 8 Dec 2013 08:52:52 +0100
Subject: [PATCH] ath9k: support only one P2P interface

Preparation for adding P2P powersave and multi-channel support.

Signed-off-by: Felix Fietkau <nbd@openwrt.org>
---
 drivers/net/wireless/ath/ath9k/init.c | 4 ++--
  1 file changed, 2 insertions(+), 2 deletions(-)

--- a/drivers/net/wireless/ath/ath9k/init.c
+++ b/drivers/net/wireless/ath/ath9k/init.c
@@ -863,15 +863,15 @@ void ath9k_reload_chainmask_settings(str
 
 static const struct ieee80211_iface_limit if_limits[] = {
 	{ .max = 2048,	.types = BIT(NL80211_IFTYPE_STATION) |
-				 BIT(NL80211_IFTYPE_P2P_CLIENT) |
 				 BIT(NL80211_IFTYPE_WDS) },
 	{ .max = 8,	.types =
 #ifdef CPTCFG_MAC80211_MESH
 				 BIT(NL80211_IFTYPE_MESH_POINT) |
 #endif
-				 BIT(NL80211_IFTYPE_AP) |
-				 BIT(NL80211_IFTYPE_P2P_GO) },
+				 BIT(NL80211_IFTYPE_AP) },
 	{ .max = 1,	.types = BIT(NL80211_IFTYPE_ADHOC) },
+	{ .max = 1,	.types = BIT(NL80211_IFTYPE_P2P_CLIENT) |
+				 BIT(NL80211_IFTYPE_P2P_GO) },
 };
 
 static const struct ieee80211_iface_limit if_dfs_limits[] = {
