From dae0e37c2df466f5eb6459d05f392e86b4236666 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Sat, 5 Oct 2013 14:53:48 +0200
Subject: [PATCH] ARM: sunxi: Register the A31 reset IP in init_time

The A31 has a reset IP that maintains a few other IPs in reset by
default. Among these IPs are the UARTs, and most notably the timers. We
thus need to register the reset driver before initializing the timers so
that the reset timer can use the reset framework.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
Acked-by: Philipp Zabel <p.zabel@pengutronix.de>
---
 arch/arm/mach-sunxi/sunxi.c | 11 +++++++++++
 1 file changed, 11 insertions(+)

--- a/arch/arm/mach-sunxi/sunxi.c
+++ b/arch/arm/mach-sunxi/sunxi.c
@@ -10,6 +10,8 @@
  * warranty of any kind, whether express or implied.
  */
 
+#include <linux/clk-provider.h>
+#include <linux/clocksource.h>
 #include <linux/delay.h>
 #include <linux/kernel.h>
 #include <linux/init.h>
@@ -132,8 +134,17 @@ static const char * const sun6i_board_dt
 	NULL,
 };
 
+extern void __init sun6i_reset_init(void);
+static void __init sun6i_timer_init(void)
+{
+	of_clk_init(NULL);
+	sun6i_reset_init();
+	clocksource_of_init();
+}
+
 DT_MACHINE_START(SUN6I_DT, "Allwinner sun6i (A31) Family")
 	.init_machine	= sunxi_dt_init,
+	.init_time	= sun6i_timer_init,
 	.dt_compat	= sun6i_board_dt_compat,
 	.restart	= sun6i_restart,
 MACHINE_END
