From 6d3ca59232090bff1b5e1abfd3417a3859e47425 Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?Emilio=20L=C3=B3pez?= <emilio@elopez.com.ar>
Date: Mon, 23 Dec 2013 00:32:38 -0300
Subject: [PATCH] ARM: sunxi: add PLL5 and PLL6 support
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

This commit adds PLL5 and PLL6 nodes to the sun4i, sun5i and sun7i
device trees.

Signed-off-by: Emilio López <emilio@elopez.com.ar>
Acked-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun4i-a10.dtsi  | 19 +++++++++++++++++--
 arch/arm/boot/dts/sun5i-a10s.dtsi | 19 +++++++++++++++++--
 arch/arm/boot/dts/sun5i-a13.dtsi  | 19 +++++++++++++++++--
 arch/arm/boot/dts/sun7i-a20.dtsi  | 28 ++++++++++++++++------------
 4 files changed, 67 insertions(+), 18 deletions(-)

--- a/arch/arm/boot/dts/sun4i-a10.dtsi
+++ b/arch/arm/boot/dts/sun4i-a10.dtsi
@@ -73,6 +73,22 @@
 			clocks = <&osc24M>;
 		};
 
+		pll5: pll5@01c20020 {
+			#clock-cells = <1>;
+			compatible = "allwinner,sun4i-pll5-clk";
+			reg = <0x01c20020 0x4>;
+			clocks = <&osc24M>;
+			clock-output-names = "pll5_ddr", "pll5_other";
+		};
+
+		pll6: pll6@01c20028 {
+			#clock-cells = <1>;
+			compatible = "allwinner,sun4i-pll6-clk";
+			reg = <0x01c20028 0x4>;
+			clocks = <&osc24M>;
+			clock-output-names = "pll6_sata", "pll6_other", "pll6";
+		};
+
 		/* dummy is 200M */
 		cpu: cpu@01c20054 {
 			#clock-cells = <0>;
@@ -138,12 +154,11 @@
 				"apb0_ir1", "apb0_keypad";
 		};
 
-		/* dummy is pll62 */
 		apb1_mux: apb1_mux@01c20058 {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-apb1-mux-clk";
 			reg = <0x01c20058 0x4>;
-			clocks = <&osc24M>, <&dummy>, <&osc32k>;
+			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
 		};
 
 		apb1: apb1@01c20058 {
--- a/arch/arm/boot/dts/sun5i-a10s.dtsi
+++ b/arch/arm/boot/dts/sun5i-a10s.dtsi
@@ -70,6 +70,22 @@
 			clocks = <&osc24M>;
 		};
 
+		pll5: pll5@01c20020 {
+			#clock-cells = <1>;
+			compatible = "allwinner,sun4i-pll5-clk";
+			reg = <0x01c20020 0x4>;
+			clocks = <&osc24M>;
+			clock-output-names = "pll5_ddr", "pll5_other";
+		};
+
+		pll6: pll6@01c20028 {
+			#clock-cells = <1>;
+			compatible = "allwinner,sun4i-pll6-clk";
+			reg = <0x01c20028 0x4>;
+			clocks = <&osc24M>;
+			clock-output-names = "pll6_sata", "pll6_other", "pll6";
+		};
+
 		/* dummy is 200M */
 		cpu: cpu@01c20054 {
 			#clock-cells = <0>;
@@ -130,12 +146,11 @@
 				"apb0_ir", "apb0_keypad";
 		};
 
-		/* dummy is pll62 */
 		apb1_mux: apb1_mux@01c20058 {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-apb1-mux-clk";
 			reg = <0x01c20058 0x4>;
-			clocks = <&osc24M>, <&dummy>, <&osc32k>;
+			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
 		};
 
 		apb1: apb1@01c20058 {
--- a/arch/arm/boot/dts/sun5i-a13.dtsi
+++ b/arch/arm/boot/dts/sun5i-a13.dtsi
@@ -74,6 +74,22 @@
 			clocks = <&osc24M>;
 		};
 
+		pll5: pll5@01c20020 {
+			#clock-cells = <1>;
+			compatible = "allwinner,sun4i-pll5-clk";
+			reg = <0x01c20020 0x4>;
+			clocks = <&osc24M>;
+			clock-output-names = "pll5_ddr", "pll5_other";
+		};
+
+		pll6: pll6@01c20028 {
+			#clock-cells = <1>;
+			compatible = "allwinner,sun4i-pll6-clk";
+			reg = <0x01c20028 0x4>;
+			clocks = <&osc24M>;
+			clock-output-names = "pll6_sata", "pll6_other", "pll6";
+		};
+
 		/* dummy is 200M */
 		cpu: cpu@01c20054 {
 			#clock-cells = <0>;
@@ -132,12 +148,11 @@
 			clock-output-names = "apb0_codec", "apb0_pio", "apb0_ir";
 		};
 
-		/* dummy is pll6 */
 		apb1_mux: apb1_mux@01c20058 {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-apb1-mux-clk";
 			reg = <0x01c20058 0x4>;
-			clocks = <&osc24M>, <&dummy>, <&osc32k>;
+			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
 		};
 
 		apb1: apb1@01c20058 {
--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -69,23 +69,27 @@
 			clocks = <&osc24M>;
 		};
 
-		/*
-		 * This is a dummy clock, to be used as placeholder on
-		 * other mux clocks when a specific parent clock is not
-		 * yet implemented. It should be dropped when the driver
-		 * is complete.
-		 */
-		pll6: pll6 {
-			#clock-cells = <0>;
-			compatible = "fixed-clock";
-			clock-frequency = <0>;
+		pll5: pll5@01c20020 {
+			#clock-cells = <1>;
+			compatible = "allwinner,sun4i-pll5-clk";
+			reg = <0x01c20020 0x4>;
+			clocks = <&osc24M>;
+			clock-output-names = "pll5_ddr", "pll5_other";
+		};
+
+		pll6: pll6@01c20028 {
+			#clock-cells = <1>;
+			compatible = "allwinner,sun4i-pll6-clk";
+			reg = <0x01c20028 0x4>;
+			clocks = <&osc24M>;
+			clock-output-names = "pll6_sata", "pll6_other", "pll6";
 		};
 
 		cpu: cpu@01c20054 {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-cpu-clk";
 			reg = <0x01c20054 0x4>;
-			clocks = <&osc32k>, <&osc24M>, <&pll1>, <&pll6>;
+			clocks = <&osc32k>, <&osc24M>, <&pll1>, <&pll6 1>;
 		};
 
 		axi: axi@01c20054 {
@@ -144,7 +148,7 @@
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-apb1-mux-clk";
 			reg = <0x01c20058 0x4>;
-			clocks = <&osc24M>, <&pll6>, <&osc32k>;
+			clocks = <&osc24M>, <&pll6 1>, <&osc32k>;
 		};
 
 		apb1: apb1@01c20058 {
