From 27fb9d199aa3d2f89b4d0b1930062bb1a5a69a57 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Thu, 2 Jan 2014 22:05:04 +0100
Subject: [PATCH] ARM: sun6i: Add missing serial aliases

Some UART aliases have been defined, but not all of them. Add the remaining
ones to be consistent and to ease the parsing of the DT by the bootloaders.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun6i-a31.dtsi | 10 ++++++++++
 1 file changed, 10 insertions(+)

diff --git a/arch/arm/boot/dts/sun6i-a31.dtsi b/arch/arm/boot/dts/sun6i-a31.dtsi
index 5256ad9..092bf97 100644
--- a/arch/arm/boot/dts/sun6i-a31.dtsi
+++ b/arch/arm/boot/dts/sun6i-a31.dtsi
@@ -16,6 +16,16 @@
 / {
 	interrupt-parent = <&gic>;
 
+	aliases {
+		serial0 = &uart0;
+		serial1 = &uart1;
+		serial2 = &uart2;
+		serial3 = &uart3;
+		serial4 = &uart4;
+		serial5 = &uart5;
+	};
+
+
 	cpus {
 		#address-cells = <1>;
 		#size-cells = <0>;
-- 
1.8.5.5

