From a71b4438af8242f383906071205db95a8b8e7b6d Mon Sep 17 00:00:00 2001
From: FUKAUMI Naoki <naobsd@gmail.com>
Date: Wed, 20 Aug 2014 14:25:03 +0900
Subject: ARM: sun7i: Add support for Olimex A20-OLinuXino-LIME

This patch adds support for Olimex A20-OLinuXino-LIME board.

Signed-off-by: FUKAUMI Naoki <naobsd@gmail.com>
Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -293,6 +293,7 @@ dtb-$(CONFIG_ARCH_SUNXI) += \
 	sun7i-a20-bananapi.dtb \
 	sun7i-a20-cubieboard2.dtb \
 	sun7i-a20-cubietruck.dtb \
+	sun7i-a20-olinuxino-lime.dtb \
 	sun7i-a20-olinuxino-micro.dtb \
 	sun7i-a20-pcduino3.dtb
 dtb-$(CONFIG_ARCH_TEGRA) += tegra20-harmony.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/sun7i-a20-olinuxino-lime.dts
@@ -0,0 +1,136 @@
+/*
+ * This is based on sun4i-a10-olinuxino-lime.dts
+ *
+ * Copyright 2014 - Hans de Goede <hdegoede@redhat.com>
+ * Copyright (c) 2014 FUKAUMI Naoki <naobsd@gmail.com>
+ *
+ * The code contained herein is licensed under the GNU General Public
+ * License. You may obtain a copy of the GNU General Public License
+ * Version 2 or later at the following locations:
+ *
+ * http://www.opensource.org/licenses/gpl-license.html
+ * http://www.gnu.org/copyleft/gpl.html
+ */
+
+/dts-v1/;
+/include/ "sun7i-a20.dtsi"
+/include/ "sunxi-common-regulators.dtsi"
+
+/ {
+	model = "Olimex A20-OLinuXino-LIME";
+	compatible = "olimex,a20-olinuxino-lime", "allwinner,sun7i-a20";
+
+	soc@01c00000 {
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_reference_design>;
+			cd-gpios = <&pio 7 1 0>; /* PH1 */
+			cd-mode = <1>;
+			status = "okay";
+		};
+
+		usbphy: phy@01c13400 {
+			usb1_vbus-supply = <&reg_usb1_vbus>;
+			usb2_vbus-supply = <&reg_usb2_vbus>;
+			status = "okay";
+		};
+
+		ehci0: usb@01c14000 {
+			status = "okay";
+		};
+
+		ohci0: usb@01c14400 {
+			status = "okay";
+		};
+
+		ahci: sata@01c18000 {
+			target-supply = <&reg_ahci_5v>;
+			status = "okay";
+		};
+
+		ehci1: usb@01c1c000 {
+			status = "okay";
+		};
+
+		ohci1: usb@01c1c400 {
+			status = "okay";
+		};
+
+		pinctrl@01c20800 {
+			ahci_pwr_pin_olinuxinolime: ahci_pwr_pin@1 {
+				allwinner,pins = "PC3";
+				allwinner,function = "gpio_out";
+				allwinner,drive = <0>;
+				allwinner,pull = <0>;
+			};
+
+			led_pins_olinuxinolime: led_pins@0 {
+				allwinner,pins = "PH2";
+				allwinner,function = "gpio_out";
+				allwinner,drive = <1>;
+				allwinner,pull = <0>;
+			};
+		};
+
+		uart0: serial@01c28000 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&uart0_pins_a>;
+			status = "okay";
+		};
+
+		i2c0: i2c@01c2ac00 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c0_pins_a>;
+			status = "okay";
+
+			axp: axp20x@34 {
+				reg = <0x34>;
+				interrupt-parent = <&nmi_intc>;
+				interrupts = <0 8>;
+
+				axp,system-power-controller;
+
+				/include/ "x-powers-axp209.dtsi"
+			};
+		};
+
+		gmac: ethernet@01c50000 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&gmac_pins_mii_a>;
+			phy = <&phy1>;
+			phy-mode = "mii";
+			status = "okay";
+
+			phy1: ethernet-phy@1 {
+				reg = <1>;
+			};
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+		pinctrl-names = "default";
+		pinctrl-0 = <&led_pins_olinuxinolime>;
+
+		green {
+			label = "a20-olinuxino-lime:green:usr";
+			gpios = <&pio 7 2 0>;
+			default-state = "on";
+		};
+	};
+
+	reg_ahci_5v: ahci-5v {
+		pinctrl-0 = <&ahci_pwr_pin_olinuxinolime>;
+		gpio = <&pio 2 3 0>;
+		status = "okay";
+	};
+
+	reg_usb1_vbus: usb1-vbus {
+		status = "okay";
+	};
+
+	reg_usb2_vbus: usb2-vbus {
+		status = "okay";
+	};
+};
