#
# Routed point-to-point server
#
config openvpn_recipe server_tun_ptp
	option _description		"Simple server configuration for a routed point-to-point VPN"
	option _role			"server"
	option dev			"tun"
	option ifconfig			"10.0.0.1 10.0.0.2"
	option secret			"shared-secret.key"
	option keepalive		"10 60"
	option comp_lzo			"yes"
	option verb			"3"
        option mssfix			"1420"

#
# Routed point-to-point client
#
config openvpn_recipe client_tun_ptp
	option _description		"Simple client configuration for a routed point-to-point VPN"
	option _role			"client"
	option dev			"tun"
	list   remote			"vpnserver.example.org"
	option ifconfig			"10.0.0.2 10.0.0.1"
	option secret			"shared-secret.key"
	option nobind			"1"
	option comp_lzo			"yes"
	option verb			"3"

#
# Routed multi-client server
#
config openvpn_recipe server_tun
	option _description		"Server configuration for a routed multi-client VPN"
	option _role			"server"
	option dev			"tun"
	option server			"10.0.100.0 255.255.255.0"
	option ca			"ca.crt"
	option cert			"server.crt"
	option key 			"server.key"
	option dh 			"dh1024.pem"
	option keepalive		"10 60"
	option comp_lzo			"yes"
	option verb			"3"
        option mssfix			"1420"

#
# Routed client
#
config openvpn_recipe client_tun
	option _description		"Client configuration for a routed multi-client VPN"
	option _role			"client"
	option client			"1"
	option dev			"tun"
	list   remote			"vpnserver.example.org"
	option pkcs12			"my_client.p12"
	option remote_cert_tls		"server"
	option comp_lzo			"yes"
	option nobind			"1"
	option persist_key		"1"
	option persist_tun		"1"
	option verb			"3"
	option reneg_sec		"0"
	option float			"1"

#
# Multi-client ethernet bridge server
#
config openvpn_recipe server_tap_bridge
	option _description		"Server configuration for an ethernet bridge VPN"
	option _role			"server"
	option dev			"tap"
	option server_bridge		"192.168.1.1 255.255.255.0 192.168.1.128 192.168.1.254"
	option ca			"ca.crt"
	option cert			"server.crt"
	option key 			"server.key"
	option dh 			"dh1024.pem"
	option keepalive		"10 60"
	option comp_lzo			"yes"
	option verb			"3"
        option mssfix			"1420"

#
# Ethernet bridge client
#
config openvpn_recipe client_tap_bridge
	option _description		"Client configuration for an ethernet bridge VPN"
	option _role			"client"
	option client			"1"
	option dev 			"tap"
	list   remote			"vpnserver.example.org"
	option ca 			"ca.crt"
	option cert			"my_client.crt"
	option key 			"my_client.key"
	option dh 			"dh1024.pem"
	option remote_cert_tls		"server"
	option comp_lzo			"yes"
	option nobind			"1"
	option persist_key		"1"
	option verb			"3"
	option reneg_sec		"0"
	option float			"1"

