From 46d3d005e5f91d8221676cbb6307e790d4b63345 Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Wed, 5 Mar 2014 20:40:26 +0100
Subject: [PATCH] ARM: sun4i: dt: Add address- and size-cells info to i2c
 controller nodes

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun4i-a10.dtsi | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/arch/arm/boot/dts/sun4i-a10.dtsi
+++ b/arch/arm/boot/dts/sun4i-a10.dtsi
@@ -712,6 +712,8 @@
 			clocks = <&apb1_gates 0>;
 			clock-frequency = <100000>;
 			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
 		};
 
 		i2c1: i2c@01c2b000 {
@@ -721,6 +723,8 @@
 			clocks = <&apb1_gates 1>;
 			clock-frequency = <100000>;
 			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
 		};
 
 		i2c2: i2c@01c2b400 {
@@ -730,6 +734,8 @@
 			clocks = <&apb1_gates 2>;
 			clock-frequency = <100000>;
 			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
 		};
 	};
 };
