From: Felix Fietkau <nbd@openwrt.org>
Date: Sat, 15 Nov 2014 22:38:21 +0100
Subject: [PATCH] mac80211: minstrel_ht: switch to .tx_status_noskb

Signed-off-by: Felix Fietkau <nbd@openwrt.org>
---

--- a/net/mac80211/rc80211_minstrel_ht.c
+++ b/net/mac80211/rc80211_minstrel_ht.c
@@ -709,11 +709,10 @@ minstrel_aggr_check(struct ieee80211_sta
 static void
 minstrel_ht_tx_status(void *priv, struct ieee80211_supported_band *sband,
                       struct ieee80211_sta *sta, void *priv_sta,
-                      struct sk_buff *skb)
+                      struct ieee80211_tx_info *info)
 {
 	struct minstrel_ht_sta_priv *msp = priv_sta;
 	struct minstrel_ht_sta *mi = &msp->ht;
-	struct ieee80211_tx_info *info = IEEE80211_SKB_CB(skb);
 	struct ieee80211_tx_rate *ar = info->status.rates;
 	struct minstrel_rate_stats *rate, *rate2;
 	struct minstrel_priv *mp = priv;
@@ -721,7 +720,8 @@ minstrel_ht_tx_status(void *priv, struct
 	int i;
 
 	if (!msp->is_ht)
-		return mac80211_minstrel.tx_status(priv, sband, sta, &msp->legacy, skb);
+		return mac80211_minstrel.tx_status_noskb(priv, sband, sta,
+							 &msp->legacy, info);
 
 	/* This packet was aggregated but doesn't carry status info */
 	if ((info->flags & IEEE80211_TX_CTL_AMPDU) &&
@@ -1343,7 +1343,7 @@ static u32 minstrel_ht_get_expected_thro
 
 static const struct rate_control_ops mac80211_minstrel_ht = {
 	.name = "minstrel_ht",
-	.tx_status = minstrel_ht_tx_status,
+	.tx_status_noskb = minstrel_ht_tx_status,
 	.get_rate = minstrel_ht_get_rate,
 	.rate_init = minstrel_ht_rate_init,
 	.rate_update = minstrel_ht_rate_update,
