From 505ad20db47442ae2650a41eca0a7a869aace789 Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Wed, 5 Mar 2014 20:40:44 +0100
Subject: [PATCH] ARM: sun5i: dt: Add address- and size-cells info to i2c
 controller nodes

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun5i-a13.dtsi | 6 ++++++
 1 file changed, 6 insertions(+)

--- a/arch/arm/boot/dts/sun5i-a13.dtsi
+++ b/arch/arm/boot/dts/sun5i-a13.dtsi
@@ -503,6 +503,8 @@
 			clocks = <&apb1_gates 0>;
 			clock-frequency = <100000>;
 			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
 		};
 
 		i2c1: i2c@01c2b000 {
@@ -512,6 +514,8 @@
 			clocks = <&apb1_gates 1>;
 			clock-frequency = <100000>;
 			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
 		};
 
 		i2c2: i2c@01c2b400 {
@@ -521,6 +525,8 @@
 			clocks = <&apb1_gates 2>;
 			clock-frequency = <100000>;
 			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
 		};
 
 		timer@01c60000 {
