From eda34c0692e479dd9cd2b7cb70986ae57f15187f Mon Sep 17 00:00:00 2001
From: Chen-Yu Tsai <wens@csie.org>
Date: Tue, 7 Jan 2014 18:50:01 +0800
Subject: [PATCH] ARM: dts: sun7i: Add #interrupt-cells to pinctrl node

The pinctrl device is also an interrupt controller for external
interrupts. Add the missing #interrupt-cells property.

Also remove the unused #address-cells property.

Signed-off-by: Chen-Yu Tsai <wens@csie.org>
---
 arch/arm/boot/dts/sun7i-a20.dtsi | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/arch/arm/boot/dts/sun7i-a20.dtsi
+++ b/arch/arm/boot/dts/sun7i-a20.dtsi
@@ -424,7 +424,7 @@
 			clocks = <&apb0_gates 5>;
 			gpio-controller;
 			interrupt-controller;
-			#address-cells = <1>;
+			#interrupt-cells = <2>;
 			#size-cells = <0>;
 			#gpio-cells = <3>;
 
