--- a/drivers/bcma/Makefile
+++ b/drivers/bcma/Makefile
@@ -1,8 +1,10 @@
 bcma-y					+= main.o scan.o core.o sprom.o
 bcma-y					+= driver_chipcommon.o driver_chipcommon_pmu.o
+bcma-y					+= driver_chipcommon_b.o
 bcma-$(CONFIG_BCMA_SFLASH)		+= driver_chipcommon_sflash.o
 bcma-$(CONFIG_BCMA_NFLASH)		+= driver_chipcommon_nflash.o
 bcma-y					+= driver_pci.o
+bcma-y					+= driver_pcie2.o
 bcma-$(CONFIG_BCMA_DRIVER_PCI_HOSTMODE)	+= driver_pci_host.o
 bcma-$(CONFIG_BCMA_DRIVER_MIPS)		+= driver_mips.o
 bcma-$(CONFIG_BCMA_DRIVER_GMAC_CMN)	+= driver_gmac_cmn.o
--- a/drivers/bcma/driver_chipcommon.c
+++ b/drivers/bcma/driver_chipcommon.c
@@ -339,7 +339,7 @@ void bcma_chipco_serial_init(struct bcma
 		return;
 	}
 
-	irq = bcma_core_irq(cc->core);
+	irq = bcma_core_irq(cc->core, 0);
 
 	/* Determine the registers of the UARTs */
 	cc->nr_serial_ports = (cc->capabilities & BCMA_CC_CAP_NRUART);
--- a/drivers/bcma/driver_chipcommon_pmu.c
+++ b/drivers/bcma/driver_chipcommon_pmu.c
@@ -603,6 +603,8 @@ void bcma_pmu_spuravoid_pllupdate(struct
 		tmp = BCMA_CC_PMU_CTL_PLL_UPD | BCMA_CC_PMU_CTL_NOILPONW;
 		break;
 
+	case BCMA_CHIP_ID_BCM43131:
+	case BCMA_CHIP_ID_BCM43217:
 	case BCMA_CHIP_ID_BCM43227:
 	case BCMA_CHIP_ID_BCM43228:
 	case BCMA_CHIP_ID_BCM43428:
--- a/drivers/bcma/driver_gpio.c
+++ b/drivers/bcma/driver_gpio.c
@@ -76,7 +76,7 @@ static void bcma_gpio_free(struct gpio_c
 	bcma_chipco_gpio_pullup(cc, 1 << gpio, 0);
 }
 
-#if IS_BUILTIN(CONFIG_BCMA_HOST_SOC)
+#if IS_BUILTIN(CONFIG_BCM47XX)
 static int bcma_gpio_to_irq(struct gpio_chip *chip, unsigned gpio)
 {
 	struct bcma_drv_cc *cc = bcma_gpio_get_cc(chip);
@@ -152,7 +152,7 @@ static int bcma_gpio_irq_domain_init(str
 					 handle_simple_irq);
 	}
 
-	hwirq = bcma_core_irq(cc->core);
+	hwirq = bcma_core_irq(cc->core, 0);
 	err = request_irq(hwirq, bcma_gpio_irq_handler, IRQF_SHARED, "gpio",
 			  cc);
 	if (err)
@@ -183,7 +183,7 @@ static void bcma_gpio_irq_domain_exit(st
 		return;
 
 	bcma_cc_mask32(cc, BCMA_CC_IRQMASK, ~BCMA_CC_IRQ_GPIO);
-	free_irq(bcma_core_irq(cc->core), cc);
+	free_irq(bcma_core_irq(cc->core, 0), cc);
 	for (gpio = 0; gpio < chip->ngpio; gpio++) {
 		int irq = irq_find_mapping(cc->irq_domain, gpio);
 
@@ -215,10 +215,22 @@ int bcma_gpio_init(struct bcma_drv_cc *c
 	chip->set		= bcma_gpio_set_value;
 	chip->direction_input	= bcma_gpio_direction_input;
 	chip->direction_output	= bcma_gpio_direction_output;
-#if IS_BUILTIN(CONFIG_BCMA_HOST_SOC)
+#if IS_BUILTIN(CONFIG_BCM47XX)
 	chip->to_irq		= bcma_gpio_to_irq;
 #endif
-	chip->ngpio		= 16;
+#if IS_BUILTIN(CONFIG_OF)
+	if (cc->core->bus->hosttype == BCMA_HOSTTYPE_SOC)
+		chip->of_node	= cc->core->dev.of_node;
+#endif
+	switch (cc->core->bus->chipinfo.id) {
+	case BCMA_CHIP_ID_BCM5357:
+	case BCMA_CHIP_ID_BCM53572:
+		chip->ngpio	= 32;
+		break;
+	default:
+		chip->ngpio	= 16;
+	}
+
 	/* There is just one SoC in one device and its GPIO addresses should be
 	 * deterministic to address them more easily. The other buses could get
 	 * a random base number. */
@@ -243,5 +255,6 @@ int bcma_gpio_init(struct bcma_drv_cc *c
 int bcma_gpio_unregister(struct bcma_drv_cc *cc)
 {
 	bcma_gpio_irq_domain_exit(cc);
-	return gpiochip_remove(&cc->gpio);
+	gpiochip_remove(&cc->gpio);
+	return 0;
 }
--- a/drivers/bcma/driver_pci_host.c
+++ b/drivers/bcma/driver_pci_host.c
@@ -593,7 +593,7 @@ int bcma_core_pci_plat_dev_init(struct p
 	pr_info("PCI: Fixing up device %s\n", pci_name(dev));
 
 	/* Fix up interrupt lines */
-	dev->irq = bcma_core_irq(pc_host->pdev->core);
+	dev->irq = bcma_core_irq(pc_host->pdev->core, 0);
 	pci_write_config_byte(dev, PCI_INTERRUPT_LINE, dev->irq);
 
 	readrq = pcie_get_readrq(dev);
@@ -617,6 +617,6 @@ int bcma_core_pci_pcibios_map_irq(const 
 
 	pc_host = container_of(dev->bus->ops, struct bcma_drv_pci_host,
 			       pci_ops);
-	return bcma_core_irq(pc_host->pdev->core);
+	return bcma_core_irq(pc_host->pdev->core, 0);
 }
 EXPORT_SYMBOL(bcma_core_pci_pcibios_map_irq);
--- /dev/null
+++ b/drivers/bcma/driver_pcie2.c
@@ -0,0 +1,175 @@
+/*
+ * Broadcom specific AMBA
+ * PCIe Gen 2 Core
+ *
+ * Copyright 2014, Broadcom Corporation
+ * Copyright 2014, Rafał Miłecki <zajec5@gmail.com>
+ *
+ * Licensed under the GNU/GPL. See COPYING for details.
+ */
+
+#include "bcma_private.h"
+#include <linux/bcma/bcma.h>
+
+/**************************************************
+ * R/W ops.
+ **************************************************/
+
+#if 0
+static u32 bcma_core_pcie2_cfg_read(struct bcma_drv_pcie2 *pcie2, u32 addr)
+{
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDADDR, addr);
+	pcie2_read32(pcie2, BCMA_CORE_PCIE2_CONFIGINDADDR);
+	return pcie2_read32(pcie2, BCMA_CORE_PCIE2_CONFIGINDDATA);
+}
+#endif
+
+static void bcma_core_pcie2_cfg_write(struct bcma_drv_pcie2 *pcie2, u32 addr,
+				      u32 val)
+{
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDADDR, addr);
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDDATA, val);
+}
+
+/**************************************************
+ * Init.
+ **************************************************/
+
+static u32 bcma_core_pcie2_war_delay_perst_enab(struct bcma_drv_pcie2 *pcie2,
+						bool enable)
+{
+	u32 val;
+
+	/* restore back to default */
+	val = pcie2_read32(pcie2, BCMA_CORE_PCIE2_CLK_CONTROL);
+	val |= PCIE2_CLKC_DLYPERST;
+	val &= ~PCIE2_CLKC_DISSPROMLD;
+	if (enable) {
+		val &= ~PCIE2_CLKC_DLYPERST;
+		val |= PCIE2_CLKC_DISSPROMLD;
+	}
+	pcie2_write32(pcie2, (BCMA_CORE_PCIE2_CLK_CONTROL), val);
+	/* flush */
+	return pcie2_read32(pcie2, BCMA_CORE_PCIE2_CLK_CONTROL);
+}
+
+static void bcma_core_pcie2_set_ltr_vals(struct bcma_drv_pcie2 *pcie2)
+{
+	/* LTR0 */
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDADDR, 0x844);
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDDATA, 0x883c883c);
+	/* LTR1 */
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDADDR, 0x848);
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDDATA, 0x88648864);
+	/* LTR2 */
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDADDR, 0x84C);
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDDATA, 0x90039003);
+}
+
+static void bcma_core_pcie2_hw_ltr_war(struct bcma_drv_pcie2 *pcie2)
+{
+	u8 core_rev = pcie2->core->id.rev;
+	u32 devstsctr2;
+
+	if (core_rev < 2 || core_rev == 10 || core_rev > 13)
+		return;
+
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDADDR,
+		      PCIE2_CAP_DEVSTSCTRL2_OFFSET);
+	devstsctr2 = pcie2_read32(pcie2, BCMA_CORE_PCIE2_CONFIGINDDATA);
+	if (devstsctr2 & PCIE2_CAP_DEVSTSCTRL2_LTRENAB) {
+		/* force the right LTR values */
+		bcma_core_pcie2_set_ltr_vals(pcie2);
+
+		/* TODO:
+		si_core_wrapperreg(pcie2, 3, 0x60, 0x8080, 0); */
+
+		/* enable the LTR */
+		devstsctr2 |= PCIE2_CAP_DEVSTSCTRL2_LTRENAB;
+		pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDADDR,
+			      PCIE2_CAP_DEVSTSCTRL2_OFFSET);
+		pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDDATA, devstsctr2);
+
+		/* set the LTR state to be active */
+		pcie2_write32(pcie2, BCMA_CORE_PCIE2_LTR_STATE,
+			      PCIE2_LTR_ACTIVE);
+		usleep_range(1000, 2000);
+
+		/* set the LTR state to be sleep */
+		pcie2_write32(pcie2, BCMA_CORE_PCIE2_LTR_STATE,
+			      PCIE2_LTR_SLEEP);
+		usleep_range(1000, 2000);
+	}
+}
+
+static void pciedev_crwlpciegen2(struct bcma_drv_pcie2 *pcie2)
+{
+	u8 core_rev = pcie2->core->id.rev;
+	bool pciewar160, pciewar162;
+
+	pciewar160 = core_rev == 7 || core_rev == 9 || core_rev == 11;
+	pciewar162 = core_rev == 5 || core_rev == 7 || core_rev == 8 ||
+		     core_rev == 9 || core_rev == 11;
+
+	if (!pciewar160 && !pciewar162)
+		return;
+
+/* TODO */
+#if 0
+	pcie2_set32(pcie2, BCMA_CORE_PCIE2_CLK_CONTROL,
+		    PCIE_DISABLE_L1CLK_GATING);
+#if 0
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDADDR,
+		      PCIEGEN2_COE_PVT_TL_CTRL_0);
+	pcie2_mask32(pcie2, BCMA_CORE_PCIE2_CONFIGINDDATA,
+		     ~(1 << COE_PVT_TL_CTRL_0_PM_DIS_L1_REENTRY_BIT));
+#endif
+#endif
+}
+
+static void pciedev_crwlpciegen2_180(struct bcma_drv_pcie2 *pcie2)
+{
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDADDR, PCIE2_PMCR_REFUP);
+	pcie2_set32(pcie2, BCMA_CORE_PCIE2_CONFIGINDDATA, 0x1f);
+}
+
+static void pciedev_crwlpciegen2_182(struct bcma_drv_pcie2 *pcie2)
+{
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDADDR, PCIE2_SBMBX);
+	pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDDATA, 1 << 0);
+}
+
+static void pciedev_reg_pm_clk_period(struct bcma_drv_pcie2 *pcie2)
+{
+	struct bcma_drv_cc *drv_cc = &pcie2->core->bus->drv_cc;
+	u8 core_rev = pcie2->core->id.rev;
+	u32 alp_khz, pm_value;
+
+	if (core_rev <= 13) {
+		alp_khz = bcma_pmu_get_alp_clock(drv_cc) / 1000;
+		pm_value = (1000000 * 2) / alp_khz;
+		pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDADDR,
+			      PCIE2_PVT_REG_PM_CLK_PERIOD);
+		pcie2_write32(pcie2, BCMA_CORE_PCIE2_CONFIGINDDATA, pm_value);
+	}
+}
+
+void bcma_core_pcie2_init(struct bcma_drv_pcie2 *pcie2)
+{
+	struct bcma_chipinfo *ci = &pcie2->core->bus->chipinfo;
+	u32 tmp;
+
+	tmp = pcie2_read32(pcie2, BCMA_CORE_PCIE2_SPROM(54));
+	if ((tmp & 0xe) >> 1 == 2)
+		bcma_core_pcie2_cfg_write(pcie2, 0x4e0, 0x17);
+
+	/* TODO: Do we need pcie_reqsize? */
+
+	if (ci->id == BCMA_CHIP_ID_BCM4360 && ci->rev > 3)
+		bcma_core_pcie2_war_delay_perst_enab(pcie2, true);
+	bcma_core_pcie2_hw_ltr_war(pcie2);
+	pciedev_crwlpciegen2(pcie2);
+	pciedev_reg_pm_clk_period(pcie2);
+	pciedev_crwlpciegen2_180(pcie2);
+	pciedev_crwlpciegen2_182(pcie2);
+}
--- a/drivers/bcma/host_pci.c
+++ b/drivers/bcma/host_pci.c
@@ -208,6 +208,9 @@ static int bcma_host_pci_probe(struct pc
 	bus->boardinfo.vendor = bus->host_pci->subsystem_vendor;
 	bus->boardinfo.type = bus->host_pci->subsystem_device;
 
+	/* Initialize struct, detect chip */
+	bcma_init_bus(bus);
+
 	/* Register */
 	err = bcma_bus_register(bus);
 	if (err)
@@ -272,14 +275,18 @@ static SIMPLE_DEV_PM_OPS(bcma_pm_ops, bc
 static const struct pci_device_id bcma_pci_bridge_tbl[] = {
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x0576) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4313) },
-	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 43224) },
+	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 43224) },	/* 0xa8d8 */
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4331) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4353) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4357) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4358) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4359) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4365) },
+	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x43a9) },
+	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x43aa) },
 	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 0x4727) },
+	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 43227) },	/* 0xa8db, BCM43217 (sic!) */
+	{ PCI_DEVICE(PCI_VENDOR_ID_BROADCOM, 43228) },	/* 0xa8dc */
 	{ 0, },
 };
 MODULE_DEVICE_TABLE(pci, bcma_pci_bridge_tbl);
--- a/drivers/bcma/main.c
+++ b/drivers/bcma/main.c
@@ -10,6 +10,8 @@
 #include <linux/platform_device.h>
 #include <linux/bcma/bcma.h>
 #include <linux/slab.h>
+#include <linux/of_address.h>
+#include <linux/of_irq.h>
 
 MODULE_DESCRIPTION("Broadcom's specific AMBA driver");
 MODULE_LICENSE("GPL");
@@ -120,56 +122,195 @@ static void bcma_release_core_dev(struct
 	kfree(core);
 }
 
-static int bcma_register_cores(struct bcma_bus *bus)
+static bool bcma_is_core_needed_early(u16 core_id)
+{
+	switch (core_id) {
+	case BCMA_CORE_NS_NAND:
+	case BCMA_CORE_NS_QSPI:
+		return true;
+	}
+
+	return false;
+}
+
+#if defined(CONFIG_OF) && defined(CONFIG_OF_ADDRESS)
+static struct device_node *bcma_of_find_child_device(struct platform_device *parent,
+						     struct bcma_device *core)
+{
+	struct device_node *node;
+	u64 size;
+	const __be32 *reg;
+
+	if (!parent || !parent->dev.of_node)
+		return NULL;
+
+	for_each_child_of_node(parent->dev.of_node, node) {
+		reg = of_get_address(node, 0, &size, NULL);
+		if (!reg)
+			continue;
+		if (of_translate_address(node, reg) == core->addr)
+			return node;
+	}
+	return NULL;
+}
+
+static int bcma_of_irq_parse(struct platform_device *parent,
+			     struct bcma_device *core,
+			     struct of_phandle_args *out_irq, int num)
+{
+	__be32 laddr[1];
+	int rc;
+
+	if (core->dev.of_node) {
+		rc = of_irq_parse_one(core->dev.of_node, num, out_irq);
+		if (!rc)
+			return rc;
+	}
+
+	out_irq->np = parent->dev.of_node;
+	out_irq->args_count = 1;
+	out_irq->args[0] = num;
+
+	laddr[0] = cpu_to_be32(core->addr);
+	return of_irq_parse_raw(laddr, out_irq);
+}
+
+static unsigned int bcma_of_get_irq(struct platform_device *parent,
+				    struct bcma_device *core, int num)
+{
+	struct of_phandle_args out_irq;
+	int ret;
+
+	if (!parent || !parent->dev.of_node)
+		return 0;
+
+	ret = bcma_of_irq_parse(parent, core, &out_irq, num);
+	if (ret) {
+		bcma_debug(core->bus, "bcma_of_get_irq() failed with rc=%d\n",
+			   ret);
+		return 0;
+	}
+
+	return irq_create_of_mapping(&out_irq);
+}
+
+static void bcma_of_fill_device(struct platform_device *parent,
+				struct bcma_device *core)
+{
+	struct device_node *node;
+
+	node = bcma_of_find_child_device(parent, core);
+	if (node)
+		core->dev.of_node = node;
+
+	core->irq = bcma_of_get_irq(parent, core, 0);
+}
+#else
+static void bcma_of_fill_device(struct platform_device *parent,
+				struct bcma_device *core)
+{
+}
+static inline unsigned int bcma_of_get_irq(struct platform_device *parent,
+					   struct bcma_device *core, int num)
+{
+	return 0;
+}
+#endif /* CONFIG_OF */
+
+unsigned int bcma_core_irq(struct bcma_device *core, int num)
+{
+	struct bcma_bus *bus = core->bus;
+	unsigned int mips_irq;
+
+	switch (bus->hosttype) {
+	case BCMA_HOSTTYPE_PCI:
+		return bus->host_pci->irq;
+	case BCMA_HOSTTYPE_SOC:
+		if (bus->drv_mips.core && num == 0) {
+			mips_irq = bcma_core_mips_irq(core);
+			return mips_irq <= 4 ? mips_irq + 2 : 0;
+		}
+		if (bus->host_pdev)
+			return bcma_of_get_irq(bus->host_pdev, core, num);
+		return 0;
+	case BCMA_HOSTTYPE_SDIO:
+		return 0;
+	}
+
+	return 0;
+}
+EXPORT_SYMBOL(bcma_core_irq);
+
+void bcma_prepare_core(struct bcma_bus *bus, struct bcma_device *core)
+{
+	core->dev.release = bcma_release_core_dev;
+	core->dev.bus = &bcma_bus_type;
+	dev_set_name(&core->dev, "bcma%d:%d", bus->num, core->core_index);
+
+	switch (bus->hosttype) {
+	case BCMA_HOSTTYPE_PCI:
+		core->dev.parent = &bus->host_pci->dev;
+		core->dma_dev = &bus->host_pci->dev;
+		core->irq = bus->host_pci->irq;
+		break;
+	case BCMA_HOSTTYPE_SOC:
+		core->dev.dma_mask = &core->dev.coherent_dma_mask;
+		if (bus->host_pdev) {
+			core->dma_dev = &bus->host_pdev->dev;
+			core->dev.parent = &bus->host_pdev->dev;
+			bcma_of_fill_device(bus->host_pdev, core);
+		} else {
+			core->dma_dev = &core->dev;
+		}
+		break;
+	case BCMA_HOSTTYPE_SDIO:
+		break;
+	}
+}
+
+static void bcma_register_core(struct bcma_bus *bus, struct bcma_device *core)
+{
+	int err;
+
+	err = device_register(&core->dev);
+	if (err) {
+		bcma_err(bus, "Could not register dev for core 0x%03X\n",
+			 core->id.id);
+		put_device(&core->dev);
+		return;
+	}
+	core->dev_registered = true;
+}
+
+static int bcma_register_devices(struct bcma_bus *bus)
 {
 	struct bcma_device *core;
-	int err, dev_id = 0;
+	int err;
 
 	list_for_each_entry(core, &bus->cores, list) {
 		/* We support that cores ourself */
 		switch (core->id.id) {
 		case BCMA_CORE_4706_CHIPCOMMON:
 		case BCMA_CORE_CHIPCOMMON:
+		case BCMA_CORE_NS_CHIPCOMMON_B:
 		case BCMA_CORE_PCI:
 		case BCMA_CORE_PCIE:
+		case BCMA_CORE_PCIE2:
 		case BCMA_CORE_MIPS_74K:
 		case BCMA_CORE_4706_MAC_GBIT_COMMON:
 			continue;
 		}
 
+		/* Early cores were already registered */
+		if (bcma_is_core_needed_early(core->id.id))
+			continue;
+
 		/* Only first GMAC core on BCM4706 is connected and working */
 		if (core->id.id == BCMA_CORE_4706_MAC_GBIT &&
 		    core->core_unit > 0)
 			continue;
 
-		core->dev.release = bcma_release_core_dev;
-		core->dev.bus = &bcma_bus_type;
-		dev_set_name(&core->dev, "bcma%d:%d", bus->num, dev_id);
-
-		switch (bus->hosttype) {
-		case BCMA_HOSTTYPE_PCI:
-			core->dev.parent = &bus->host_pci->dev;
-			core->dma_dev = &bus->host_pci->dev;
-			core->irq = bus->host_pci->irq;
-			break;
-		case BCMA_HOSTTYPE_SOC:
-			core->dev.dma_mask = &core->dev.coherent_dma_mask;
-			core->dma_dev = &core->dev;
-			break;
-		case BCMA_HOSTTYPE_SDIO:
-			break;
-		}
-
-		err = device_register(&core->dev);
-		if (err) {
-			bcma_err(bus,
-				 "Could not register dev for core 0x%03X\n",
-				 core->id.id);
-			put_device(&core->dev);
-			continue;
-		}
-		core->dev_registered = true;
-		dev_id++;
+		bcma_register_core(bus, core);
 	}
 
 #ifdef CONFIG_BCMA_DRIVER_MIPS
@@ -246,6 +387,12 @@ int bcma_bus_register(struct bcma_bus *b
 		bcma_core_chipcommon_early_init(&bus->drv_cc);
 	}
 
+	/* Cores providing flash access go before SPROM init */
+	list_for_each_entry(core, &bus->cores, list) {
+		if (bcma_is_core_needed_early(core->id.id))
+			bcma_register_core(bus, core);
+	}
+
 	/* Try to get SPROM */
 	err = bcma_sprom_get(bus);
 	if (err == -ENOENT) {
@@ -260,6 +407,13 @@ int bcma_bus_register(struct bcma_bus *b
 		bcma_core_chipcommon_init(&bus->drv_cc);
 	}
 
+	/* Init CC core */
+	core = bcma_find_core(bus, BCMA_CORE_NS_CHIPCOMMON_B);
+	if (core) {
+		bus->drv_cc_b.core = core;
+		bcma_core_chipcommon_b_init(&bus->drv_cc_b);
+	}
+
 	/* Init MIPS core */
 	core = bcma_find_core(bus, BCMA_CORE_MIPS_74K);
 	if (core) {
@@ -281,6 +435,13 @@ int bcma_bus_register(struct bcma_bus *b
 		bcma_core_pci_init(&bus->drv_pci[1]);
 	}
 
+	/* Init PCIe Gen 2 core */
+	core = bcma_find_core_unit(bus, BCMA_CORE_PCIE2, 0);
+	if (core) {
+		bus->drv_pcie2.core = core;
+		bcma_core_pcie2_init(&bus->drv_pcie2);
+	}
+
 	/* Init GBIT MAC COMMON core */
 	core = bcma_find_core(bus, BCMA_CORE_4706_MAC_GBIT_COMMON);
 	if (core) {
@@ -289,7 +450,7 @@ int bcma_bus_register(struct bcma_bus *b
 	}
 
 	/* Register found cores */
-	bcma_register_cores(bus);
+	bcma_register_devices(bus);
 
 	bcma_info(bus, "Bus registered\n");
 
@@ -307,6 +468,8 @@ void bcma_bus_unregister(struct bcma_bus
 	else if (err)
 		bcma_err(bus, "Can not unregister GPIO driver: %i\n", err);
 
+	bcma_core_chipcommon_b_free(&bus->drv_cc_b);
+
 	cores[0] = bcma_find_core(bus, BCMA_CORE_MIPS_74K);
 	cores[1] = bcma_find_core(bus, BCMA_CORE_PCIE);
 	cores[2] = bcma_find_core(bus, BCMA_CORE_4706_MAC_GBIT_COMMON);
@@ -326,8 +489,6 @@ int __init bcma_bus_early_register(struc
 	struct bcma_device *core;
 	struct bcma_device_id match;
 
-	bcma_init_bus(bus);
-
 	match.manuf = BCMA_MANUF_BCM;
 	match.id = bcma_cc_core_id(bus);
 	match.class = BCMA_CL_SIM;
@@ -486,6 +647,11 @@ static int __init bcma_modinit(void)
 	if (err)
 		return err;
 
+	err = bcma_host_soc_register_driver();
+	if (err) {
+		pr_err("SoC host initialization failed\n");
+		err = 0;
+	}
 #ifdef CONFIG_BCMA_HOST_PCI
 	err = bcma_host_pci_init();
 	if (err) {
@@ -503,6 +669,7 @@ static void __exit bcma_modexit(void)
 #ifdef CONFIG_BCMA_HOST_PCI
 	bcma_host_pci_exit();
 #endif
+	bcma_host_soc_unregister_driver();
 	bus_unregister(&bcma_bus_type);
 }
 module_exit(bcma_modexit)
--- a/drivers/bcma/sprom.c
+++ b/drivers/bcma/sprom.c
@@ -201,6 +201,23 @@ static int bcma_sprom_valid(struct bcma_
 		SPEX(_field[7], _offset + 14, _mask, _shift);	\
 	} while (0)
 
+static s8 sprom_extract_antgain(const u16 *in, u16 offset, u16 mask, u16 shift)
+{
+	u16 v;
+	u8 gain;
+
+	v = in[SPOFF(offset)];
+	gain = (v & mask) >> shift;
+	if (gain == 0xFF) {
+		gain = 8; /* If unset use 2dBm */
+	} else {
+		/* Q5.2 Fractional part is stored in 0xC0 */
+		gain = ((gain & 0xC0) >> 6) | ((gain & 0x3F) << 2);
+	}
+
+	return (s8)gain;
+}
+
 static void bcma_sprom_extract_r8(struct bcma_bus *bus, const u16 *sprom)
 {
 	u16 v, o;
@@ -381,14 +398,22 @@ static void bcma_sprom_extract_r8(struct
 	SPEX32(ofdm5ghpo, SSB_SPROM8_OFDM5GHPO, ~0, 0);
 
 	/* Extract the antenna gain values. */
-	SPEX(antenna_gain.a0, SSB_SPROM8_AGAIN01,
-	     SSB_SPROM8_AGAIN0, SSB_SPROM8_AGAIN0_SHIFT);
-	SPEX(antenna_gain.a1, SSB_SPROM8_AGAIN01,
-	     SSB_SPROM8_AGAIN1, SSB_SPROM8_AGAIN1_SHIFT);
-	SPEX(antenna_gain.a2, SSB_SPROM8_AGAIN23,
-	     SSB_SPROM8_AGAIN2, SSB_SPROM8_AGAIN2_SHIFT);
-	SPEX(antenna_gain.a3, SSB_SPROM8_AGAIN23,
-	     SSB_SPROM8_AGAIN3, SSB_SPROM8_AGAIN3_SHIFT);
+	bus->sprom.antenna_gain.a0 = sprom_extract_antgain(sprom,
+							   SSB_SPROM8_AGAIN01,
+							   SSB_SPROM8_AGAIN0,
+							   SSB_SPROM8_AGAIN0_SHIFT);
+	bus->sprom.antenna_gain.a1 = sprom_extract_antgain(sprom,
+							   SSB_SPROM8_AGAIN01,
+							   SSB_SPROM8_AGAIN1,
+							   SSB_SPROM8_AGAIN1_SHIFT);
+	bus->sprom.antenna_gain.a2 = sprom_extract_antgain(sprom,
+							   SSB_SPROM8_AGAIN23,
+							   SSB_SPROM8_AGAIN2,
+							   SSB_SPROM8_AGAIN2_SHIFT);
+	bus->sprom.antenna_gain.a3 = sprom_extract_antgain(sprom,
+							   SSB_SPROM8_AGAIN23,
+							   SSB_SPROM8_AGAIN3,
+							   SSB_SPROM8_AGAIN3_SHIFT);
 
 	SPEX(leddc_on_time, SSB_SPROM8_LEDDC, SSB_SPROM8_LEDDC_ON,
 	     SSB_SPROM8_LEDDC_ON_SHIFT);
@@ -509,6 +534,8 @@ static bool bcma_sprom_onchip_available(
 		/* for these chips OTP is always available */
 		present = true;
 		break;
+	case BCMA_CHIP_ID_BCM43131:
+	case BCMA_CHIP_ID_BCM43217:
 	case BCMA_CHIP_ID_BCM43227:
 	case BCMA_CHIP_ID_BCM43228:
 	case BCMA_CHIP_ID_BCM43428:
--- a/include/linux/bcma/bcma.h
+++ b/include/linux/bcma/bcma.h
@@ -6,6 +6,7 @@
 
 #include <linux/bcma/bcma_driver_chipcommon.h>
 #include <linux/bcma/bcma_driver_pci.h>
+#include <linux/bcma/bcma_driver_pcie2.h>
 #include <linux/bcma/bcma_driver_mips.h>
 #include <linux/bcma/bcma_driver_gmac_cmn.h>
 #include <linux/ssb/ssb.h> /* SPROM sharing */
@@ -72,17 +73,17 @@ struct bcma_host_ops {
 /* Core-ID values. */
 #define BCMA_CORE_OOB_ROUTER		0x367	/* Out of band */
 #define BCMA_CORE_4706_CHIPCOMMON	0x500
-#define BCMA_CORE_PCIEG2		0x501
-#define BCMA_CORE_DMA			0x502
-#define BCMA_CORE_SDIO3			0x503
-#define BCMA_CORE_USB20			0x504
-#define BCMA_CORE_USB30			0x505
-#define BCMA_CORE_A9JTAG		0x506
-#define BCMA_CORE_DDR23			0x507
-#define BCMA_CORE_ROM			0x508
-#define BCMA_CORE_NAND			0x509
-#define BCMA_CORE_QSPI			0x50A
-#define BCMA_CORE_CHIPCOMMON_B		0x50B
+#define BCMA_CORE_NS_PCIEG2		0x501
+#define BCMA_CORE_NS_DMA		0x502
+#define BCMA_CORE_NS_SDIO3		0x503
+#define BCMA_CORE_NS_USB20		0x504
+#define BCMA_CORE_NS_USB30		0x505
+#define BCMA_CORE_NS_A9JTAG		0x506
+#define BCMA_CORE_NS_DDR23		0x507
+#define BCMA_CORE_NS_ROM		0x508
+#define BCMA_CORE_NS_NAND		0x509
+#define BCMA_CORE_NS_QSPI		0x50A
+#define BCMA_CORE_NS_CHIPCOMMON_B	0x50B
 #define BCMA_CORE_4706_SOC_RAM		0x50E
 #define BCMA_CORE_ARMCA9		0x510
 #define BCMA_CORE_4706_MAC_GBIT		0x52D
@@ -157,6 +158,9 @@ struct bcma_host_ops {
 /* Chip IDs of PCIe devices */
 #define BCMA_CHIP_ID_BCM4313	0x4313
 #define BCMA_CHIP_ID_BCM43142	43142
+#define BCMA_CHIP_ID_BCM43131	43131
+#define BCMA_CHIP_ID_BCM43217	43217
+#define BCMA_CHIP_ID_BCM43222	43222
 #define BCMA_CHIP_ID_BCM43224	43224
 #define  BCMA_PKG_ID_BCM43224_FAB_CSM	0x8
 #define  BCMA_PKG_ID_BCM43224_FAB_SMIC	0xa
@@ -263,7 +267,7 @@ struct bcma_device {
 	u8 core_unit;
 
 	u32 addr;
-	u32 addr1;
+	u32 addr_s[8];
 	u32 wrap;
 
 	void __iomem *io_addr;
@@ -319,6 +323,8 @@ struct bcma_bus {
 		struct pci_dev *host_pci;
 		/* Pointer to the SDIO device (only for BCMA_HOSTTYPE_SDIO) */
 		struct sdio_func *host_sdio;
+		/* Pointer to platform device (only for BCMA_HOSTTYPE_SOC) */
+		struct platform_device *host_pdev;
 	};
 
 	struct bcma_chipinfo chipinfo;
@@ -328,11 +334,12 @@ struct bcma_bus {
 	struct bcma_device *mapped_core;
 	struct list_head cores;
 	u8 nr_cores;
-	u8 init_done:1;
 	u8 num;
 
 	struct bcma_drv_cc drv_cc;
+	struct bcma_drv_cc_b drv_cc_b;
 	struct bcma_drv_pci drv_pci[2];
+	struct bcma_drv_pcie2 drv_pcie2;
 	struct bcma_drv_mips drv_mips;
 	struct bcma_drv_gmac_cmn drv_gmac_cmn;
 
@@ -440,4 +447,6 @@ extern u32 bcma_chipco_pll_read(struct b
 #define  BCMA_DMA_TRANSLATION_DMA64_CMT	0x80000000 /* Client Mode Translation for 64-bit DMA */
 extern u32 bcma_core_dma_translation(struct bcma_device *core);
 
+extern unsigned int bcma_core_irq(struct bcma_device *core, int num);
+
 #endif /* LINUX_BCMA_H_ */
--- a/include/linux/bcma/bcma_driver_mips.h
+++ b/include/linux/bcma/bcma_driver_mips.h
@@ -43,12 +43,12 @@ struct bcma_drv_mips {
 extern void bcma_core_mips_init(struct bcma_drv_mips *mcore);
 extern void bcma_core_mips_early_init(struct bcma_drv_mips *mcore);
 
-extern unsigned int bcma_core_irq(struct bcma_device *core);
+extern unsigned int bcma_core_mips_irq(struct bcma_device *dev);
 #else
 static inline void bcma_core_mips_init(struct bcma_drv_mips *mcore) { }
 static inline void bcma_core_mips_early_init(struct bcma_drv_mips *mcore) { }
 
-static inline unsigned int bcma_core_irq(struct bcma_device *core)
+static inline unsigned int bcma_core_mips_irq(struct bcma_device *dev)
 {
 	return 0;
 }
--- /dev/null
+++ b/include/linux/bcma/bcma_driver_pcie2.h
@@ -0,0 +1,158 @@
+#ifndef LINUX_BCMA_DRIVER_PCIE2_H_
+#define LINUX_BCMA_DRIVER_PCIE2_H_
+
+#define BCMA_CORE_PCIE2_CLK_CONTROL		0x0000
+#define  PCIE2_CLKC_RST_OE			0x0001 /* When set, drives PCI_RESET out to pin */
+#define  PCIE2_CLKC_RST				0x0002 /* Value driven out to pin */
+#define  PCIE2_CLKC_SPERST			0x0004 /* SurvivePeRst */
+#define  PCIE2_CLKC_DISABLE_L1CLK_GATING	0x0010
+#define  PCIE2_CLKC_DLYPERST			0x0100 /* Delay PeRst to CoE Core */
+#define  PCIE2_CLKC_DISSPROMLD			0x0200 /* DisableSpromLoadOnPerst */
+#define  PCIE2_CLKC_WAKE_MODE_L2		0x1000 /* Wake on L2 */
+#define BCMA_CORE_PCIE2_RC_PM_CONTROL		0x0004
+#define BCMA_CORE_PCIE2_RC_PM_STATUS		0x0008
+#define BCMA_CORE_PCIE2_EP_PM_CONTROL		0x000C
+#define BCMA_CORE_PCIE2_EP_PM_STATUS		0x0010
+#define BCMA_CORE_PCIE2_EP_LTR_CONTROL		0x0014
+#define BCMA_CORE_PCIE2_EP_LTR_STATUS		0x0018
+#define BCMA_CORE_PCIE2_EP_OBFF_STATUS		0x001C
+#define BCMA_CORE_PCIE2_PCIE_ERR_STATUS		0x0020
+#define BCMA_CORE_PCIE2_RC_AXI_CONFIG		0x0100
+#define BCMA_CORE_PCIE2_EP_AXI_CONFIG		0x0104
+#define BCMA_CORE_PCIE2_RXDEBUG_STATUS0		0x0108
+#define BCMA_CORE_PCIE2_RXDEBUG_CONTROL0	0x010C
+#define BCMA_CORE_PCIE2_CONFIGINDADDR		0x0120
+#define BCMA_CORE_PCIE2_CONFIGINDDATA		0x0124
+#define BCMA_CORE_PCIE2_MDIOCONTROL		0x0128
+#define BCMA_CORE_PCIE2_MDIOWRDATA		0x012C
+#define BCMA_CORE_PCIE2_MDIORDDATA		0x0130
+#define BCMA_CORE_PCIE2_DATAINTF		0x0180
+#define BCMA_CORE_PCIE2_D2H_INTRLAZY_0		0x0188
+#define BCMA_CORE_PCIE2_H2D_INTRLAZY_0		0x018c
+#define BCMA_CORE_PCIE2_H2D_INTSTAT_0		0x0190
+#define BCMA_CORE_PCIE2_H2D_INTMASK_0		0x0194
+#define BCMA_CORE_PCIE2_D2H_INTSTAT_0		0x0198
+#define BCMA_CORE_PCIE2_D2H_INTMASK_0		0x019c
+#define BCMA_CORE_PCIE2_LTR_STATE		0x01A0 /* Latency Tolerance Reporting */
+#define  PCIE2_LTR_ACTIVE			2
+#define  PCIE2_LTR_ACTIVE_IDLE			1
+#define  PCIE2_LTR_SLEEP			0
+#define  PCIE2_LTR_FINAL_MASK			0x300
+#define  PCIE2_LTR_FINAL_SHIFT			8
+#define BCMA_CORE_PCIE2_PWR_INT_STATUS		0x01A4
+#define BCMA_CORE_PCIE2_PWR_INT_MASK		0x01A8
+#define BCMA_CORE_PCIE2_CFG_ADDR		0x01F8
+#define BCMA_CORE_PCIE2_CFG_DATA		0x01FC
+#define BCMA_CORE_PCIE2_SYS_EQ_PAGE		0x0200
+#define BCMA_CORE_PCIE2_SYS_MSI_PAGE		0x0204
+#define BCMA_CORE_PCIE2_SYS_MSI_INTREN		0x0208
+#define BCMA_CORE_PCIE2_SYS_MSI_CTRL0		0x0210
+#define BCMA_CORE_PCIE2_SYS_MSI_CTRL1		0x0214
+#define BCMA_CORE_PCIE2_SYS_MSI_CTRL2		0x0218
+#define BCMA_CORE_PCIE2_SYS_MSI_CTRL3		0x021C
+#define BCMA_CORE_PCIE2_SYS_MSI_CTRL4		0x0220
+#define BCMA_CORE_PCIE2_SYS_MSI_CTRL5		0x0224
+#define BCMA_CORE_PCIE2_SYS_EQ_HEAD0		0x0250
+#define BCMA_CORE_PCIE2_SYS_EQ_TAIL0		0x0254
+#define BCMA_CORE_PCIE2_SYS_EQ_HEAD1		0x0258
+#define BCMA_CORE_PCIE2_SYS_EQ_TAIL1		0x025C
+#define BCMA_CORE_PCIE2_SYS_EQ_HEAD2		0x0260
+#define BCMA_CORE_PCIE2_SYS_EQ_TAIL2		0x0264
+#define BCMA_CORE_PCIE2_SYS_EQ_HEAD3		0x0268
+#define BCMA_CORE_PCIE2_SYS_EQ_TAIL3		0x026C
+#define BCMA_CORE_PCIE2_SYS_EQ_HEAD4		0x0270
+#define BCMA_CORE_PCIE2_SYS_EQ_TAIL4		0x0274
+#define BCMA_CORE_PCIE2_SYS_EQ_HEAD5		0x0278
+#define BCMA_CORE_PCIE2_SYS_EQ_TAIL5		0x027C
+#define BCMA_CORE_PCIE2_SYS_RC_INTX_EN		0x0330
+#define BCMA_CORE_PCIE2_SYS_RC_INTX_CSR		0x0334
+#define BCMA_CORE_PCIE2_SYS_MSI_REQ		0x0340
+#define BCMA_CORE_PCIE2_SYS_HOST_INTR_EN	0x0344
+#define BCMA_CORE_PCIE2_SYS_HOST_INTR_CSR	0x0348
+#define BCMA_CORE_PCIE2_SYS_HOST_INTR0		0x0350
+#define BCMA_CORE_PCIE2_SYS_HOST_INTR1		0x0354
+#define BCMA_CORE_PCIE2_SYS_HOST_INTR2		0x0358
+#define BCMA_CORE_PCIE2_SYS_HOST_INTR3		0x035C
+#define BCMA_CORE_PCIE2_SYS_EP_INT_EN0		0x0360
+#define BCMA_CORE_PCIE2_SYS_EP_INT_EN1		0x0364
+#define BCMA_CORE_PCIE2_SYS_EP_INT_CSR0		0x0370
+#define BCMA_CORE_PCIE2_SYS_EP_INT_CSR1		0x0374
+#define BCMA_CORE_PCIE2_SPROM(wordoffset)	(0x0800 + ((wordoffset) * 2))
+#define BCMA_CORE_PCIE2_FUNC0_IMAP0_0		0x0C00
+#define BCMA_CORE_PCIE2_FUNC0_IMAP0_1		0x0C04
+#define BCMA_CORE_PCIE2_FUNC0_IMAP0_2		0x0C08
+#define BCMA_CORE_PCIE2_FUNC0_IMAP0_3		0x0C0C
+#define BCMA_CORE_PCIE2_FUNC0_IMAP0_4		0x0C10
+#define BCMA_CORE_PCIE2_FUNC0_IMAP0_5		0x0C14
+#define BCMA_CORE_PCIE2_FUNC0_IMAP0_6		0x0C18
+#define BCMA_CORE_PCIE2_FUNC0_IMAP0_7		0x0C1C
+#define BCMA_CORE_PCIE2_FUNC1_IMAP0_0		0x0C20
+#define BCMA_CORE_PCIE2_FUNC1_IMAP0_1		0x0C24
+#define BCMA_CORE_PCIE2_FUNC1_IMAP0_2		0x0C28
+#define BCMA_CORE_PCIE2_FUNC1_IMAP0_3		0x0C2C
+#define BCMA_CORE_PCIE2_FUNC1_IMAP0_4		0x0C30
+#define BCMA_CORE_PCIE2_FUNC1_IMAP0_5		0x0C34
+#define BCMA_CORE_PCIE2_FUNC1_IMAP0_6		0x0C38
+#define BCMA_CORE_PCIE2_FUNC1_IMAP0_7		0x0C3C
+#define BCMA_CORE_PCIE2_FUNC0_IMAP1		0x0C80
+#define BCMA_CORE_PCIE2_FUNC1_IMAP1		0x0C88
+#define BCMA_CORE_PCIE2_FUNC0_IMAP2		0x0CC0
+#define BCMA_CORE_PCIE2_FUNC1_IMAP2		0x0CC8
+#define BCMA_CORE_PCIE2_IARR0_LOWER		0x0D00
+#define BCMA_CORE_PCIE2_IARR0_UPPER		0x0D04
+#define BCMA_CORE_PCIE2_IARR1_LOWER		0x0D08
+#define BCMA_CORE_PCIE2_IARR1_UPPER		0x0D0C
+#define BCMA_CORE_PCIE2_IARR2_LOWER		0x0D10
+#define BCMA_CORE_PCIE2_IARR2_UPPER		0x0D14
+#define BCMA_CORE_PCIE2_OARR0			0x0D20
+#define BCMA_CORE_PCIE2_OARR1			0x0D28
+#define BCMA_CORE_PCIE2_OARR2			0x0D30
+#define BCMA_CORE_PCIE2_OMAP0_LOWER		0x0D40
+#define BCMA_CORE_PCIE2_OMAP0_UPPER		0x0D44
+#define BCMA_CORE_PCIE2_OMAP1_LOWER		0x0D48
+#define BCMA_CORE_PCIE2_OMAP1_UPPER		0x0D4C
+#define BCMA_CORE_PCIE2_OMAP2_LOWER		0x0D50
+#define BCMA_CORE_PCIE2_OMAP2_UPPER		0x0D54
+#define BCMA_CORE_PCIE2_FUNC1_IARR1_SIZE	0x0D58
+#define BCMA_CORE_PCIE2_FUNC1_IARR2_SIZE	0x0D5C
+#define BCMA_CORE_PCIE2_MEM_CONTROL		0x0F00
+#define BCMA_CORE_PCIE2_MEM_ECC_ERRLOG0		0x0F04
+#define BCMA_CORE_PCIE2_MEM_ECC_ERRLOG1		0x0F08
+#define BCMA_CORE_PCIE2_LINK_STATUS		0x0F0C
+#define BCMA_CORE_PCIE2_STRAP_STATUS		0x0F10
+#define BCMA_CORE_PCIE2_RESET_STATUS		0x0F14
+#define BCMA_CORE_PCIE2_RESETEN_IN_LINKDOWN	0x0F18
+#define BCMA_CORE_PCIE2_MISC_INTR_EN		0x0F1C
+#define BCMA_CORE_PCIE2_TX_DEBUG_CFG		0x0F20
+#define BCMA_CORE_PCIE2_MISC_CONFIG		0x0F24
+#define BCMA_CORE_PCIE2_MISC_STATUS		0x0F28
+#define BCMA_CORE_PCIE2_INTR_EN			0x0F30
+#define BCMA_CORE_PCIE2_INTR_CLEAR		0x0F34
+#define BCMA_CORE_PCIE2_INTR_STATUS		0x0F38
+
+/* PCIE gen2 config regs */
+#define PCIE2_INTSTATUS				0x090
+#define PCIE2_INTMASK				0x094
+#define PCIE2_SBMBX				0x098
+
+#define PCIE2_PMCR_REFUP			0x1814 /* Trefup time */
+
+#define PCIE2_CAP_DEVSTSCTRL2_OFFSET		0xD4
+#define PCIE2_CAP_DEVSTSCTRL2_LTRENAB		0x400
+#define PCIE2_PVT_REG_PM_CLK_PERIOD		0x184c
+
+struct bcma_drv_pcie2 {
+	struct bcma_device *core;
+};
+
+#define pcie2_read16(pcie2, offset)		bcma_read16((pcie2)->core, offset)
+#define pcie2_read32(pcie2, offset)		bcma_read32((pcie2)->core, offset)
+#define pcie2_write16(pcie2, offset, val)	bcma_write16((pcie2)->core, offset, val)
+#define pcie2_write32(pcie2, offset, val)	bcma_write32((pcie2)->core, offset, val)
+
+#define pcie2_set32(pcie2, offset, set)		bcma_set32((pcie2)->core, offset, set)
+#define pcie2_mask32(pcie2, offset, mask)	bcma_mask32((pcie2)->core, offset, mask)
+
+void bcma_core_pcie2_init(struct bcma_drv_pcie2 *pcie2);
+
+#endif /* LINUX_BCMA_DRIVER_PCIE2_H_ */
--- a/drivers/bcma/scan.c
+++ b/drivers/bcma/scan.c
@@ -32,17 +32,17 @@ static const struct bcma_device_id_name 
 	{ BCMA_CORE_4706_CHIPCOMMON, "BCM4706 ChipCommon" },
 	{ BCMA_CORE_4706_SOC_RAM, "BCM4706 SOC RAM" },
 	{ BCMA_CORE_4706_MAC_GBIT, "BCM4706 GBit MAC" },
-	{ BCMA_CORE_PCIEG2, "PCIe Gen 2" },
-	{ BCMA_CORE_DMA, "DMA" },
-	{ BCMA_CORE_SDIO3, "SDIO3" },
-	{ BCMA_CORE_USB20, "USB 2.0" },
-	{ BCMA_CORE_USB30, "USB 3.0" },
-	{ BCMA_CORE_A9JTAG, "ARM Cortex A9 JTAG" },
-	{ BCMA_CORE_DDR23, "Denali DDR2/DDR3 memory controller" },
-	{ BCMA_CORE_ROM, "ROM" },
-	{ BCMA_CORE_NAND, "NAND flash controller" },
-	{ BCMA_CORE_QSPI, "SPI flash controller" },
-	{ BCMA_CORE_CHIPCOMMON_B, "Chipcommon B" },
+	{ BCMA_CORE_NS_PCIEG2, "PCIe Gen 2" },
+	{ BCMA_CORE_NS_DMA, "DMA" },
+	{ BCMA_CORE_NS_SDIO3, "SDIO3" },
+	{ BCMA_CORE_NS_USB20, "USB 2.0" },
+	{ BCMA_CORE_NS_USB30, "USB 3.0" },
+	{ BCMA_CORE_NS_A9JTAG, "ARM Cortex A9 JTAG" },
+	{ BCMA_CORE_NS_DDR23, "Denali DDR2/DDR3 memory controller" },
+	{ BCMA_CORE_NS_ROM, "ROM" },
+	{ BCMA_CORE_NS_NAND, "NAND flash controller" },
+	{ BCMA_CORE_NS_QSPI, "SPI flash controller" },
+	{ BCMA_CORE_NS_CHIPCOMMON_B, "Chipcommon B" },
 	{ BCMA_CORE_ARMCA9, "ARM Cortex A9 core (ihost)" },
 	{ BCMA_CORE_AMEMC, "AMEMC (DDR)" },
 	{ BCMA_CORE_ALTA, "ALTA (I2S)" },
@@ -276,7 +276,7 @@ static int bcma_get_next_core(struct bcm
 			      struct bcma_device *core)
 {
 	u32 tmp;
-	u8 i, j;
+	u8 i, j, k;
 	s32 cia, cib;
 	u8 ports[2], wrappers[2];
 
@@ -314,6 +314,7 @@ static int bcma_get_next_core(struct bcm
 		/* Some specific cores don't need wrappers */
 		switch (core->id.id) {
 		case BCMA_CORE_4706_MAC_GBIT_COMMON:
+		case BCMA_CORE_NS_CHIPCOMMON_B:
 		/* Not used yet: case BCMA_CORE_OOB_ROUTER: */
 			break;
 		default:
@@ -367,6 +368,7 @@ static int bcma_get_next_core(struct bcm
 	core->addr = tmp;
 
 	/* get & parse slave ports */
+	k = 0;
 	for (i = 0; i < ports[1]; i++) {
 		for (j = 0; ; j++) {
 			tmp = bcma_erom_get_addr_desc(bus, eromptr,
@@ -376,9 +378,9 @@ static int bcma_get_next_core(struct bcm
 				/* pr_debug("erom: slave port %d "
 				 * "has %d descriptors\n", i, j); */
 				break;
-			} else {
-				if (i == 0 && j == 0)
-					core->addr1 = tmp;
+			} else if (k < ARRAY_SIZE(core->addr_s)) {
+				core->addr_s[k] = tmp;
+				k++;
 			}
 		}
 	}
@@ -421,10 +423,13 @@ static int bcma_get_next_core(struct bcm
 		core->io_addr = ioremap_nocache(core->addr, BCMA_CORE_SIZE);
 		if (!core->io_addr)
 			return -ENOMEM;
-		core->io_wrap = ioremap_nocache(core->wrap, BCMA_CORE_SIZE);
-		if (!core->io_wrap) {
-			iounmap(core->io_addr);
-			return -ENOMEM;
+		if (core->wrap) {
+			core->io_wrap = ioremap_nocache(core->wrap,
+							BCMA_CORE_SIZE);
+			if (!core->io_wrap) {
+				iounmap(core->io_addr);
+				return -ENOMEM;
+			}
 		}
 	}
 	return 0;
@@ -434,9 +439,7 @@ void bcma_init_bus(struct bcma_bus *bus)
 {
 	s32 tmp;
 	struct bcma_chipinfo *chipinfo = &(bus->chipinfo);
-
-	if (bus->init_done)
-		return;
+	char chip_id[8];
 
 	INIT_LIST_HEAD(&bus->cores);
 	bus->nr_cores = 0;
@@ -447,10 +450,11 @@ void bcma_init_bus(struct bcma_bus *bus)
 	chipinfo->id = (tmp & BCMA_CC_ID_ID) >> BCMA_CC_ID_ID_SHIFT;
 	chipinfo->rev = (tmp & BCMA_CC_ID_REV) >> BCMA_CC_ID_REV_SHIFT;
 	chipinfo->pkg = (tmp & BCMA_CC_ID_PKG) >> BCMA_CC_ID_PKG_SHIFT;
-	bcma_info(bus, "Found chip with id 0x%04X, rev 0x%02X and package 0x%02X\n",
-		  chipinfo->id, chipinfo->rev, chipinfo->pkg);
 
-	bus->init_done = true;
+	snprintf(chip_id, ARRAY_SIZE(chip_id),
+		 (chipinfo->id > 0x9999) ? "%d" : "0x%04X", chipinfo->id);
+	bcma_info(bus, "Found chip with id %s, rev 0x%02X and package 0x%02X\n",
+		  chip_id, chipinfo->rev, chipinfo->pkg);
 }
 
 int bcma_bus_scan(struct bcma_bus *bus)
@@ -460,8 +464,6 @@ int bcma_bus_scan(struct bcma_bus *bus)
 
 	int err, core_num = 0;
 
-	bcma_init_bus(bus);
-
 	erombase = bcma_scan_read32(bus, 0, BCMA_CC_EROM);
 	if (bus->hosttype == BCMA_HOSTTYPE_SOC) {
 		eromptr = ioremap_nocache(erombase, BCMA_CORE_SIZE);
@@ -503,6 +505,7 @@ int bcma_bus_scan(struct bcma_bus *bus)
 		bus->nr_cores++;
 		other_core = bcma_find_core_reverse(bus, core->id.id);
 		core->core_unit = (other_core == NULL) ? 0 : other_core->core_unit + 1;
+		bcma_prepare_core(bus, core);
 
 		bcma_info(bus, "Core %d found: %s (manuf 0x%03X, id 0x%03X, rev 0x%02X, class 0x%X)\n",
 			  core->core_index, bcma_device_name(&core->id),
--- a/drivers/bcma/host_soc.c
+++ b/drivers/bcma/host_soc.c
@@ -7,6 +7,9 @@
 
 #include "bcma_private.h"
 #include "scan.h"
+#include <linux/slab.h>
+#include <linux/module.h>
+#include <linux/of_address.h>
 #include <linux/bcma/bcma.h>
 #include <linux/bcma/bcma_soc.h>
 
@@ -134,12 +137,16 @@ static void bcma_host_soc_block_write(st
 
 static u32 bcma_host_soc_aread32(struct bcma_device *core, u16 offset)
 {
+	if (WARN_ONCE(!core->io_wrap, "Accessed core has no wrapper/agent\n"))
+		return ~0;
 	return readl(core->io_wrap + offset);
 }
 
 static void bcma_host_soc_awrite32(struct bcma_device *core, u16 offset,
 				  u32 value)
 {
+	if (WARN_ONCE(!core->io_wrap, "Accessed core has no wrapper/agent\n"))
+		return;
 	writel(value, core->io_wrap + offset);
 }
 
@@ -161,7 +168,6 @@ static const struct bcma_host_ops bcma_h
 int __init bcma_host_soc_register(struct bcma_soc *soc)
 {
 	struct bcma_bus *bus = &soc->bus;
-	int err;
 
 	/* iomap only first core. We have to read some register on this core
 	 * to scan the bus.
@@ -173,11 +179,100 @@ int __init bcma_host_soc_register(struct
 	/* Host specific */
 	bus->hosttype = BCMA_HOSTTYPE_SOC;
 	bus->ops = &bcma_host_soc_ops;
+	bus->host_pdev = NULL;
 
-	/* Register */
+	/* Initialize struct, detect chip */
+	bcma_init_bus(bus);
+
+	return 0;
+}
+
+int __init bcma_host_soc_init(struct bcma_soc *soc)
+{
+	struct bcma_bus *bus = &soc->bus;
+	int err;
+
+	/* Scan bus and initialize it */
 	err = bcma_bus_early_register(bus, &soc->core_cc, &soc->core_mips);
 	if (err)
 		iounmap(bus->mmio);
 
 	return err;
 }
+
+#ifdef CONFIG_OF
+static int bcma_host_soc_probe(struct platform_device *pdev)
+{
+	struct device *dev = &pdev->dev;
+	struct device_node *np = dev->of_node;
+	struct bcma_bus *bus;
+	int err;
+
+	/* Alloc */
+	bus = devm_kzalloc(dev, sizeof(*bus), GFP_KERNEL);
+	if (!bus)
+		return -ENOMEM;
+
+	/* Map MMIO */
+	bus->mmio = of_iomap(np, 0);
+	if (!bus->mmio)
+		return -ENOMEM;
+
+	/* Host specific */
+	bus->hosttype = BCMA_HOSTTYPE_SOC;
+	bus->ops = &bcma_host_soc_ops;
+	bus->host_pdev = pdev;
+
+	/* Initialize struct, detect chip */
+	bcma_init_bus(bus);
+
+	/* Register */
+	err = bcma_bus_register(bus);
+	if (err)
+		goto err_unmap_mmio;
+
+	platform_set_drvdata(pdev, bus);
+
+	return err;
+
+err_unmap_mmio:
+	iounmap(bus->mmio);
+	return err;
+}
+
+static int bcma_host_soc_remove(struct platform_device *pdev)
+{
+	struct bcma_bus *bus = platform_get_drvdata(pdev);
+
+	bcma_bus_unregister(bus);
+	iounmap(bus->mmio);
+	platform_set_drvdata(pdev, NULL);
+
+	return 0;
+}
+
+static const struct of_device_id bcma_host_soc_of_match[] = {
+	{ .compatible = "brcm,bus-axi", },
+	{},
+};
+MODULE_DEVICE_TABLE(of, bcma_host_soc_of_match);
+
+static struct platform_driver bcma_host_soc_driver = {
+	.driver = {
+		.name = "bcma-host-soc",
+		.of_match_table = bcma_host_soc_of_match,
+	},
+	.probe		= bcma_host_soc_probe,
+	.remove		= bcma_host_soc_remove,
+};
+
+int __init bcma_host_soc_register_driver(void)
+{
+	return platform_driver_register(&bcma_host_soc_driver);
+}
+
+void __exit bcma_host_soc_unregister_driver(void)
+{
+	platform_driver_unregister(&bcma_host_soc_driver);
+}
+#endif /* CONFIG_OF */
--- a/drivers/bcma/driver_mips.c
+++ b/drivers/bcma/driver_mips.c
@@ -21,6 +21,14 @@
 #include <linux/serial_reg.h>
 #include <linux/time.h>
 
+enum bcma_boot_dev {
+	BCMA_BOOT_DEV_UNK = 0,
+	BCMA_BOOT_DEV_ROM,
+	BCMA_BOOT_DEV_PARALLEL,
+	BCMA_BOOT_DEV_SERIAL,
+	BCMA_BOOT_DEV_NAND,
+};
+
 static const char * const part_probes[] = { "bcm47xxpart", NULL };
 
 static struct physmap_flash_data bcma_pflash_data = {
@@ -107,7 +115,7 @@ static u32 bcma_core_mips_irqflag(struct
  * If disabled, 5 is returned.
  * If not supported, 6 is returned.
  */
-static unsigned int bcma_core_mips_irq(struct bcma_device *dev)
+unsigned int bcma_core_mips_irq(struct bcma_device *dev)
 {
 	struct bcma_device *mdev = dev->bus->drv_mips.core;
 	u32 irqflag;
@@ -125,13 +133,6 @@ static unsigned int bcma_core_mips_irq(s
 	return 5;
 }
 
-unsigned int bcma_core_irq(struct bcma_device *dev)
-{
-	unsigned int mips_irq = bcma_core_mips_irq(dev);
-	return mips_irq <= 4 ? mips_irq + 2 : 0;
-}
-EXPORT_SYMBOL(bcma_core_irq);
-
 static void bcma_core_mips_set_irq(struct bcma_device *dev, unsigned int irq)
 {
 	unsigned int oldirq = bcma_core_mips_irq(dev);
@@ -229,11 +230,51 @@ u32 bcma_cpu_clock(struct bcma_drv_mips 
 }
 EXPORT_SYMBOL(bcma_cpu_clock);
 
+static enum bcma_boot_dev bcma_boot_dev(struct bcma_bus *bus)
+{
+	struct bcma_drv_cc *cc = &bus->drv_cc;
+	u8 cc_rev = cc->core->id.rev;
+
+	if (cc_rev == 42) {
+		struct bcma_device *core;
+
+		core = bcma_find_core(bus, BCMA_CORE_NS_ROM);
+		if (core) {
+			switch (bcma_aread32(core, BCMA_IOST) &
+				BCMA_NS_ROM_IOST_BOOT_DEV_MASK) {
+			case BCMA_NS_ROM_IOST_BOOT_DEV_NOR:
+				return BCMA_BOOT_DEV_SERIAL;
+			case BCMA_NS_ROM_IOST_BOOT_DEV_NAND:
+				return BCMA_BOOT_DEV_NAND;
+			case BCMA_NS_ROM_IOST_BOOT_DEV_ROM:
+			default:
+				return BCMA_BOOT_DEV_ROM;
+			}
+		}
+	} else {
+		if (cc_rev == 38) {
+			if (cc->status & BCMA_CC_CHIPST_5357_NAND_BOOT)
+				return BCMA_BOOT_DEV_NAND;
+			else if (cc->status & BIT(5))
+				return BCMA_BOOT_DEV_ROM;
+		}
+
+		if ((cc->capabilities & BCMA_CC_CAP_FLASHT) ==
+		    BCMA_CC_FLASHT_PARA)
+			return BCMA_BOOT_DEV_PARALLEL;
+		else
+			return BCMA_BOOT_DEV_SERIAL;
+	}
+
+	return BCMA_BOOT_DEV_SERIAL;
+}
+
 static void bcma_core_mips_flash_detect(struct bcma_drv_mips *mcore)
 {
 	struct bcma_bus *bus = mcore->core->bus;
 	struct bcma_drv_cc *cc = &bus->drv_cc;
 	struct bcma_pflash *pflash = &cc->pflash;
+	enum bcma_boot_dev boot_dev;
 
 	switch (cc->capabilities & BCMA_CC_CAP_FLASHT) {
 	case BCMA_CC_FLASHT_STSER:
@@ -269,6 +310,20 @@ static void bcma_core_mips_flash_detect(
 			bcma_nflash_init(cc);
 		}
 	}
+
+	/* Determine flash type this SoC boots from */
+	boot_dev = bcma_boot_dev(bus);
+	switch (boot_dev) {
+	case BCMA_BOOT_DEV_PARALLEL:
+	case BCMA_BOOT_DEV_SERIAL:
+		/* TODO: Init NVRAM using BCMA_SOC_FLASH2 window */
+		break;
+	case BCMA_BOOT_DEV_NAND:
+		/* TODO: Init NVRAM using BCMA_SOC_FLASH1 window */
+		break;
+	default:
+		break;
+	}
 }
 
 void bcma_core_mips_early_init(struct bcma_drv_mips *mcore)
@@ -361,7 +416,7 @@ void bcma_core_mips_init(struct bcma_drv
 		break;
 	default:
 		list_for_each_entry(core, &bus->cores, list) {
-			core->irq = bcma_core_irq(core);
+			core->irq = bcma_core_irq(core, 0);
 		}
 		bcma_err(bus,
 			 "Unknown device (0x%x) found, can not configure IRQs\n",
--- a/include/linux/bcma/bcma_regs.h
+++ b/include/linux/bcma/bcma_regs.h
@@ -39,6 +39,11 @@
 #define  BCMA_RESET_CTL_RESET		0x0001
 #define BCMA_RESET_ST			0x0804
 
+#define BCMA_NS_ROM_IOST_BOOT_DEV_MASK	0x0003
+#define BCMA_NS_ROM_IOST_BOOT_DEV_NOR	0x0000
+#define BCMA_NS_ROM_IOST_BOOT_DEV_NAND	0x0001
+#define BCMA_NS_ROM_IOST_BOOT_DEV_ROM	0x0002
+
 /* BCMA PCI config space registers. */
 #define BCMA_PCI_PMCSR			0x44
 #define  BCMA_PCI_PE			0x100
--- a/drivers/usb/host/bcma-hcd.c
+++ b/drivers/usb/host/bcma-hcd.c
@@ -237,7 +237,7 @@ static int bcma_hcd_probe(struct bcma_de
 	bcma_hcd_init_chip(dev);
 
 	/* In AI chips EHCI is addrspace 0, OHCI is 1 */
-	ohci_addr = dev->addr1;
+	ohci_addr = dev->addr_s[0];
 	if ((chipinfo->id == 0x5357 || chipinfo->id == 0x4749)
 	    && chipinfo->rev == 0)
 		ohci_addr = 0x18009000;
--- a/drivers/bcma/bcma_private.h
+++ b/drivers/bcma/bcma_private.h
@@ -24,6 +24,7 @@ struct bcma_bus;
 /* main.c */
 bool bcma_wait_value(struct bcma_device *core, u16 reg, u32 mask, u32 value,
 		     int timeout);
+void bcma_prepare_core(struct bcma_bus *bus, struct bcma_device *core);
 int bcma_bus_register(struct bcma_bus *bus);
 void bcma_bus_unregister(struct bcma_bus *bus);
 int __init bcma_bus_early_register(struct bcma_bus *bus,
@@ -50,6 +51,10 @@ void bcma_chipco_serial_init(struct bcma
 extern struct platform_device bcma_pflash_dev;
 #endif /* CONFIG_BCMA_DRIVER_MIPS */
 
+/* driver_chipcommon_b.c */
+int bcma_core_chipcommon_b_init(struct bcma_drv_cc_b *ccb);
+void bcma_core_chipcommon_b_free(struct bcma_drv_cc_b *ccb);
+
 /* driver_chipcommon_pmu.c */
 u32 bcma_pmu_get_alp_clock(struct bcma_drv_cc *cc);
 u32 bcma_pmu_get_cpu_clock(struct bcma_drv_cc *cc);
@@ -84,6 +89,20 @@ extern int __init bcma_host_pci_init(voi
 extern void __exit bcma_host_pci_exit(void);
 #endif /* CONFIG_BCMA_HOST_PCI */
 
+/* host_soc.c */
+#if defined(CONFIG_BCMA_HOST_SOC) && defined(CONFIG_OF)
+extern int __init bcma_host_soc_register_driver(void);
+extern void __exit bcma_host_soc_unregister_driver(void);
+#else
+static inline int __init bcma_host_soc_register_driver(void)
+{
+	return 0;
+}
+static inline void __exit bcma_host_soc_unregister_driver(void)
+{
+}
+#endif /* CONFIG_BCMA_HOST_SOC && CONFIG_OF */
+
 /* driver_pci.c */
 u32 bcma_pcie_read(struct bcma_drv_pci *pc, u32 address);
 
--- /dev/null
+++ b/drivers/bcma/driver_chipcommon_b.c
@@ -0,0 +1,61 @@
+/*
+ * Broadcom specific AMBA
+ * ChipCommon B Unit driver
+ *
+ * Copyright 2014, Hauke Mehrtens <hauke@hauke-m.de>
+ *
+ * Licensed under the GNU/GPL. See COPYING for details.
+ */
+
+#include "bcma_private.h"
+#include <linux/export.h>
+#include <linux/bcma/bcma.h>
+
+static bool bcma_wait_reg(struct bcma_bus *bus, void __iomem *addr, u32 mask,
+			  u32 value, int timeout)
+{
+	unsigned long deadline = jiffies + timeout;
+	u32 val;
+
+	do {
+		val = readl(addr);
+		if ((val & mask) == value)
+			return true;
+		cpu_relax();
+		udelay(10);
+	} while (!time_after_eq(jiffies, deadline));
+
+	bcma_err(bus, "Timeout waiting for register %p\n", addr);
+
+	return false;
+}
+
+void bcma_chipco_b_mii_write(struct bcma_drv_cc_b *ccb, u32 offset, u32 value)
+{
+	struct bcma_bus *bus = ccb->core->bus;
+
+	writel(offset, ccb->mii + 0x00);
+	bcma_wait_reg(bus, ccb->mii + 0x00, 0x0100, 0x0000, 100);
+	writel(value, ccb->mii + 0x04);
+	bcma_wait_reg(bus, ccb->mii + 0x00, 0x0100, 0x0000, 100);
+}
+EXPORT_SYMBOL_GPL(bcma_chipco_b_mii_write);
+
+int bcma_core_chipcommon_b_init(struct bcma_drv_cc_b *ccb)
+{
+	if (ccb->setup_done)
+		return 0;
+
+	ccb->setup_done = 1;
+	ccb->mii = ioremap_nocache(ccb->core->addr_s[1], BCMA_CORE_SIZE);
+	if (!ccb->mii)
+		return -ENOMEM;
+
+	return 0;
+}
+
+void bcma_core_chipcommon_b_free(struct bcma_drv_cc_b *ccb)
+{
+	if (ccb->mii)
+		iounmap(ccb->mii);
+}
--- a/include/linux/bcma/bcma_driver_chipcommon.h
+++ b/include/linux/bcma/bcma_driver_chipcommon.h
@@ -644,6 +644,12 @@ struct bcma_drv_cc {
 #endif
 };
 
+struct bcma_drv_cc_b {
+	struct bcma_device *core;
+	u8 setup_done:1;
+	void __iomem *mii;
+};
+
 /* Register access */
 #define bcma_cc_read32(cc, offset) \
 	bcma_read32((cc)->core, offset)
@@ -699,4 +705,6 @@ extern void bcma_pmu_spuravoid_pllupdate
 
 extern u32 bcma_pmu_get_bus_clock(struct bcma_drv_cc *cc);
 
+void bcma_chipco_b_mii_write(struct bcma_drv_cc_b *ccb, u32 offset, u32 value);
+
 #endif /* LINUX_BCMA_DRIVER_CC_H_ */
--- a/arch/mips/bcm47xx/setup.c
+++ b/arch/mips/bcm47xx/setup.c
@@ -202,6 +202,10 @@ static void __init bcm47xx_register_bcma
 
 	err = bcma_host_soc_register(&bcm47xx_bus.bcma);
 	if (err)
+		panic("Failed to register BCMA bus (err %d)", err);
+
+	err = bcma_host_soc_init(&bcm47xx_bus.bcma);
+	if (err)
 		panic("Failed to initialize BCMA bus (err %d)", err);
 
 	bcm47xx_fill_bcma_boardinfo(&bcm47xx_bus.bcma.bus.boardinfo, NULL);
--- a/include/linux/bcma/bcma_soc.h
+++ b/include/linux/bcma/bcma_soc.h
@@ -10,6 +10,7 @@ struct bcma_soc {
 };
 
 int __init bcma_host_soc_register(struct bcma_soc *soc);
+int __init bcma_host_soc_init(struct bcma_soc *soc);
 
 int bcma_bus_register(struct bcma_bus *bus);
 
--- /dev/null
+++ b/Documentation/devicetree/bindings/bus/bcma.txt
@@ -0,0 +1,53 @@
+Driver for ARM AXI Bus with Broadcom Plugins (bcma)
+
+Required properties:
+
+- compatible : brcm,bus-axi
+
+- reg : iomem address range of chipcommon core
+
+The cores on the AXI bus are automatically detected by bcma with the
+memory ranges they are using and they get registered afterwards.
+Automatic detection of the IRQ number is not working on
+BCM47xx/BCM53xx ARM SoCs. To assign IRQ numbers to the cores, provide
+them manually through device tree. Use an interrupt-map to specify the
+IRQ used by the devices on the bus. The first address is just an index,
+because we do not have any special register.
+
+The top-level axi bus may contain children representing attached cores
+(devices). This is needed since some hardware details can't be auto
+detected (e.g. IRQ numbers). Also some of the cores may be responsible
+for extra things, e.g. ChipCommon providing access to the GPIO chip.
+
+Example:
+
+	axi@18000000 {
+		compatible = "brcm,bus-axi";
+		reg = <0x18000000 0x1000>;
+		ranges = <0x00000000 0x18000000 0x00100000>;
+		#address-cells = <1>;
+		#size-cells = <1>;
+		#interrupt-cells = <1>;
+		interrupt-map-mask = <0x000fffff 0xffff>;
+		interrupt-map =
+			/* Ethernet Controller 0 */
+			<0x00024000 0 &gic GIC_SPI 147 IRQ_TYPE_LEVEL_HIGH>,
+
+			/* Ethernet Controller 1 */
+			<0x00025000 0 &gic GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>;
+
+			/* PCIe Controller 0 */
+			<0x00012000 0 &gic GIC_SPI 126 IRQ_TYPE_LEVEL_HIGH>,
+			<0x00012000 1 &gic GIC_SPI 127 IRQ_TYPE_LEVEL_HIGH>,
+			<0x00012000 2 &gic GIC_SPI 128 IRQ_TYPE_LEVEL_HIGH>,
+			<0x00012000 3 &gic GIC_SPI 129 IRQ_TYPE_LEVEL_HIGH>,
+			<0x00012000 4 &gic GIC_SPI 130 IRQ_TYPE_LEVEL_HIGH>,
+			<0x00012000 5 &gic GIC_SPI 131 IRQ_TYPE_LEVEL_HIGH>;
+
+		chipcommon {
+			reg = <0x00000000 0x1000>;
+
+			gpio-controller;
+			#gpio-cells = <2>;
+		};
+	};
