From b5325f9813a6a7cf80ede22fbee66376abbe2384 Mon Sep 17 00:00:00 2001
From: Roman Byshko <rbyshko@gmail.com>
Date: Fri, 7 Feb 2014 16:21:51 +0100
Subject: [PATCH] ARM: sun4i: dt: Add bindings for USB clocks

Signed-off-by: Roman Byshko <rbyshko@gmail.com>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 arch/arm/boot/dts/sun4i-a10.dtsi | 9 +++++++++
 1 file changed, 9 insertions(+)

--- a/arch/arm/boot/dts/sun4i-a10.dtsi
+++ b/arch/arm/boot/dts/sun4i-a10.dtsi
@@ -315,6 +315,15 @@
 			clock-output-names = "ir1";
 		};
 
+		usb_clk: clk@01c200cc {
+			#clock-cells = <1>;
+		        #reset-cells = <1>;
+			compatible = "allwinner,sun4i-a10-usb-clk";
+			reg = <0x01c200cc 0x4>;
+			clocks = <&pll6 1>;
+			clock-output-names = "usb_ohci0", "usb_ohci1", "usb_phy";
+		};
+
 		spi3_clk: clk@01c200d4 {
 			#clock-cells = <0>;
 			compatible = "allwinner,sun4i-mod0-clk";
