From bfea2b9be28b20e076d5df8863c25e966f413fa3 Mon Sep 17 00:00:00 2001
From: Maxime Ripard <maxime.ripard@free-electrons.com>
Date: Fri, 20 Dec 2013 22:41:07 +0100
Subject: [PATCH] reset: Add of_reset_control_get

In some cases, you might need to deassert from reset an hardware block that
doesn't associated to a struct device (CPUs, timers, etc.).

Add a small helper to retrieve the reset controller from the device tree
without the need to pass a struct device.

Signed-off-by: Maxime Ripard <maxime.ripard@free-electrons.com>
---
 drivers/reset/core.c  | 39 ++++++++++++++++++++++++++++++---------
 include/linux/reset.h |  4 ++++
 2 files changed, 34 insertions(+), 9 deletions(-)

--- a/drivers/reset/core.c
+++ b/drivers/reset/core.c
@@ -127,15 +127,16 @@ int reset_control_deassert(struct reset_
 EXPORT_SYMBOL_GPL(reset_control_deassert);
 
 /**
- * reset_control_get - Lookup and obtain a reference to a reset controller.
- * @dev: device to be reset by the controller
+ * of_reset_control_get - Lookup and obtain a reference to a reset controller.
+ * @node: device to be reset by the controller
  * @id: reset line name
  *
  * Returns a struct reset_control or IS_ERR() condition containing errno.
  *
  * Use of id names is optional.
  */
-struct reset_control *reset_control_get(struct device *dev, const char *id)
+struct reset_control *of_reset_control_get(struct device_node *node,
+					   const char *id)
 {
 	struct reset_control *rstc = ERR_PTR(-EPROBE_DEFER);
 	struct reset_controller_dev *r, *rcdev;
@@ -144,13 +145,10 @@ struct reset_control *reset_control_get(
 	int rstc_id;
 	int ret;
 
-	if (!dev)
-		return ERR_PTR(-EINVAL);
-
 	if (id)
-		index = of_property_match_string(dev->of_node,
+		index = of_property_match_string(node,
 						 "reset-names", id);
-	ret = of_parse_phandle_with_args(dev->of_node, "resets", "#reset-cells",
+	ret = of_parse_phandle_with_args(node, "resets", "#reset-cells",
 					 index, &args);
 	if (ret)
 		return ERR_PTR(ret);
@@ -185,12 +183,35 @@ struct reset_control *reset_control_get(
 		return ERR_PTR(-ENOMEM);
 	}
 
-	rstc->dev = dev;
 	rstc->rcdev = rcdev;
 	rstc->id = rstc_id;
 
 	return rstc;
 }
+EXPORT_SYMBOL_GPL(of_reset_control_get);
+
+/**
+ * reset_control_get - Lookup and obtain a reference to a reset controller.
+ * @dev: device to be reset by the controller
+ * @id: reset line name
+ *
+ * Returns a struct reset_control or IS_ERR() condition containing errno.
+ *
+ * Use of id names is optional.
+ */
+struct reset_control *reset_control_get(struct device *dev, const char *id)
+{
+	struct reset_control *rstc;
+
+	if (!dev)
+		return ERR_PTR(-EINVAL);
+
+	rstc = of_reset_control_get(dev->of_node, id);
+	if (!IS_ERR(rstc))
+		rstc->dev = dev;
+
+	return rstc;
+}
 EXPORT_SYMBOL_GPL(reset_control_get);
 
 /**
--- a/include/linux/reset.h
+++ b/include/linux/reset.h
@@ -1,6 +1,8 @@
 #ifndef _LINUX_RESET_H_
 #define _LINUX_RESET_H_
 
+#include <linux/of.h>
+
 struct device;
 struct reset_control;
 
@@ -8,6 +10,8 @@ int reset_control_reset(struct reset_con
 int reset_control_assert(struct reset_control *rstc);
 int reset_control_deassert(struct reset_control *rstc);
 
+struct reset_control *of_reset_control_get(struct device_node *node,
+					   const char *id);
 struct reset_control *reset_control_get(struct device *dev, const char *id);
 void reset_control_put(struct reset_control *rstc);
 struct reset_control *devm_reset_control_get(struct device *dev, const char *id);
