From d09483e1cfcc00be70450c469c3c23496a063d98 Mon Sep 17 00:00:00 2001
From: Chen-Yu Tsai <wens@csie.org>
Date: Mon, 10 Feb 2014 18:35:51 +0800
Subject: [PATCH] ARM: dts: sun7i: cubietruck: Enable the GMAC

The CubieTruck uses the GMAC with an RGMII phy.

Signed-off-by: Chen-Yu Tsai <wens@csie.org>
---
 arch/arm/boot/dts/sun7i-a20-cubietruck.dts | 12 ++++++++++++
 1 file changed, 12 insertions(+)

--- a/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
@@ -65,6 +65,18 @@
 			pinctrl-0 = <&i2c2_pins_a>;
 			status = "okay";
 		};
+
+		gmac: ethernet@01c50000 {
+			pinctrl-names = "default";
+			pinctrl-0 = <&gmac_pins_rgmii_a>;
+			phy = <&phy1>;
+			phy-mode = "rgmii";
+			status = "okay";
+
+			phy1: ethernet-phy@1 {
+				reg = <1>;
+			};
+		};
 	};
 
 	leds {
