From df25859babd9c164a61e86d953d5c88400009a14 Mon Sep 17 00:00:00 2001
From: Hante Meuleman <meuleman@broadcom.com>
Date: Wed, 29 Jan 2014 15:32:16 +0100
Subject: [PATCH] brcmfmac: fix sdio sending of large buffers.

the function brcmf_sdiod_ramrw is supposed to be able to send
large blobs of data. However inside the loop the skb->len field
did not correctly get reset each round. As a result only small
blobs could be sent. This patch fixes this problem.

Reviewed-by: Arend Van Spriel <arend@broadcom.com>
Reviewed-by: Franky (Zhenhui) Lin <frankyl@broadcom.com>
Reviewed-by: Pieter-Paul Giesberts <pieterpg@broadcom.com>
Reviewed-by: Daniel (Deognyoun) Kim <dekim@broadcom.com>
Signed-off-by: Hante Meuleman <meuleman@broadcom.com>
Signed-off-by: Arend van Spriel <arend@broadcom.com>
Signed-off-by: John W. Linville <linville@tuxdriver.com>
---
 drivers/net/wireless/brcm80211/brcmfmac/bcmsdh.c | 2 +-
 1 file changed, 1 insertion(+), 1 deletion(-)

--- a/drivers/net/wireless/brcm80211/brcmfmac/bcmsdh.c
+++ b/drivers/net/wireless/brcm80211/brcmfmac/bcmsdh.c
@@ -827,7 +827,7 @@ brcmf_sdiod_ramrw(struct brcmf_sdio_dev 
 		}
 		if (!write)
 			memcpy(data, pkt->data, dsize);
-		skb_trim(pkt, dsize);
+		skb_trim(pkt, 0);
 
 		/* Adjust for next transfer (if any) */
 		size -= dsize;
