--- a/arch/mips/include/asm/mach-bcm63xx/bcm963xx_tag.h
+++ /dev/null
@@ -1,96 +0,0 @@
-#ifndef __BCM963XX_TAG_H
-#define __BCM963XX_TAG_H
-
-#define TAGVER_LEN		4	/* Length of Tag Version */
-#define TAGLAYOUT_LEN		4	/* Length of FlashLayoutVer */
-#define SIG1_LEN		20	/* Company Signature 1 Length */
-#define SIG2_LEN		14	/* Company Signature 2 Length */
-#define BOARDID_LEN		16	/* Length of BoardId */
-#define ENDIANFLAG_LEN		2	/* Endian Flag Length */
-#define CHIPID_LEN		6	/* Chip Id Length */
-#define IMAGE_LEN		10	/* Length of Length Field */
-#define ADDRESS_LEN		12	/* Length of Address field */
-#define DUALFLAG_LEN		2	/* Dual Image flag Length */
-#define INACTIVEFLAG_LEN	2	/* Inactie Flag Length */
-#define RSASIG_LEN		20	/* Length of RSA Signature in tag */
-#define TAGINFO1_LEN		30	/* Length of vendor information field1 in tag */
-#define FLASHLAYOUTVER_LEN	4	/* Length of Flash Layout Version String tag */
-#define TAGINFO2_LEN		16	/* Length of vendor information field2 in tag */
-#define ALTTAGINFO_LEN		54	/* Alternate length for vendor information; Pirelli */
-
-#define NUM_PIRELLI		2
-#define IMAGETAG_CRC_START	0xFFFFFFFF
-
-#define PIRELLI_BOARDS { \
-	"AGPF-S0", \
-	"DWV-S0", \
-}
-
-/*
- * The broadcom firmware assumes the rootfs starts the image,
- * therefore uses the rootfs start (flash_image_address)
- * to determine where to flash the image.  Since we have the kernel first
- * we have to give it the kernel address, but the crc uses the length
- * associated with this address (root_length), which is added to the kernel
- * length (kernel_length) to determine the length of image to flash and thus
- * needs to be rootfs + deadcode (jffs2 EOF marker)
-*/
-
-struct bcm_tag {
-	/* 0-3: Version of the image tag */
-	char tag_version[TAGVER_LEN];
-	/* 4-23: Company Line 1 */
-	char sig_1[SIG1_LEN];
-	/*  24-37: Company Line 2 */
-	char sig_2[SIG2_LEN];
-	/* 38-43: Chip this image is for */
-	char chip_id[CHIPID_LEN];
-	/* 44-59: Board name */
-	char board_id[BOARDID_LEN];
-	/* 60-61: Map endianness -- 1 BE 0 LE */
-	char big_endian[ENDIANFLAG_LEN];
-	/* 62-71: Total length of image */
-	char total_length[IMAGE_LEN];
-	/* 72-83: Address in memory of CFE */
-	char cfe__address[ADDRESS_LEN];
-	/* 84-93: Size of CFE */
-	char cfe_length[IMAGE_LEN];
-	/* 94-105: Address in memory of image start
-	 * (kernel for libreCMC, rootfs for stock firmware)
-	 */
-	char flash_image_start[ADDRESS_LEN];
-	/* 106-115: Size of rootfs */
-	char root_length[IMAGE_LEN];
-	/* 116-127: Address in memory of kernel */
-	char kernel_address[ADDRESS_LEN];
-	/* 128-137: Size of kernel */
-	char kernel_length[IMAGE_LEN];
-	/* 138-139: Unused at the moment */
-	char dual_image[DUALFLAG_LEN];
-	/* 140-141: Unused at the moment */
-	char inactive_flag[INACTIVEFLAG_LEN];
-	/* 142-161: RSA Signature (not used; some vendors may use this) */
-	char rsa_signature[RSASIG_LEN];
-	/* 162-191: Compilation and related information (not used in libreCMC) */
-	char information1[TAGINFO1_LEN];
-	/* 192-195: Version flash layout */
-	char flash_layout_ver[FLASHLAYOUTVER_LEN];
-	/* 196-199: kernel+rootfs CRC32 */
-	__u32 fskernel_crc;
-	/* 200-215: Unused except on Alice Gate where is is information */
-	char information2[TAGINFO2_LEN];
-	/* 216-219: CRC32 of image less imagetag (kernel for Alice Gate) */
-	__u32 image_crc;
-	/* 220-223: CRC32 of rootfs partition */
-	__u32 rootfs_crc;
-	/* 224-227: CRC32 of kernel partition */
-	__u32 kernel_crc;
-	/* 228-235: Unused at present */
-	char reserved1[8];
-	/* 236-239: CRC32 of header excluding last 20 bytes */
-	__u32 header_crc;
-	/* 240-255: Unused at present */
-	char reserved2[16];
-};
-
-#endif /* __BCM63XX_TAG_H */
--- a/drivers/mtd/bcm63xxpart.c
+++ b/drivers/mtd/bcm63xxpart.c
@@ -34,7 +34,7 @@
 #include <linux/mtd/partitions.h>
 
 #include <asm/mach-bcm63xx/bcm63xx_nvram.h>
-#include <asm/mach-bcm63xx/bcm963xx_tag.h>
+#include <linux/bcm963xx_tag.h>
 #include <asm/mach-bcm63xx/board_bcm963xx.h>
 
 #define BCM63XX_EXTENDED_SIZE	0xBFC00000	/* Extended flash address */
--- a/include/uapi/linux/Kbuild
+++ b/include/uapi/linux/Kbuild
@@ -70,6 +70,7 @@ header-y += blktrace_api.h
 header-y += bpf.h
 header-y += bpf_common.h
 header-y += bpqether.h
+header-y += bcm963xx_tag.h
 header-y += bsg.h
 header-y += btrfs.h
 header-y += can.h
--- /dev/null
+++ b/include/uapi/linux/bcm963xx_tag.h
@@ -0,0 +1,96 @@
+#ifndef __BCM963XX_TAG_H
+#define __BCM963XX_TAG_H
+
+#define TAGVER_LEN		4	/* Length of Tag Version */
+#define TAGLAYOUT_LEN		4	/* Length of FlashLayoutVer */
+#define SIG1_LEN		20	/* Company Signature 1 Length */
+#define SIG2_LEN		14	/* Company Signature 2 Length */
+#define BOARDID_LEN		16	/* Length of BoardId */
+#define ENDIANFLAG_LEN		2	/* Endian Flag Length */
+#define CHIPID_LEN		6	/* Chip Id Length */
+#define IMAGE_LEN		10	/* Length of Length Field */
+#define ADDRESS_LEN		12	/* Length of Address field */
+#define DUALFLAG_LEN		2	/* Dual Image flag Length */
+#define INACTIVEFLAG_LEN	2	/* Inactie Flag Length */
+#define RSASIG_LEN		20	/* Length of RSA Signature in tag */
+#define TAGINFO1_LEN		30	/* Length of vendor information field1 in tag */
+#define FLASHLAYOUTVER_LEN	4	/* Length of Flash Layout Version String tag */
+#define TAGINFO2_LEN		16	/* Length of vendor information field2 in tag */
+#define ALTTAGINFO_LEN		54	/* Alternate length for vendor information; Pirelli */
+
+#define NUM_PIRELLI		2
+#define IMAGETAG_CRC_START	0xFFFFFFFF
+
+#define PIRELLI_BOARDS { \
+	"AGPF-S0", \
+	"DWV-S0", \
+}
+
+/*
+ * The broadcom firmware assumes the rootfs starts the image,
+ * therefore uses the rootfs start (flash_image_address)
+ * to determine where to flash the image.  Since we have the kernel first
+ * we have to give it the kernel address, but the crc uses the length
+ * associated with this address (root_length), which is added to the kernel
+ * length (kernel_length) to determine the length of image to flash and thus
+ * needs to be rootfs + deadcode (jffs2 EOF marker)
+*/
+
+struct bcm_tag {
+	/* 0-3: Version of the image tag */
+	char tag_version[TAGVER_LEN];
+	/* 4-23: Company Line 1 */
+	char sig_1[SIG1_LEN];
+	/*  24-37: Company Line 2 */
+	char sig_2[SIG2_LEN];
+	/* 38-43: Chip this image is for */
+	char chip_id[CHIPID_LEN];
+	/* 44-59: Board name */
+	char board_id[BOARDID_LEN];
+	/* 60-61: Map endianness -- 1 BE 0 LE */
+	char big_endian[ENDIANFLAG_LEN];
+	/* 62-71: Total length of image */
+	char total_length[IMAGE_LEN];
+	/* 72-83: Address in memory of CFE */
+	char cfe__address[ADDRESS_LEN];
+	/* 84-93: Size of CFE */
+	char cfe_length[IMAGE_LEN];
+	/* 94-105: Address in memory of image start
+	 * (kernel for libreCMC, rootfs for stock firmware)
+	 */
+	char flash_image_start[ADDRESS_LEN];
+	/* 106-115: Size of rootfs */
+	char root_length[IMAGE_LEN];
+	/* 116-127: Address in memory of kernel */
+	char kernel_address[ADDRESS_LEN];
+	/* 128-137: Size of kernel */
+	char kernel_length[IMAGE_LEN];
+	/* 138-139: Unused at the moment */
+	char dual_image[DUALFLAG_LEN];
+	/* 140-141: Unused at the moment */
+	char inactive_flag[INACTIVEFLAG_LEN];
+	/* 142-161: RSA Signature (not used; some vendors may use this) */
+	char rsa_signature[RSASIG_LEN];
+	/* 162-191: Compilation and related information (not used in libreCMC) */
+	char information1[TAGINFO1_LEN];
+	/* 192-195: Version flash layout */
+	char flash_layout_ver[FLASHLAYOUTVER_LEN];
+	/* 196-199: kernel+rootfs CRC32 */
+	__u32 fskernel_crc;
+	/* 200-215: Unused except on Alice Gate where is is information */
+	char information2[TAGINFO2_LEN];
+	/* 216-219: CRC32 of image less imagetag (kernel for Alice Gate) */
+	__u32 image_crc;
+	/* 220-223: CRC32 of rootfs partition */
+	__u32 rootfs_crc;
+	/* 224-227: CRC32 of kernel partition */
+	__u32 kernel_crc;
+	/* 228-235: Unused at present */
+	char reserved1[8];
+	/* 236-239: CRC32 of header excluding last 20 bytes */
+	__u32 header_crc;
+	/* 240-255: Unused at present */
+	char reserved2[16];
+};
+
+#endif /* __BCM63XX_TAG_H */
