From 56de1b69bf6782338193e373cee06fff252b31da Mon Sep 17 00:00:00 2001
From: Hans de Goede <hdegoede@redhat.com>
Date: Tue, 17 Dec 2013 23:04:57 +0100
Subject: [PATCH] ARM: sun7i: dt: Add USB host nodes to cubietruck dts

Add nodes for the usb-phy and ehci- and ohci-usb-host controllers.

Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun7i-a20-cubietruck.dts | 30 ++++++++++++++++++++++++++++++
 1 file changed, 30 insertions(+)

--- a/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubietruck.dts
@@ -20,11 +20,33 @@
 	compatible = "cubietech,cubietruck", "allwinner,sun7i-a20";
 
 	soc@01c00000 {
+		usbphy: phy@01c13400 {
+			usb1_vbus-supply = <&reg_usb1_vbus>;
+			usb2_vbus-supply = <&reg_usb2_vbus>;
+			status = "okay";
+		};
+
+		ehci0: usb@01c14000 {
+			status = "okay";
+		};
+
+		ohci0: usb@01c14400 {
+			status = "okay";
+		};
+
 		ahci: sata@01c18000 {
 			target-supply = <&reg_ahci_5v>;
 			status = "okay";
 		};
 
+		ehci1: usb@01c1c000 {
+			status = "okay";
+		};
+
+		ohci1: usb@01c1c400 {
+			status = "okay";
+		};
+
 		pinctrl@01c20800 {
 			ahci_pwr_pin_cubietruck: ahci_pwr_pin@1 {
 				allwinner,pins = "PH12";
@@ -123,4 +145,12 @@
 		gpio = <&pio 7 12 0>;
 		status = "okay";
 	};
+
+	reg_usb1_vbus: usb1-vbus {
+		status = "okay";
+	};
+
+	reg_usb2_vbus: usb2-vbus {
+		status = "okay";
+	};
 };
--- a/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
+++ b/arch/arm/boot/dts/sun7i-a20-cubieboard2.dts
@@ -20,11 +20,33 @@
 	compatible = "cubietech,cubieboard2", "allwinner,sun7i-a20";
 
 	soc@01c00000 {
+		usbphy: phy@01c13400 {
+			usb1_vbus-supply = <&reg_usb1_vbus>;
+			usb2_vbus-supply = <&reg_usb2_vbus>;
+			status = "okay";
+		};
+
+		ehci0: usb@01c14000 {
+			status = "okay";
+		};
+
+		ohci0: usb@01c14400 {
+			status = "okay";
+		};
+
 		ahci: sata@01c18000 {
 			target-supply = <&reg_ahci_5v>;
 			status = "okay";
 		};
 
+		ehci1: usb@01c1c000 {
+			status = "okay";
+		};
+
+		ohci1: usb@01c1c400 {
+			status = "okay";
+		};
+
 		pinctrl@01c20800 {
 			led_pins_cubieboard2: led_pins@0 {
 				allwinner,pins = "PH20", "PH21";
@@ -84,4 +106,12 @@
 	reg_ahci_5v: ahci-5v {
 		status = "okay";
 	};
+
+	reg_usb1_vbus: usb1-vbus {
+		status = "okay";
+	};
+
+	reg_usb2_vbus: usb2-vbus {
+		status = "okay";
+	};
 };
--- a/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts
+++ b/arch/arm/boot/dts/sun7i-a20-olinuxino-micro.dts
@@ -31,6 +31,20 @@
 			status = "okay";
 		};
 
+		usbphy: phy@01c13400 {
+			usb1_vbus-supply = <&reg_usb1_vbus>;
+			usb2_vbus-supply = <&reg_usb2_vbus>;
+			status = "okay";
+		};
+
+		ehci0: usb@01c14000 {
+			status = "okay";
+		};
+
+		ohci0: usb@01c14400 {
+			status = "okay";
+		};
+
 		spi2: spi@01c17000 {
 			pinctrl-names = "default";
 			pinctrl-0 = <&spi2_pins_a>;
@@ -42,6 +56,14 @@
 			status = "okay";
 		};
 
+		ehci1: usb@01c1c000 {
+			status = "okay";
+		};
+
+		ohci1: usb@01c1c400 {
+			status = "okay";
+		};
+
 		pinctrl@01c20800 {
 			led_pins_olinuxino: led_pins@0 {
 				allwinner,pins = "PH2";
@@ -115,4 +137,12 @@
 	reg_ahci_5v: ahci-5v {
 		status = "okay";
 	};
+
+	reg_usb1_vbus: usb1-vbus {
+		status = "okay";
+	};
+
+	reg_usb2_vbus: usb2-vbus {
+		status = "okay";
+	};
 };
