From b66989fe7a41e1093b1f825967ab29963e06cccd Mon Sep 17 00:00:00 2001
From: =?UTF-8?q?David=20Lanzend=C3=B6rfer?= <david.lanzendoerfer@o2s.ch>
Date: Sat, 15 Feb 2014 14:02:51 +0100
Subject: [PATCH] ARM: dts: sun4i: Add support for mmc
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Signed-off-by: David Lanzendörfer <david.lanzendoerfer@o2s.ch>
Signed-off-by: Hans de Goede <hdegoede@redhat.com>
---
 arch/arm/boot/dts/sun4i-a10-a1000.dts      |  8 +++++
 arch/arm/boot/dts/sun4i-a10-cubieboard.dts |  8 +++++
 arch/arm/boot/dts/sun4i-a10.dtsi           | 58 ++++++++++++++++++++++++++++++
 3 files changed, 74 insertions(+)

--- a/arch/arm/boot/dts/sun4i-a10-cubieboard.dts
+++ b/arch/arm/boot/dts/sun4i-a10-cubieboard.dts
@@ -34,6 +34,14 @@
 			};
 		};
 
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_reference_design>;
+			cd-gpios = <&pio 7 1 0>; /* PH1 */
+			status = "okay";
+		};
+
 		usbphy: phy@01c13400 {
 			usb1_vbus-supply = <&reg_usb1_vbus>;
 			usb2_vbus-supply = <&reg_usb2_vbus>;
--- a/arch/arm/boot/dts/sun4i-a10.dtsi
+++ b/arch/arm/boot/dts/sun4i-a10.dtsi
@@ -377,6 +377,50 @@
 			#size-cells = <0>;
 		};
 
+		mmc0: mmc@01c0f000 {
+			compatible = "allwinner,sun4i-a10-mmc";
+			reg = <0x01c0f000 0x1000>;
+			clocks = <&ahb_gates 8>, <&mmc0_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <32>;
+			bus-width = <4>;
+			cd-inverted;
+			status = "disabled";
+		};
+
+		mmc1: mmc@01c10000 {
+			compatible = "allwinner,sun4i-a10-mmc";
+			reg = <0x01c10000 0x1000>;
+			clocks = <&ahb_gates 9>, <&mmc1_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <33>;
+			bus-width = <4>;
+			cd-inverted;
+			status = "disabled";
+		};
+
+		mmc2: mmc@01c11000 {
+			compatible = "allwinner,sun4i-a10-mmc";
+			reg = <0x01c11000 0x1000>;
+			clocks = <&ahb_gates 10>, <&mmc2_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <34>;
+			bus-width = <4>;
+			cd-inverted;
+			status = "disabled";
+		};
+
+		mmc3: mmc@01c12000 {
+			compatible = "allwinner,sun4i-a10-mmc";
+			reg = <0x01c12000 0x1000>;
+			clocks = <&ahb_gates 11>, <&mmc3_clk>;
+			clock-names = "ahb", "mod";
+			interrupts = <35>;
+			bus-width = <4>;
+			cd-inverted;
+			status = "disabled";
+		};
+
 		usbphy: phy@01c13400 {
 			#phy-cells = <1>;
 			compatible = "allwinner,sun4i-a10-usb-phy";
@@ -529,6 +573,20 @@
 				allwinner,drive = <0>;
 				allwinner,pull = <0>;
 			};
+
+			mmc0_pins_a: mmc0@0 {
+				allwinner,pins = "PF0","PF1","PF2","PF3","PF4","PF5";
+				allwinner,function = "mmc0";
+				allwinner,drive = <2>;
+				allwinner,pull = <0>;
+			};
+
+			mmc0_cd_pin_reference_design: mmc0_cd_pin@0 {
+				allwinner,pins = "PH1";
+				allwinner,function = "gpio_in";
+				allwinner,drive = <0>;
+				allwinner,pull = <1>;
+			};
 		};
 
 		timer@01c20c00 {
--- a/arch/arm/boot/dts/sun4i-a10-mini-xplus.dts
+++ b/arch/arm/boot/dts/sun4i-a10-mini-xplus.dts
@@ -20,6 +20,14 @@
 	compatible = "pineriver,mini-xplus", "allwinner,sun4i-a10";
 
 	soc@01c00000 {
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_reference_design>;
+			cd-gpios = <&pio 7 1 0>; /* PH1 */
+			status = "okay";
+		};
+
 		usbphy: phy@01c13400 {
 			usb1_vbus-supply = <&reg_usb1_vbus>;
 			usb2_vbus-supply = <&reg_usb2_vbus>;
--- a/arch/arm/boot/dts/sun4i-a10-olinuxino-lime.dts
+++ b/arch/arm/boot/dts/sun4i-a10-olinuxino-lime.dts
@@ -33,6 +33,15 @@
 			};
 		};
 
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_reference_design>;
+			cd-gpios = <&pio 7 1 0>; /* PH1 */
+			cd-mode = <1>;
+			status = "okay";
+		};
+
 		usbphy: phy@01c13400 {
 			usb1_vbus-supply = <&reg_usb1_vbus>;
 			usb2_vbus-supply = <&reg_usb2_vbus>;
--- a/arch/arm/boot/dts/sun4i-a10-pcduino.dts
+++ b/arch/arm/boot/dts/sun4i-a10-pcduino.dts
@@ -34,6 +34,14 @@
 			};
 		};
 
+		mmc0: mmc@01c0f000 {
+			pinctrl-names = "default", "default";
+			pinctrl-0 = <&mmc0_pins_a>;
+			pinctrl-1 = <&mmc0_cd_pin_reference_design>;
+			cd-gpios = <&pio 7 1 0>; /* PH1 */
+			status = "okay";
+		};
+
 		usbphy: phy@01c13400 {
 			usb1_vbus-supply = <&reg_usb1_vbus>;
 			usb2_vbus-supply = <&reg_usb2_vbus>;
