From: Felix Fietkau <nbd@openwrt.org>
Date: Sat, 15 Nov 2014 22:38:07 +0100
Subject: [PATCH] mac80211: minstrel: switch to .tx_status_noskb

Signed-off-by: Felix Fietkau <nbd@openwrt.org>
---

--- a/net/mac80211/rc80211_minstrel.c
+++ b/net/mac80211/rc80211_minstrel.c
@@ -223,11 +223,10 @@ minstrel_update_stats(struct minstrel_pr
 static void
 minstrel_tx_status(void *priv, struct ieee80211_supported_band *sband,
 		   struct ieee80211_sta *sta, void *priv_sta,
-		   struct sk_buff *skb)
+		   struct ieee80211_tx_info *info)
 {
 	struct minstrel_priv *mp = priv;
 	struct minstrel_sta_info *mi = priv_sta;
-	struct ieee80211_tx_info *info = IEEE80211_SKB_CB(skb);
 	struct ieee80211_tx_rate *ar = info->status.rates;
 	int i, ndx;
 	int success;
@@ -674,7 +673,7 @@ static u32 minstrel_get_expected_through
 
 const struct rate_control_ops mac80211_minstrel = {
 	.name = "minstrel",
-	.tx_status = minstrel_tx_status,
+	.tx_status_noskb = minstrel_tx_status,
 	.get_rate = minstrel_get_rate,
 	.rate_init = minstrel_rate_init,
 	.alloc = minstrel_alloc,
