--- a/drivers/bcma/bcma_private.h
+++ b/drivers/bcma/bcma_private.h
@@ -24,6 +24,7 @@ struct bcma_bus;
 /* main.c */
 bool bcma_wait_value(struct bcma_device *core, u16 reg, u32 mask, u32 value,
 		     int timeout);
+void bcma_prepare_core(struct bcma_bus *bus, struct bcma_device *core);
 int bcma_bus_register(struct bcma_bus *bus);
 void bcma_bus_unregister(struct bcma_bus *bus);
 int __init bcma_bus_early_register(struct bcma_bus *bus,
--- a/drivers/bcma/driver_chipcommon.c
+++ b/drivers/bcma/driver_chipcommon.c
@@ -339,7 +339,7 @@ void bcma_chipco_serial_init(struct bcma
 		return;
 	}
 
-	irq = bcma_core_irq(cc->core);
+	irq = bcma_core_irq(cc->core, 0);
 
 	/* Determine the registers of the UARTs */
 	cc->nr_serial_ports = (cc->capabilities & BCMA_CC_CAP_NRUART);
--- a/drivers/bcma/driver_gpio.c
+++ b/drivers/bcma/driver_gpio.c
@@ -152,7 +152,7 @@ static int bcma_gpio_irq_domain_init(str
 					 handle_simple_irq);
 	}
 
-	hwirq = bcma_core_irq(cc->core);
+	hwirq = bcma_core_irq(cc->core, 0);
 	err = request_irq(hwirq, bcma_gpio_irq_handler, IRQF_SHARED, "gpio",
 			  cc);
 	if (err)
@@ -183,7 +183,7 @@ static void bcma_gpio_irq_domain_exit(st
 		return;
 
 	bcma_cc_mask32(cc, BCMA_CC_IRQMASK, ~BCMA_CC_IRQ_GPIO);
-	free_irq(bcma_core_irq(cc->core), cc);
+	free_irq(bcma_core_irq(cc->core, 0), cc);
 	for (gpio = 0; gpio < chip->ngpio; gpio++) {
 		int irq = irq_find_mapping(cc->irq_domain, gpio);
 
--- a/drivers/bcma/driver_mips.c
+++ b/drivers/bcma/driver_mips.c
@@ -115,7 +115,7 @@ static u32 bcma_core_mips_irqflag(struct
  * If disabled, 5 is returned.
  * If not supported, 6 is returned.
  */
-static unsigned int bcma_core_mips_irq(struct bcma_device *dev)
+unsigned int bcma_core_mips_irq(struct bcma_device *dev)
 {
 	struct bcma_device *mdev = dev->bus->drv_mips.core;
 	u32 irqflag;
@@ -133,13 +133,6 @@ static unsigned int bcma_core_mips_irq(s
 	return 5;
 }
 
-unsigned int bcma_core_irq(struct bcma_device *dev)
-{
-	unsigned int mips_irq = bcma_core_mips_irq(dev);
-	return mips_irq <= 4 ? mips_irq + 2 : 0;
-}
-EXPORT_SYMBOL(bcma_core_irq);
-
 static void bcma_core_mips_set_irq(struct bcma_device *dev, unsigned int irq)
 {
 	unsigned int oldirq = bcma_core_mips_irq(dev);
@@ -423,7 +416,7 @@ void bcma_core_mips_init(struct bcma_drv
 		break;
 	default:
 		list_for_each_entry(core, &bus->cores, list) {
-			core->irq = bcma_core_irq(core);
+			core->irq = bcma_core_irq(core, 0);
 		}
 		bcma_err(bus,
 			 "Unknown device (0x%x) found, can not configure IRQs\n",
--- a/drivers/bcma/driver_pci_host.c
+++ b/drivers/bcma/driver_pci_host.c
@@ -593,7 +593,7 @@ int bcma_core_pci_plat_dev_init(struct p
 	pr_info("PCI: Fixing up device %s\n", pci_name(dev));
 
 	/* Fix up interrupt lines */
-	dev->irq = bcma_core_irq(pc_host->pdev->core);
+	dev->irq = bcma_core_irq(pc_host->pdev->core, 0);
 	pci_write_config_byte(dev, PCI_INTERRUPT_LINE, dev->irq);
 
 	readrq = pcie_get_readrq(dev);
@@ -617,6 +617,6 @@ int bcma_core_pci_pcibios_map_irq(const 
 
 	pc_host = container_of(dev->bus->ops, struct bcma_drv_pci_host,
 			       pci_ops);
-	return bcma_core_irq(pc_host->pdev->core);
+	return bcma_core_irq(pc_host->pdev->core, 0);
 }
 EXPORT_SYMBOL(bcma_core_pci_pcibios_map_irq);
--- a/drivers/bcma/main.c
+++ b/drivers/bcma/main.c
@@ -11,6 +11,7 @@
 #include <linux/bcma/bcma.h>
 #include <linux/slab.h>
 #include <linux/of_address.h>
+#include <linux/of_irq.h>
 
 MODULE_DESCRIPTION("Broadcom's specific AMBA driver");
 MODULE_LICENSE("GPL");
@@ -153,6 +154,46 @@ static struct device_node *bcma_of_find_
 	return NULL;
 }
 
+static int bcma_of_irq_parse(struct platform_device *parent,
+			     struct bcma_device *core,
+			     struct of_phandle_args *out_irq, int num)
+{
+	__be32 laddr[1];
+	int rc;
+
+	if (core->dev.of_node) {
+		rc = of_irq_parse_one(core->dev.of_node, num, out_irq);
+		if (!rc)
+			return rc;
+	}
+
+	out_irq->np = parent->dev.of_node;
+	out_irq->args_count = 1;
+	out_irq->args[0] = num;
+
+	laddr[0] = cpu_to_be32(core->addr);
+	return of_irq_parse_raw(laddr, out_irq);
+}
+
+static unsigned int bcma_of_get_irq(struct platform_device *parent,
+				    struct bcma_device *core, int num)
+{
+	struct of_phandle_args out_irq;
+	int ret;
+
+	if (!parent || !parent->dev.of_node)
+		return 0;
+
+	ret = bcma_of_irq_parse(parent, core, &out_irq, num);
+	if (ret) {
+		bcma_debug(core->bus, "bcma_of_get_irq() failed with rc=%d\n",
+			   ret);
+		return 0;
+	}
+
+	return irq_create_of_mapping(&out_irq);
+}
+
 static void bcma_of_fill_device(struct platform_device *parent,
 				struct bcma_device *core)
 {
@@ -161,18 +202,47 @@ static void bcma_of_fill_device(struct p
 	node = bcma_of_find_child_device(parent, core);
 	if (node)
 		core->dev.of_node = node;
+
+	core->irq = bcma_of_get_irq(parent, core, 0);
 }
 #else
 static void bcma_of_fill_device(struct platform_device *parent,
 				struct bcma_device *core)
 {
 }
+static inline unsigned int bcma_of_get_irq(struct platform_device *parent,
+					   struct bcma_device *core, int num)
+{
+	return 0;
+}
 #endif /* CONFIG_OF */
 
-static void bcma_register_core(struct bcma_bus *bus, struct bcma_device *core)
+unsigned int bcma_core_irq(struct bcma_device *core, int num)
 {
-	int err;
+	struct bcma_bus *bus = core->bus;
+	unsigned int mips_irq;
+
+	switch (bus->hosttype) {
+	case BCMA_HOSTTYPE_PCI:
+		return bus->host_pci->irq;
+	case BCMA_HOSTTYPE_SOC:
+		if (bus->drv_mips.core && num == 0) {
+			mips_irq = bcma_core_mips_irq(core);
+			return mips_irq <= 4 ? mips_irq + 2 : 0;
+		}
+		if (bus->host_pdev)
+			return bcma_of_get_irq(bus->host_pdev, core, num);
+		return 0;
+	case BCMA_HOSTTYPE_SDIO:
+		return 0;
+	}
 
+	return 0;
+}
+EXPORT_SYMBOL(bcma_core_irq);
+
+void bcma_prepare_core(struct bcma_bus *bus, struct bcma_device *core)
+{
 	core->dev.release = bcma_release_core_dev;
 	core->dev.bus = &bcma_bus_type;
 	dev_set_name(&core->dev, "bcma%d:%d", bus->num, core->core_index);
@@ -196,6 +266,11 @@ static void bcma_register_core(struct bc
 	case BCMA_HOSTTYPE_SDIO:
 		break;
 	}
+}
+
+static void bcma_register_core(struct bcma_bus *bus, struct bcma_device *core)
+{
+	int err;
 
 	err = device_register(&core->dev);
 	if (err) {
--- a/drivers/bcma/scan.c
+++ b/drivers/bcma/scan.c
@@ -505,6 +505,7 @@ int bcma_bus_scan(struct bcma_bus *bus)
 		bus->nr_cores++;
 		other_core = bcma_find_core_reverse(bus, core->id.id);
 		core->core_unit = (other_core == NULL) ? 0 : other_core->core_unit + 1;
+		bcma_prepare_core(bus, core);
 
 		bcma_info(bus, "Core %d found: %s (manuf 0x%03X, id 0x%03X, rev 0x%02X, class 0x%X)\n",
 			  core->core_index, bcma_device_name(&core->id),
--- a/include/linux/bcma/bcma.h
+++ b/include/linux/bcma/bcma.h
@@ -447,4 +447,6 @@ extern u32 bcma_chipco_pll_read(struct b
 #define  BCMA_DMA_TRANSLATION_DMA64_CMT	0x80000000 /* Client Mode Translation for 64-bit DMA */
 extern u32 bcma_core_dma_translation(struct bcma_device *core);
 
+extern unsigned int bcma_core_irq(struct bcma_device *core, int num);
+
 #endif /* LINUX_BCMA_H_ */
--- a/include/linux/bcma/bcma_driver_mips.h
+++ b/include/linux/bcma/bcma_driver_mips.h
@@ -43,12 +43,12 @@ struct bcma_drv_mips {
 extern void bcma_core_mips_init(struct bcma_drv_mips *mcore);
 extern void bcma_core_mips_early_init(struct bcma_drv_mips *mcore);
 
-extern unsigned int bcma_core_irq(struct bcma_device *core);
+extern unsigned int bcma_core_mips_irq(struct bcma_device *dev);
 #else
 static inline void bcma_core_mips_init(struct bcma_drv_mips *mcore) { }
 static inline void bcma_core_mips_early_init(struct bcma_drv_mips *mcore) { }
 
-static inline unsigned int bcma_core_irq(struct bcma_device *core)
+static inline unsigned int bcma_core_mips_irq(struct bcma_device *dev)
 {
 	return 0;
 }
