--- a/nl80211.h
+++ b/nl80211.h
@@ -503,6 +503,9 @@
  *	TX status event pertaining to the TX request.
  *	%NL80211_ATTR_TX_NO_CCK_RATE is used to decide whether to send the
  *	management frames at CCK rate or not in 2GHz band.
+ *	%NL80211_ATTR_CSA_C_OFFSETS_TX is an array of offsets to CSA
+ *	counters which will be updated to the current value. This attribute
+ *	is used during CSA period.
  * @NL80211_CMD_FRAME_WAIT_CANCEL: When an off-channel TX was requested, this
  *	command may be used with the corresponding cookie to cancel the wait
  *	time if it is known that it is no longer necessary.
@@ -719,6 +722,22 @@
  *	QoS mapping is relevant for IP packets, it is only valid during an
  *	association. This is cleared on disassociation and AP restart.
  *
+ * @NL80211_CMD_ADD_TX_TS: Ask the kernel to add a traffic stream for the given
+ *	%NL80211_ATTR_TSID and %NL80211_ATTR_MAC with %NL80211_ATTR_USER_PRIO
+ *	and %NL80211_ATTR_ADMITTED_TIME parameters.
+ *	Note that the action frame handshake with the AP shall be handled by
+ *	userspace via the normal management RX/TX framework, this only sets
+ *	up the TX TS in the driver/device.
+ *	If the admitted time attribute is not added then the request just checks
+ *	if a subsequent setup could be successful, the intent is to use this to
+ *	avoid setting up a session with the AP when local restrictions would
+ *	make that impossible. However, the subsequent "real" setup may still
+ *	fail even if the check was successful.
+ * @NL80211_CMD_DEL_TX_TS: Remove an existing TS with the %NL80211_ATTR_TSID
+ *	and %NL80211_ATTR_MAC parameters. It isn't necessary to call this
+ *	before removing a station entry entirely, or before disassociating
+ *	or similar, cleanup will happen in the driver/device in this case.
+ *
  * @NL80211_CMD_MAX: highest used command number
  * @__NL80211_CMD_AFTER_LAST: internal use
  */
@@ -890,6 +909,9 @@ enum nl80211_commands {
 
 	NL80211_CMD_SET_QOS_MAP,
 
+	NL80211_CMD_ADD_TX_TS,
+	NL80211_CMD_DEL_TX_TS,
+
 	/* add new commands above here */
 
 	/* used to define NL80211_CMD_MAX below */
@@ -1525,10 +1547,10 @@ enum nl80211_commands {
  *	operation).
  * @NL80211_ATTR_CSA_IES: Nested set of attributes containing the IE information
  *	for the time while performing a channel switch.
- * @NL80211_ATTR_CSA_C_OFF_BEACON: Offset of the channel switch counter
- *	field in the beacons tail (%NL80211_ATTR_BEACON_TAIL).
- * @NL80211_ATTR_CSA_C_OFF_PRESP: Offset of the channel switch counter
- *	field in the probe response (%NL80211_ATTR_PROBE_RESP).
+ * @NL80211_ATTR_CSA_C_OFF_BEACON: An array of offsets (u16) to the channel
+ *	switch counters in the beacons tail (%NL80211_ATTR_BEACON_TAIL).
+ * @NL80211_ATTR_CSA_C_OFF_PRESP: An array of offsets (u16) to the channel
+ *	switch counters in the probe response (%NL80211_ATTR_PROBE_RESP).
  *
  * @NL80211_ATTR_RXMGMT_FLAGS: flags for nl80211_send_mgmt(), u32.
  *	As specified in the &enum nl80211_rxmgmt_flags.
@@ -1576,9 +1598,49 @@ enum nl80211_commands {
  *	advertise values that cannot always be met. In such cases, an attempt
  *	to add a new station entry with @NL80211_CMD_NEW_STATION may fail.
  *
+ * @NL80211_ATTR_CSA_C_OFFSETS_TX: An array of csa counter offsets (u16) which
+ *	should be updated when the frame is transmitted.
+ * @NL80211_ATTR_MAX_CSA_COUNTERS: U8 attribute used to advertise the maximum
+ *	supported number of csa counters.
+ *
  * @NL80211_ATTR_TDLS_PEER_CAPABILITY: flags for TDLS peer capabilities, u32.
  *	As specified in the &enum nl80211_tdls_peer_capability.
  *
+ * @NL80211_ATTR_IFACE_SOCKET_OWNER: flag attribute, if set during interface
+ *	creation then the new interface will be owned by the netlink socket
+ *	that created it and will be destroyed when the socket is closed
+ *
+ * @NL80211_ATTR_TDLS_INITIATOR: flag attribute indicating the current end is
+ *	the TDLS link initiator.
+ *
+ * @NL80211_ATTR_USE_RRM: flag for indicating whether the current connection
+ *	shall support Radio Resource Measurements (11k). This attribute can be
+ *	used with %NL80211_CMD_ASSOCIATE and %NL80211_CMD_CONNECT requests.
+ *	User space applications are expected to use this flag only if the
+ *	underlying device supports these minimal RRM features:
+ *		%NL80211_FEATURE_DS_PARAM_SET_IE_IN_PROBES,
+ *		%NL80211_FEATURE_QUIET,
+ *	If this flag is used, driver must add the Power Capabilities IE to the
+ *	association request. In addition, it must also set the RRM capability
+ *	flag in the association request's Capability Info field.
+ *
+ * @NL80211_ATTR_WIPHY_DYN_ACK: flag attribute used to enable ACK timeout
+ *	estimation algorithm (dynack). In order to activate dynack
+ *	%NL80211_FEATURE_ACKTO_ESTIMATION feature flag must be set by lower
+ *	drivers to indicate dynack capability. Dynack is automatically disabled
+ *	setting valid value for coverage class.
+ *
+ * @NL80211_ATTR_TSID: a TSID value (u8 attribute)
+ * @NL80211_ATTR_USER_PRIO: user priority value (u8 attribute)
+ * @NL80211_ATTR_ADMITTED_TIME: admitted time in units of 32 microseconds
+ *	(per second) (u16 attribute)
+ *
+ * @NL80211_ATTR_SMPS_MODE: SMPS mode to use (ap mode). see
+ *	&enum nl80211_smps_mode.
+ *
+ * @NL80211_ATTR_WIPHY_ANTENNA_GAIN: Configured antenna gain. Used to reduce
+ *	transmit power to stay within regulatory limits. u32, dBi.
+ *
  * @NL80211_ATTR_MAX: highest attribute number currently defined
  * @__NL80211_ATTR_AFTER_LAST: internal use
  */
@@ -1914,6 +1976,25 @@ enum nl80211_attrs {
 
 	NL80211_ATTR_TDLS_PEER_CAPABILITY,
 
+	NL80211_ATTR_IFACE_SOCKET_OWNER,
+
+	NL80211_ATTR_CSA_C_OFFSETS_TX,
+	NL80211_ATTR_MAX_CSA_COUNTERS,
+
+	NL80211_ATTR_TDLS_INITIATOR,
+
+	NL80211_ATTR_USE_RRM,
+
+	NL80211_ATTR_WIPHY_DYN_ACK,
+
+	NL80211_ATTR_TSID,
+	NL80211_ATTR_USER_PRIO,
+	NL80211_ATTR_ADMITTED_TIME,
+
+	NL80211_ATTR_SMPS_MODE,
+
+	NL80211_ATTR_WIPHY_ANTENNA_GAIN,
+
 	/* add attributes here, update the policy in nl80211.c */
 
 	__NL80211_ATTR_AFTER_LAST,
@@ -2182,6 +2263,8 @@ enum nl80211_sta_bss_param {
  *	Contains a nested array of signal strength attributes (u8, dBm)
  * @NL80211_STA_INFO_CHAIN_SIGNAL_AVG: per-chain signal strength average
  *	Same format as NL80211_STA_INFO_CHAIN_SIGNAL.
+ * @NL80211_STA_EXPECTED_THROUGHPUT: expected throughput considering also the
+ *	802.11 header (u32, kbps)
  * @__NL80211_STA_INFO_AFTER_LAST: internal
  * @NL80211_STA_INFO_MAX: highest possible station info attribute
  */
@@ -2213,6 +2296,7 @@ enum nl80211_sta_info {
 	NL80211_STA_INFO_TX_BYTES64,
 	NL80211_STA_INFO_CHAIN_SIGNAL,
 	NL80211_STA_INFO_CHAIN_SIGNAL_AVG,
+	NL80211_STA_INFO_EXPECTED_THROUGHPUT,
 
 	/* keep last */
 	__NL80211_STA_INFO_AFTER_LAST,
@@ -2336,9 +2420,34 @@ enum nl80211_band_attr {
  *	using this channel as the primary or any of the secondary channels
  *	isn't possible
  * @NL80211_FREQUENCY_ATTR_DFS_CAC_TIME: DFS CAC time in milliseconds.
+ * @NL80211_FREQUENCY_ATTR_INDOOR_ONLY: Only indoor use is permitted on this
+ *	channel. A channel that has the INDOOR_ONLY attribute can only be
+ *	used when there is a clear assessment that the device is operating in
+ *	an indoor surroundings, i.e., it is connected to AC power (and not
+ *	through portable DC inverters) or is under the control of a master
+ *	that is acting as an AP and is connected to AC power.
+ * @NL80211_FREQUENCY_ATTR_GO_CONCURRENT: GO operation is allowed on this
+ *	channel if it's connected concurrently to a BSS on the same channel on
+ *	the 2 GHz band or to a channel in the same UNII band (on the 5 GHz
+ *	band), and IEEE80211_CHAN_RADAR is not set. Instantiating a GO on a
+ *	channel that has the GO_CONCURRENT attribute set can be done when there
+ *	is a clear assessment that the device is operating under the guidance of
+ *	an authorized master, i.e., setting up a GO while the device is also
+ *	connected to an AP with DFS and radar detection on the UNII band (it is
+ *	up to user-space, i.e., wpa_supplicant to perform the required
+ *	verifications)
+ * @NL80211_FREQUENCY_ATTR_NO_20MHZ: 20 MHz operation is not allowed
+ *	on this channel in current regulatory domain.
+ * @NL80211_FREQUENCY_ATTR_NO_10MHZ: 10 MHz operation is not allowed
+ *	on this channel in current regulatory domain.
  * @NL80211_FREQUENCY_ATTR_MAX: highest frequency attribute number
  *	currently defined
  * @__NL80211_FREQUENCY_ATTR_AFTER_LAST: internal use
+ *
+ * See https://apps.fcc.gov/eas/comments/GetPublishedDocument.html?id=327&tn=528122
+ * for more information on the FCC description of the relaxations allowed
+ * by NL80211_FREQUENCY_ATTR_INDOOR_ONLY and
+ * NL80211_FREQUENCY_ATTR_GO_CONCURRENT.
  */
 enum nl80211_frequency_attr {
 	__NL80211_FREQUENCY_ATTR_INVALID,
@@ -2355,6 +2464,10 @@ enum nl80211_frequency_attr {
 	NL80211_FREQUENCY_ATTR_NO_80MHZ,
 	NL80211_FREQUENCY_ATTR_NO_160MHZ,
 	NL80211_FREQUENCY_ATTR_DFS_CAC_TIME,
+	NL80211_FREQUENCY_ATTR_INDOOR_ONLY,
+	NL80211_FREQUENCY_ATTR_GO_CONCURRENT,
+	NL80211_FREQUENCY_ATTR_NO_20MHZ,
+	NL80211_FREQUENCY_ATTR_NO_10MHZ,
 
 	/* keep last */
 	__NL80211_FREQUENCY_ATTR_AFTER_LAST,
@@ -2573,10 +2686,13 @@ enum nl80211_dfs_regions {
  *	present has been registered with the wireless core that
  *	has listed NL80211_FEATURE_CELL_BASE_REG_HINTS as a
  *	supported feature.
+ * @NL80211_USER_REG_HINT_INDOOR: a user sent an hint indicating that the
+ *	platform is operating in an indoor environment.
  */
 enum nl80211_user_reg_hint_type {
 	NL80211_USER_REG_HINT_USER	= 0,
 	NL80211_USER_REG_HINT_CELL_BASE = 1,
+	NL80211_USER_REG_HINT_INDOOR    = 2,
 };
 
 /**
@@ -2998,14 +3114,20 @@ enum nl80211_bss_scan_width {
  * @NL80211_BSS_BSSID: BSSID of the BSS (6 octets)
  * @NL80211_BSS_FREQUENCY: frequency in MHz (u32)
  * @NL80211_BSS_TSF: TSF of the received probe response/beacon (u64)
+ *	(if @NL80211_BSS_PRESP_DATA is present then this is known to be
+ *	from a probe response, otherwise it may be from the same beacon
+ *	that the NL80211_BSS_BEACON_TSF will be from)
  * @NL80211_BSS_BEACON_INTERVAL: beacon interval of the (I)BSS (u16)
  * @NL80211_BSS_CAPABILITY: capability field (CPU order, u16)
  * @NL80211_BSS_INFORMATION_ELEMENTS: binary attribute containing the
  *	raw information elements from the probe response/beacon (bin);
- *	if the %NL80211_BSS_BEACON_IES attribute is present, the IEs here are
- *	from a Probe Response frame; otherwise they are from a Beacon frame.
+ *	if the %NL80211_BSS_BEACON_IES attribute is present and the data is
+ *	different then the IEs here are from a Probe Response frame; otherwise
+ *	they are from a Beacon frame.
  *	However, if the driver does not indicate the source of the IEs, these
  *	IEs may be from either frame subtype.
+ *	If present, the @NL80211_BSS_PRESP_DATA attribute indicates that the
+ *	data here is known to be from a probe response, without any heuristics.
  * @NL80211_BSS_SIGNAL_MBM: signal strength of probe response/beacon
  *	in mBm (100 * dBm) (s32)
  * @NL80211_BSS_SIGNAL_UNSPEC: signal strength of the probe response/beacon
@@ -3017,6 +3139,10 @@ enum nl80211_bss_scan_width {
  *	yet been received
  * @NL80211_BSS_CHAN_WIDTH: channel width of the control channel
  *	(u32, enum nl80211_bss_scan_width)
+ * @NL80211_BSS_BEACON_TSF: TSF of the last received beacon (u64)
+ *	(not present if no beacon frame has been received yet)
+ * @NL80211_BSS_PRESP_DATA: the data in @NL80211_BSS_INFORMATION_ELEMENTS and
+ *	@NL80211_BSS_TSF is known to be from a probe response (flag attribute)
  * @__NL80211_BSS_AFTER_LAST: internal
  * @NL80211_BSS_MAX: highest BSS attribute
  */
@@ -3034,6 +3160,8 @@ enum nl80211_bss {
 	NL80211_BSS_SEEN_MS_AGO,
 	NL80211_BSS_BEACON_IES,
 	NL80211_BSS_CHAN_WIDTH,
+	NL80211_BSS_BEACON_TSF,
+	NL80211_BSS_PRESP_DATA,
 
 	/* keep last */
 	__NL80211_BSS_AFTER_LAST,
@@ -3650,6 +3778,8 @@ enum nl80211_iface_limit_attrs {
  *	different channels may be used within this group.
  * @NL80211_IFACE_COMB_RADAR_DETECT_WIDTHS: u32 attribute containing the bitmap
  *	of supported channel widths for radar detection.
+ * @NL80211_IFACE_COMB_RADAR_DETECT_REGIONS: u32 attribute containing the bitmap
+ *	of supported regulatory regions for radar detection.
  * @NUM_NL80211_IFACE_COMB: number of attributes
  * @MAX_NL80211_IFACE_COMB: highest attribute number
  *
@@ -3683,6 +3813,7 @@ enum nl80211_if_combination_attrs {
 	NL80211_IFACE_COMB_STA_AP_BI_MATCH,
 	NL80211_IFACE_COMB_NUM_CHANNELS,
 	NL80211_IFACE_COMB_RADAR_DETECT_WIDTHS,
+	NL80211_IFACE_COMB_RADAR_DETECT_REGIONS,
 
 	/* keep last */
 	NUM_NL80211_IFACE_COMB,
@@ -3893,6 +4024,29 @@ enum nl80211_ap_sme_features {
  *	interface. An active monitor interface behaves like a normal monitor
  *	interface, but gets added to the driver. It ensures that incoming
  *	unicast packets directed at the configured interface address get ACKed.
+ * @NL80211_FEATURE_AP_MODE_CHAN_WIDTH_CHANGE: This driver supports dynamic
+ *	channel bandwidth change (e.g., HT 20 <-> 40 MHz channel) during the
+ *	lifetime of a BSS.
+ * @NL80211_FEATURE_DS_PARAM_SET_IE_IN_PROBES: This device adds a DS Parameter
+ *	Set IE to probe requests.
+ * @NL80211_FEATURE_WFA_TPC_IE_IN_PROBES: This device adds a WFA TPC Report IE
+ *	to probe requests.
+ * @NL80211_FEATURE_QUIET: This device, in client mode, supports Quiet Period
+ *	requests sent to it by an AP.
+ * @NL80211_FEATURE_TX_POWER_INSERTION: This device is capable of inserting the
+ *	current tx power value into the TPC Report IE in the spectrum
+ *	management TPC Report action frame, and in the Radio Measurement Link
+ *	Measurement Report action frame.
+ * @NL80211_FEATURE_ACKTO_ESTIMATION: This driver supports dynamic ACK timeout
+ *	estimation (dynack). %NL80211_ATTR_WIPHY_DYN_ACK flag attribute is used
+ *	to enable dynack.
+ * @NL80211_FEATURE_STATIC_SMPS: Device supports static spatial
+ *	multiplexing powersave, ie. can turn off all but one chain
+ *	even on HT connections that should be using more chains.
+ * @NL80211_FEATURE_DYNAMIC_SMPS: Device supports dynamic spatial
+ *	multiplexing powersave, ie. can turn off all but one chain
+ *	and then wake the rest up as required after, for example,
+ *	rts/cts handshake.
  */
 enum nl80211_feature_flags {
 	NL80211_FEATURE_SK_TX_STATUS			= 1 << 0,
@@ -3913,6 +4067,14 @@ enum nl80211_feature_flags {
 	NL80211_FEATURE_FULL_AP_CLIENT_STATE		= 1 << 15,
 	NL80211_FEATURE_USERSPACE_MPM			= 1 << 16,
 	NL80211_FEATURE_ACTIVE_MONITOR			= 1 << 17,
+	NL80211_FEATURE_AP_MODE_CHAN_WIDTH_CHANGE	= 1 << 18,
+	NL80211_FEATURE_DS_PARAM_SET_IE_IN_PROBES	= 1 << 19,
+	NL80211_FEATURE_WFA_TPC_IE_IN_PROBES		= 1 << 20,
+	NL80211_FEATURE_QUIET				= 1 << 21,
+	NL80211_FEATURE_TX_POWER_INSERTION		= 1 << 22,
+	NL80211_FEATURE_ACKTO_ESTIMATION		= 1 << 23,
+	NL80211_FEATURE_STATIC_SMPS			= 1 << 24,
+	NL80211_FEATURE_DYNAMIC_SMPS			= 1 << 25,
 };
 
 /**
@@ -3987,6 +4149,25 @@ enum nl80211_acl_policy {
 };
 
 /**
+ * enum nl80211_smps_mode - SMPS mode
+ *
+ * Requested SMPS mode (for AP mode)
+ *
+ * @NL80211_SMPS_OFF: SMPS off (use all antennas).
+ * @NL80211_SMPS_STATIC: static SMPS (use a single antenna)
+ * @NL80211_SMPS_DYNAMIC: dynamic smps (start with a single antenna and
+ *	turn on other antennas after CTS/RTS).
+ */
+enum nl80211_smps_mode {
+	NL80211_SMPS_OFF,
+	NL80211_SMPS_STATIC,
+	NL80211_SMPS_DYNAMIC,
+
+	__NL80211_SMPS_AFTER_LAST,
+	NL80211_SMPS_MAX = __NL80211_SMPS_AFTER_LAST - 1
+};
+
+/**
  * enum nl80211_radar_event - type of radar event for DFS operation
  *
  * Type of event to be used with NL80211_ATTR_RADAR_EVENT to inform userspace
