# Virtual x86
Run KolibriOS, Linux or Windows 98 in your browser

#### Select profile

Arch Linux 12 MB >_ | Complete Arch Linux with various compilers, networking and Xorg. Restored from snapshot.
Damn Small Linux 50 MB 💻 | Graphical Linux with 2.4 kernel, Firefox 2.0 and more. Takes 1 minute to boot.
Buildroot Linux 5.0 MB >_ | Minimal Linux with busybox, Lua, tests, internet access, ping, telnet and curl. Exchange files through `/mnt/`.
ReactOS 18 MB 💻 | Windows-compatible OS with QtWeb and Breakout. Restored from snapshot.
Windows 2000 22 MB 💻 | Including Pinball and Internet Explorer with internet access. Additional sectors are loaded as needed.
Windows 98 9.7 MB 💻 | Including Minesweeper and Internet Explorer with internet access. Additional sectors are loaded as needed.
Windows 95 4.6 MB 💻 | Restored from snapshot
Windows 3.1 15 MB 💻 | Takes 15 seconds to boot
Windows 1.01 0.6 MB 💻 | The first version of Microsoft Windows
MS-DOS 6.22 4.4 MB >_ | With Enhanced Tools, QBasic, vim, games and demos.
FreeDOS 0.5 MB >_ | With nasm, vim, debug.com, Rogue, some games and demos.
FreeBSD 17 MB >_ | FreeBSD 12.0 base install. Restored from snapshot.
OpenBSD 12 MB >_ | OpenBSD 6.6 base install. Restored from snapshot.
9front 4.4 MB 💻 | A Plan 9 fork.
Haiku 38 MB 💻 | An open-source operating system inspired by BeOS. Restored from snapshot. Includes network support.
SerenityOS 17 MB 💻 | A graphical Unix-like operating system. Restored from snapshot.
HelenOS 7.9 MB 💻 | A graphical operating system based on a multiserver microkernel design
FiwixOS 15 MB >_ | A Unix-like OS written from scratch. Includes Doom.
Android-x86 42 MB 💻 | An x86 port of the Android 1.6. Quite slow. Takes about 3 minutes to boot.
Oberon 1.2 MB 💻 | Native Oberon 2.3.6
KolibriOS 1.4 MB 💻 | Fast graphical OS written in Assembly
QNX 1.3 MB 💻 | QNX 4.05 Demo disk (no networking)
Snowdrop 0.3 MB >_ | A homebrew operating system from scratch, written in assembly language
Solar OS 0.3 MB 💻 | Simple graphical OS
Bootchess 512 B >_ | A tiny chess program written in the boot sector
SectorLISP 512 B >_ | A LISP interpreter that fits into the boot sector

#### Setup

CD image |
Floppy disk image |
Hard disk image |
Kernel image (bzimage) |
initrd |
BIOS |

Disk images are not uploaded to the server

Memory size | MB
Video Memory size | MB
Networking proxy (leave blank to disable) |

Disable audio |
Enable ACPI (experimental) |

Boot order |

Scale:

Running: 0s
Speed: 0 mIPS
Avg speed: 0 mIPS
IDE device
Sectors read: 0
Bytes read: 0
Sectors written: 0
Bytes written: 0
Status:
9p Filesystem
Bytes read: 0
Bytes written: 0
Last file:
Status:
Network
Bytes received: 0
Bytes transmitted: 0
VGA
Mode:
Resolution: -
Mouse: No
Send files to emulator
Get file from emulator
`Version: 98e7110c2 (Feb 16, 2021 12:02)`

Enable debug — Readme — Project on Github — Compatibility