From daf75255fb67bf44db178e4c95a803b7972ed670 Mon Sep 17 00:00:00 2001
From: Hauke Mehrtens <hauke@hauke-m.de>
Date: Tue, 26 Sep 2017 22:29:06 +0200
Subject: ARM: dts: sunxi: add support for Orange Pi R1 board

Signed-off-by: Hauke Mehrtens <hauke@hauke-m.de>
---
 arch/arm/boot/dts/Makefile                      |   1 +
 arch/arm/boot/dts/sun8i-h2-plus-orangepi-r1.dts | 171 ++++++++++++++++++++++++
 2 files changed, 172 insertions(+)
 create mode 100644 arch/arm/boot/dts/sun8i-h2-plus-orangepi-r1.dts

--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -819,6 +819,7 @@ dtb-$(CONFIG_MACH_SUN8I) += \
 	sun8i-a33-sinlinx-sina33.dtb \
 	sun8i-a83t-allwinner-h8homlet-v2.dtb \
 	sun8i-a83t-cubietruck-plus.dtb \
+	sun8i-h2-plus-orangepi-r1.dtb \
 	sun8i-h3-bananapi-m2-plus.dtb \
 	sun8i-h3-nanopi-neo.dtb \
 	sun8i-h3-orangepi-2.dtb \
--- /dev/null
+++ b/arch/arm/boot/dts/sun8i-h2-plus-orangepi-r1.dts
@@ -0,0 +1,171 @@
+/*
+ * Copyright (C) 2017 Hauke Mehrtens <hauke@hauke-m.de>
+ *
+ * Based on sun8i-h2-plus-orangepi-zero.dts, which is:
+ *   Copyright (C) 2016 Icenowy Zheng <icenowy@aosc.xyz>
+ *
+ * Based on sun8i-h3-orangepi-one.dts, which is:
+ *   Copyright (C) 2016 Hans de Goede <hdegoede@redhat.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/dts-v1/;
+#include "sun8i-h3.dtsi"
+#include "sunxi-common-regulators.dtsi"
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/pinctrl/sun4i-a10.h>
+
+/ {
+	model = "Xunlong Orange Pi R1";
+	compatible = "xunlong,orangepi-r1", "allwinner,sun8i-h2-plus";
+
+	aliases {
+		serial0 = &uart0;
+		/* ethernet0 is the H3 emac, defined in sun8i-h3.dtsi */
+		ethernet0 = &emac;
+		ethernet1 = &xr819;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		pwr_led {
+			label = "orangepi:green:pwr";
+			gpios = <&r_pio 0 10 GPIO_ACTIVE_HIGH>;
+			default-state = "on";
+		};
+
+		status_led {
+			label = "orangepi:red:status";
+			gpios = <&pio 0 17 GPIO_ACTIVE_HIGH>;
+		};
+	};
+
+	reg_vcc_wifi: reg_vcc_wifi {
+		compatible = "regulator-fixed";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-name = "vcc-wifi";
+		enable-active-high;
+		gpio = <&pio 0 20 GPIO_ACTIVE_HIGH>;
+	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&r_pio 0 7 GPIO_ACTIVE_LOW>;
+		post-power-on-delay-ms = <200>;
+	};
+};
+
+&ehci1 {
+	status = "okay";
+};
+
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
+&mmc0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc0_pins_a>;
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <4>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_HIGH>; /* PF6 */
+	cd-inverted;
+	status = "okay";
+};
+
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins_a>;
+	vmmc-supply = <&reg_vcc_wifi>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	/*
+	 * Explicitly define the sdio device, so that we can add an ethernet
+	 * alias for it (which e.g. makes u-boot set a mac-address).
+	 */
+	xr819: sdio_wifi@1 {
+		reg = <1>;
+	};
+};
+
+&mmc1_pins_a {
+	bias-pull-up;
+};
+
+&ohci1 {
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins_a>;
+	status = "okay";
+};
+
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>;
+	status = "disabled";
+};
+
+&uart2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart2_pins>;
+	status = "disabled";
+};
+
+&usbphy {
+	/* USB VBUS is always on */
+	status = "okay";
+};
