From c02bc350f9dbce7d637c394a6e1c4d29dc5b28b2 Mon Sep 17 00:00:00 2001
From: Felix Fietkau <nbd@nbd.name>
Date: Tue, 12 Apr 2016 18:27:29 +0200
Subject: [PATCH] bgmac: fix MAC soft-reset bit for corerev > 4
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Only core revisions older than 4 use BGMAC_CMDCFG_SR_REV0. This mainly
fixes support for BCM4708A0KF SoCs with Ethernet core rev 5 (it means
only some devices as most of BCM4708A0KF-s got core rev 4).
This was tested for regressions on BCM47094 which doesn't seem to care
which bit gets used.

Signed-off-by: Felix Fietkau <nbd@nbd.name>
Signed-off-by: Rafał Miłecki <zajec5@gmail.com>
Signed-off-by: David S. Miller <davem@davemloft.net>
---

--- a/drivers/net/ethernet/broadcom/bgmac.h
+++ b/drivers/net/ethernet/broadcom/bgmac.h
@@ -198,9 +198,9 @@
 #define  BGMAC_CMDCFG_TAI			0x00000200
 #define  BGMAC_CMDCFG_HD			0x00000400	/* Set if in half duplex mode */
 #define  BGMAC_CMDCFG_HD_SHIFT			10
-#define  BGMAC_CMDCFG_SR_REV0			0x00000800	/* Set to reset mode, for other revs */
-#define  BGMAC_CMDCFG_SR_REV4			0x00002000	/* Set to reset mode, only for core rev 4 */
-#define  BGMAC_CMDCFG_SR(rev)  ((rev == 4) ? BGMAC_CMDCFG_SR_REV4 : BGMAC_CMDCFG_SR_REV0)
+#define  BGMAC_CMDCFG_SR_REV0			0x00000800	/* Set to reset mode, for core rev 0-3 */
+#define  BGMAC_CMDCFG_SR_REV4			0x00002000	/* Set to reset mode, for core rev >= 4 */
+#define  BGMAC_CMDCFG_SR(rev)  ((rev >= 4) ? BGMAC_CMDCFG_SR_REV4 : BGMAC_CMDCFG_SR_REV0)
 #define  BGMAC_CMDCFG_ML			0x00008000	/* Set to activate mac loopback mode */
 #define  BGMAC_CMDCFG_AE			0x00400000
 #define  BGMAC_CMDCFG_CFE			0x00800000
