--- a/drivers/spi/Kconfig
+++ b/drivers/spi/Kconfig
@@ -761,6 +761,13 @@ config SPI_TLE62X0
 	  sysfs interface, with each line presented as a kind of GPIO
 	  exposing both switch control and diagnostic feedback.
 
+config SPI_RB4XX_CPLD
+	tristate "MikroTik RB4XX CPLD driver"
+	depends on ATH79_MACH_RB4XX
+	help
+	  SPI driver for the Xilinx CPLD chip present on the
+	  MikroTik RB4xx boards.
+
 #
 # Add new SPI protocol masters in alphabetical order above this line
 #
--- a/drivers/spi/Makefile
+++ b/drivers/spi/Makefile
@@ -73,6 +73,7 @@ spi-pxa2xx-platform-objs		:= spi-pxa2xx.
 obj-$(CONFIG_SPI_PXA2XX)		+= spi-pxa2xx-platform.o
 obj-$(CONFIG_SPI_PXA2XX_PCI)		+= spi-pxa2xx-pci.o
 obj-$(CONFIG_SPI_RB4XX)			+= spi-rb4xx.o
+obj-$(CONFIG_SPI_RB4XX_CPLD)		+= spi-rb4xx-cpld.o
 obj-$(CONFIG_SPI_QUP)			+= spi-qup.o
 obj-$(CONFIG_SPI_ROCKCHIP)		+= spi-rockchip.o
 obj-$(CONFIG_SPI_RB4XX)			+= spi-rb4xx.o
