#!/bin/sh
#
# Copyright (C) 2011 OpenWrt.org
#

. /lib/functions/uci-defaults.sh

board_config_update

board=$(board_name)

case "$board" in
a40)
	ucidef_set_led_default "status-red" "Status (red)" "a40:red:status" "0"
	ucidef_set_led_default "status-blue" "Status (blue)" "a40:blue:status" "0"
	;;
a60)
	ucidef_set_led_default "status-red" "Status (red)" "a60:red:status" "0"
	ucidef_set_led_default "status-blue" "Status (blue)" "a60:blue:status" "0"
	;;
airgateway|\
airgatewaypro)
	ucidef_set_led_wlan "wlan" "WLAN" "ubnt:blue:wlan" "phy0tpt"
	;;
alfa-nx)
	ucidef_set_led_netdev "wan" "WAN" "alfa:green:led_2" "eth0"
	ucidef_set_led_netdev "lan" "LAN" "alfa:green:led_3" "eth1"
	;;
all0258n|\
all0315n)
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "$board:red:rssilow" "wlan0" "1" "40" "0" "6"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "$board:yellow:rssimedium" "wlan0" "30" "80" "-29" "5"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "$board:green:rssihigh" "wlan0" "70" "100" "-69" "8"
	;;
antminer-s1|\
antminer-s3)
	ucidef_set_led_default "sys" "SYS" "$board:green:sys" "0"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"

	case "$board" in
	antminer-s3)
		ucidef_set_led_default "lan" "LAN" "$board:yellow:lan" "0"
		;;
	esac
	;;
antrouter-r1)
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"
	ucidef_set_led_default "btc" "BTC" "$board:green:btc" "0"
	;;
ap121f)
	ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"
	;;
ap147-010)
	ucidef_set_led_netdev "wan" "WAN" "ap147:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "ap147:green:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "ap147:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "ap147:green:lan3" "switch0" "0x04"
	ucidef_set_led_switch "lan4" "LAN4" "ap147:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan2g" "WLAN 2.4 GHz" "ap147:green:wlan-2g" "phy0tpt"
	;;
ap90q|\
cpe505n|\
cpe830|\
cpe870|\
dr531|\
e600g-v2|\
e600gac-v2)
	ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth0"
	ucidef_set_led_netdev "wan" "WAN" "$board:green:wan" "eth1"

	case "$board" in
	ap90q)
		ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"
		;;
	cpe505n)
		ucidef_set_led_wlan "wlan" "WLAN" "$board:blue:wlan" "phy0tpt"
		;;
	cpe830|\
	cpe870)
		ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"
		ucidef_set_rssimon "wlan0" "200000" "1"
		ucidef_set_led_rssi "rssilow" "RSSILOW" "$board:green:link1" "wlan0" "1" "100" "0" "13"
		ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "$board:green:link2" "wlan0" "26" "100" "-25" "13"
		ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "$board:green:link3" "wlan0" "51" "100" "-50" "13"
		ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "$board:green:link4" "wlan0" "76" "100" "-75" "13"
		;;
	esac
	;;
ap531b0|\
gl-usb150|\
sc1750|\
sc450)
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"
	;;
ap91-5g|\
n5q)
	ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth0"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "signal1" "SIGNAL1" "$board:red:signal1" "wlan0" "1" "100"
	ucidef_set_led_rssi "signal2" "SIGNAL2" "$board:orange:signal2" "wlan0" "25" "100"
	ucidef_set_led_rssi "signal3" "SIGNAL3" "$board:green:signal3" "wlan0" "50" "100"
	ucidef_set_led_rssi "signal4" "SIGNAL4" "$board:green:signal4" "wlan0" "75" "100"

	case "$board" in
	n5q)
		ucidef_set_led_netdev "wan" "WAN" "$board:green:wan" "eth1"
		ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"
		;;
	esac
	;;
archer-c25-v1)
	ucidef_set_led_netdev "wan" "WAN" "$board:green:wan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "$board:green:wlan5g" "phy0tpt"
	ucidef_set_led_switch "lan1" "LAN1" "$board:green:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "$board:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "$board:green:lan3" "switch0" "0x04"
	ucidef_set_led_switch "lan4" "LAN4" "$board:green:lan4" "switch0" "0x02"
	;;
archer-c5|\
archer-c7)
	ucidef_set_led_usbdev "usb1" "USB1" "tp-link:green:usb1" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "tp-link:green:usb2" "2-1"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "tp-link:blue:wlan2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "tp-link:blue:wlan5g" "phy0tpt"
	;;
archer-c58-v1|\
archer-c59-v1|\
archer-c60-v1|\
archer-c60-v2)
	ucidef_set_led_switch "lan" "LAN" "$board:green:lan" "switch0" "0x1E"
	ucidef_set_led_netdev "wan" "WAN" "$board:green:wan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "$board:green:wlan5g" "phy0tpt"

	case "$board" in
	archer-c59-v1)
		ucidef_set_led_usbdev "usb" "USB" "$board:green:usb" "1-1"
		;;
	esac
	;;
archer-c7-v4)
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "$board:green:wlan5g" "phy0tpt"
	ucidef_set_led_switch "wan" "WAN" "$board:green:wan" "switch0" "0x02"
	ucidef_set_led_switch "lan1" "LAN1" "$board:green:lan4" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "$board:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "$board:green:lan2" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "$board:green:lan1" "switch0" "0x20"
	ucidef_set_led_usbdev "usb1" "USB1" "$board:green:usb1" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "$board:green:usb2" "2-1"
	;;
arduino-yun)
	ucidef_set_led_wlan "wlan" "WLAN" "arduino:blue:wlan" "phy0tpt"
	ucidef_set_led_usbdev "usb" "USB" "arduino:white:usb" "1-1.1"
	;;
bhr-4grv2)
	ucidef_set_led_default "power" "POWER" "buffalo:green:power" "1"
	ucidef_set_led_default "diag" "DIAG" "buffalo:red:diag" "0"
	;;
bsb)
	ucidef_set_led_default "sys" "SYS" "$board:red:sys" "1"
	;;
bullet-m|\
loco-m-xw|\
nanostation-m|\
nanostation-m-xw|\
rocket-m|\
rocket-m-xw)
	ucidef_set_led_rssi "rssilow" "RSSILOW" "ubnt:red:link1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "ubnt:orange:link2" "wlan0" "26" "100" "-25" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "ubnt:green:link3" "wlan0" "51" "100" "-50" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "ubnt:green:link4" "wlan0" "76" "100" "-75" "13"
	;;
bxu2000n-2-a1)
	ucidef_set_led_wlan "wlan" "WLAN" "bhu:green:wlan" "phy0tpt"
	;;
cap324)
	ucidef_set_led_netdev "lan" "LAN" "pcs:green:lan" "eth0"
	ucidef_set_led_wlan "wlan_amber" "WLAN_AMBER" "pcs:amber:wlan" "phy0tpt"
	ucidef_set_led_wlan "wlan_green" "WLAN_GREEN" "pcs:green:wlan" "phy1tpt"
	;;
c-55)
	ucidef_set_led_netdev "lan_green" "LAN_GREEN" "$board:green:lan" "eth0"
	ucidef_set_led_wlan "wlan_amber" "WLAN_AMBER" "$board:amber:wlan" "phy0tpt"
	ucidef_set_led_wlan "wlan_green" "WLAN_GREEN" "$board:green:wlan" "phy1tpt"
	;;
c-60)
	ucidef_set_led_wlan "wlan1_green" "WLAN1_GREEN" "$board:green:wlan1" "phy0tpt"
	ucidef_set_led_wlan "wlan2_green" "WLAN2_GREEN" "$board:green:wlan2" "phy1tpt"
	;;
cap4200ag)
	ucidef_set_led_default "lan_green" "LAN_GREEN" "senao:green:lan" "1"
	ucidef_set_led_wlan "wlan_amber" "WLAN_AMBER" "senao:amber:wlan" "phy0tpt"
	ucidef_set_led_wlan "wlan_green" "WLAN_GREEN" "senao:green:wlan" "phy1tpt"
	;;
carambola2)
	ucidef_set_led_netdev "lan" "LAN" "$board:orange:eth0" "eth0"
	ucidef_set_led_netdev "wan" "WAN" "$board:orange:eth1" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"
	;;
cf-e316n-v2)
	ucidef_set_led_netdev "lan" "LAN" "$board:blue:lan" "eth0"
	ucidef_set_led_netdev "wan" "WAN" "$board:blue:wan" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:blue:wlan" "phy0tpt"
	;;
cf-e320n-v2)
	ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth0"
	ucidef_set_led_netdev "wan" "WAN" "$board:red:wan" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:blue:wlan" "phy0tpt"
	;;
cf-e355ac-v1|\
cf-e355ac-v2|\
cf-e375ac|\
cf-e380ac-v1|\
cf-e380ac-v2|\
cf-e385ac)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "$board:blue:wlan2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "$board:red:wlan5g" "phy0tpt"

	case "$board" in
	cf-e375ac|\
	cf-e385ac)
		ucidef_set_led_switch "lan" "LAN" "$board:green:lan" "switch0" "0x04"
		;;
	*)
		ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth0"
		;;
	esac
	;;
cf-e520n|\
cf-e530n)
	ucidef_set_led_netdev "wan" "WAN" "$board:blue:wan" "eth1"
	;;
cpe210|\
cpe510|\
wbs210|\
wbs510)
	ucidef_set_led_switch "lan0" "LAN0" "tp-link:green:lan0" "switch0" "0x20"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x10"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "tp-link:green:link1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "tp-link:green:link2" "wlan0" "26" "100" "-25" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "tp-link:green:link3" "wlan0" "51" "100" "-50" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "tp-link:green:link4" "wlan0" "76" "100" "-75" "13"
	;;
cr3000)
	ucidef_set_led_netdev "wan" "WAN" "pcs:blue:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "pcs:blue:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "pcs:blue:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "pcs:blue:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "pcs:blue:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "pcs:blue:wlan" "phy0tpt"
	;;
cr5000)
	ucidef_set_led_wlan "wlan" "WLAN" "pcs:blue:wlan" "phy0tpt"
	ucidef_set_led_usbdev "usb" "USB" "pcs:white:wps" "1-1"
	;;
db120)
	ucidef_set_led_usbdev "usb" "USB" "$board:green:usb" "1-1"
	;;
dr344)
	ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth1"
	;;
dragino2)
	ucidef_set_led_wlan "wlan" "WLAN" "$board:red:wlan" "phy0tpt"
	ucidef_set_led_netdev "lan" "LAN" "$board:red:lan" "eth0"
	ucidef_set_led_netdev "wan" "WAN" "$board:red:wan" "eth1"
	;;
dw33d)
	ucidef_set_led_usbdev "mmc" "MMC" "$board:blue:mmc" "1-1"
	ucidef_set_led_usbdev "usb" "USB" "$board:blue:usb" "2-1"
	ucidef_set_led_netdev "internet" "INTERNET" "$board:blue:internet" "eth0"
	ucidef_set_led_wlan "wlan2g" "WLAN-2.4G" "$board:blue:wlan-2g" "phy1tpt"
	;;
eap300v2)
	ucidef_set_led_netdev "lan" "LAN" "engenius:blue:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "engenius:blue:wlan" "phy0tpt"
	;;
ens202ext)
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "engenius:amber:wlan1" "wlan0" "1"  "100" "0" "13"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "engenius:red:wlan2" "wlan0" "25" "100" "-39" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "engenius:amber:wlan3" "wlan0" "50" "100" "-59" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "engenius:green:wlan4" "wlan0" "75" "100" "-79" "13"
	;;
f9k1115v2)
	ucidef_set_led_usbdev "usb2" "USB2" "belkin:green:usb2" "1-1"
	;;
fritz300e)
	ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "$board:green:rssi0" "wlan0" "1" "100"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "$board:green:rssi1" "wlan0" "20" "100"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "$board:green:rssi2" "wlan0" "40" "100"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "$board:green:rssi3" "wlan0" "60" "100"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "$board:green:rssi4" "wlan0" "80" "100"
	;;
dap-1330-a1)
	ucidef_set_rssimon "wlan0" "2000000" "2"
	ucidef_set_led_rssi "wifi-low" "wifi-low" "d-link:red:wifi" "wlan0" "1" "29"
	ucidef_set_led_rssi "wifi-medium" "wifi-medium" "d-link:green:wifi" "wlan0" "30" "100"
	ucidef_set_led_rssi "wifi-high" "wifi-high" "d-link:green:signal1" "wlan0" "50" "100"
	ucidef_set_led_rssi "wifi-max" "wifi-max" "d-link:green:signal2" "wlan0" "70" "100"
	;;
dap-2695-a1)
	ucidef_set_led_default "power" "POWER" "d-link:green:power" "1"
	ucidef_set_led_default "diag" "DIAG" "d-link:red:power" "0"
	ucidef_set_led_wlan "wlan2g" "WLAN 2.4 GHz" "d-link:green:wlan2g" "phy1tpt"
	;;
dhp-1565-a1)
	ucidef_set_led_switch "wan" "WAN" "d-link:green:planet" "switch0" "0x20"
	;;
dir-600-a1|\
dir-615-e1|\
dir-615-e4|\
ebr-2310-c1)
	ucidef_set_led_netdev "wan" "WAN" "d-link:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "d-link:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "d-link:green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "d-link:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "d-link:green:lan4" "switch0" "0x10"
	;;
dir-615-c1)
	ucidef_set_led_netdev "wan" "WAN" "d-link:green:wan" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "d-link:green:wlan" "phy0tpt"
	;;
dir-825-b1|\
dir-825-c1)
	ucidef_set_led_usbdev "usb" "USB" "d-link:blue:usb" "1-1"

	case "$board" in
	dir-825-c1)
		ucidef_set_led_wlan "wlan2g" "WLAN 2.4 GHz" "d-link:blue:wlan2g" "phy0tpt"
		;;
	esac
	;;
dir-615-i1)
	ucidef_set_led_default "power" "POWER" "d-link:green:power" "1"
	ucidef_set_led_default "diag" "DIAG" "d-link:amber:power" "0"
	ucidef_set_led_default "wps" "WPS" "d-link:blue:wps" "0"
	ucidef_set_led_netdev "wan" "WAN" "d-link:green:wan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "d-link:green:wlan" "phy0tpt"
	;;
dlan-hotspot)
	ucidef_set_led_wlan "wlan" "WLAN" "devolo:green:wifi" "phy0tpt"
	;;
dlan-pro-500-wp)
	ucidef_set_led_default "power" "System Power" "devolo:green:status" "1"
	ucidef_set_led_netdev "lan" "Ethernet Activity" "devolo:green:eth" "br-lan"
	ucidef_set_led_wlan "wlan2g" "WLAN 2.4 GHz" "devolo:green:wlan-2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN 5 GHz" "devolo:blue:wlan-5g" "none"
	;;
dlan-pro-1200-ac)
	ucidef_set_led_wlan "wlan" "WLAN" "devolo:status:wlan" "phy0radio"
	ucidef_set_led_gpio "plcw" "dLAN" "devolo:status:dlan" "17" "0"
	ucidef_set_led_gpio "plcr" "dLAN" "devolo:error:dlan" "16" "0"
	;;
e1700ac-v2)
	ucidef_set_led_usbdev "usb" "USB" "$board:green:usb" "1-1"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "$board:green:wlan2g" "phy1tpt"
	;;
esr900)
	ucidef_set_led_wlan "wlan2g" "WLAN 2.4 GHz" "engenius:blue:wlan-2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN 5 GHz" "engenius:blue:wlan-5g" "phy1tpt"
	;;
esr1750|\
epg5000)
	ucidef_set_led_wlan "wlan2g" "WLAN 2.4 GHz" "$board:blue:wlan-2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN 5 GHz" "$board:blue:wlan-5g" "phy0tpt"
	;;
fritz4020)
	ucidef_set_led_default "power" "Power" "$board:green:power" "1"
	ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth1"
	ucidef_set_led_netdev "wan" "WAN" "$board:green:wan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"
	;;
gl-ar300m)
	ucidef_set_led_wlan "wlan" "WLAN" "$board:red:wlan" "phy0tpt"
	;;
gl-ar750)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "$board:white:wlan2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "$board:white:wlan5g" "phy0tpt"
	;;
gl-ar750s)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "$board:green:wlan2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "$board:green:wlan5g" "phy0tpt"
	;;
gl-mifi)
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"
	ucidef_set_led_netdev "wan" "WAN" "$board:green:wan" "eth0"
	ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth1"
	ucidef_set_led_netdev "3gnet" "3GNET" "$board:green:net" "3g-wan"
	;;
gl-ar150)
	ucidef_set_led_wlan "wlan" "WLAN" "$board:orange:wlan" "phy0tpt"
	ucidef_set_led_netdev "wan" "WAN" "$board:green:wan" "eth0"
	ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth1"
	;;
gl-ar300)
	ucidef_set_led_wlan "wlan" "WLAN" "$board:wlan" "phy0tpt"
	;;
gl-domino|\
sc300m|\
wrt160nl)
	ucidef_set_led_wlan "wlan" "WLAN" "$board:blue:wlan" "phy0tpt"
	;;
gl-inet)
	ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:red:wlan" "phy0tpt"
	;;
hiwifi-hc6361)
	ucidef_set_led_netdev "inet" "INET" "hiwifi:blue:internet" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "hiwifi:blue:wlan-2p4" "phy0tpt"
	;;
hornet-ub|\
hornet-ub-x2)
	ucidef_set_led_netdev "lan" "LAN" "alfa:blue:lan" "eth0"
	ucidef_set_led_netdev "wan" "WAN" "alfa:blue:wan" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "alfa:blue:wlan" "phy0tpt"
	ucidef_set_led_usbdev "usb" "USB" "alfa:blue:usb" "1-1"
	;;
koala)
	ucidef_set_led_default "power" "POWER" "$board:green:power" "1"
	ucidef_set_led_wlan "wlan2g" "WLAN 2.4GHz" "$board:yellow:wlan2" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN 5GHz" "$board:red:wlan58" "phy0tpt"
	;;
lan-turtle)
	ucidef_set_led_netdev "wan" "WAN" "$board:orange:system" "eth1"
	;;
lbe-m5)
	ucidef_set_led_netdev "lan" "LAN" "ubnt:green:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "ubnt:green:wlan" "phy0tpt"
	;;
mc-mac1200r)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "mercury:green:wlan2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "mercury:green:wlan5g" "phy0tpt"
	;;
mr12|\
mr16)
	ucidef_set_led_netdev "wan" "WAN" "$board:green:wan" "eth0"
	ucidef_set_led_wlan "wlan1" "WLAN1" "$board:green:wifi1" "phy0assoc"
	ucidef_set_led_wlan "wlan2" "WLAN2" "$board:green:wifi2" "phy0assoc"
	ucidef_set_led_wlan "wlan3" "WLAN3" "$board:green:wifi3" "phy0assoc"
	ucidef_set_led_wlan "wlan4" "WLAN4" "$board:green:wifi4" "phy0tpt"
	;;
mr18)
	ucidef_set_led_netdev "wlan0" "WLAN0" "$board:blue:tricolor0" "wlan0"
	;;
mr600)
	ucidef_set_led_wlan "wlan58" "WLAN58" "$board:green:wlan58" "phy0tpt"
	ucidef_set_led_default "wps" "WPS" "mr600:blue:wps" "0"
	;;
mr600v2)
	ucidef_set_led_default "wlan24-red" "WLAN 2.4GHz (red)" "mr600:red:wlan24" "0"
	ucidef_set_led_default "wlan24-yellow" "WLAN 2.4GHz (yellow)" "mr600:yellow:wlan24" "0"
	ucidef_set_led_wlan "wlan24-green" "WLAN 4GHz (green)" "mr600:green:wlan24" "phy1tpt"
	ucidef_set_led_default "wlan5-red" "WLAN 5GHz (red)" "mr600:red:wlan58" "0"
	ucidef_set_led_default "wlan5-yellow" "WLAN 5GHz (yellow)" "mr600:yellow:wlan58" "0"
	ucidef_set_led_wlan "wlan5-green" "WLAN 5GHz (green)" "mr600:green:wlan58" "phy0tpt"
	;;
mr1750|\
mr1750v2)
	ucidef_set_led_netdev "lan" "LAN" "mr1750:blue:wan" "eth0"
	ucidef_set_led_wlan "wlan58" "WLAN58" "mr1750:blue:wlan58" "phy0tpt"
	ucidef_set_led_wlan "wlan24" "WLAN24" "mr1750:blue:wlan24" "phy1tpt"
	ucidef_set_led_default "status-red" "Status (red)" "mr1750:red:wifi" "0"
	ucidef_set_led_default "status-green" "Status (green)" "mr1750:green:wifi" "0"
	;;
mr900|\
mr900v2)
	ucidef_set_led_netdev "lan" "LAN" "mr900:blue:wan" "eth0"
	ucidef_set_led_wlan "wlan24" "WLAN24" "mr900:blue:wlan24" "phy0tpt"
	ucidef_set_led_wlan "wlan58" "WLAN58" "mr900:blue:wlan58" "phy1tpt"
	ucidef_set_led_default "status-red" "Status (red)" "mr900:red:wifi" "0"
	ucidef_set_led_default "status-green" "Status (green)" "mr900:green:wifi" "0"
	;;
mynet-n600)
	ucidef_set_led_netdev "wan" "WAN" "wd:blue:internet" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "wd:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "wd:green:lan2" "switch0" "0x10"
	ucidef_set_led_switch "lan3" "LAN3" "wd:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "wd:green:lan4" "switch0" "0x04"
	;;
mynet-rext)
	ucidef_set_led_netdev "lan" "LAN" "wd:blue:ethernet" "eth0"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "wd:blue:quality1" "wlan0" "1" "40" "0" "6"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "wd:blue:quality2" "wlan0" "30" "80" "-29" "5"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "wd:blue:quality3" "wlan0" "70" "100" "-69" "8"
	ucidef_set_led_wlan "wlan" "WLAN" "wd:blue:wireless" "phy0tpt"
	;;
mzk-w04u)
	ucidef_set_led_usbdev "usb" "USB" "planex:green:usb" "1-1"
	;;
mzk-w300nh)
	ucidef_set_led_wlan "wlan" "WLAN" "planex:green:wlan" "phy0tpt"
	;;
nbg460n_550n_550nh)
	ucidef_set_led_wlan "wlan" "WLAN" "nbg460n:green:wlan" "phy0tpt"
	;;
nbg6616)
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wifi2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5" "WLAN5" "$board:green:wifi5g" "phy0tpt"
	ucidef_set_led_usbdev "usb1" "USB1" "$board:green:usb1" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "$board:green:usb2" "2-1"
	;;
nbg6716)
	ucidef_set_led_netdev "wan" "WAN" "$board:white:internet" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:white:wifi2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5" "WLAN5" "$board:white:wifi5g" "phy0tpt"
	ucidef_set_led_usbdev "usb1" "USB1" "$board:white:usb1" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "$board:white:usb2" "2-1"
	;;
om2p|\
om2p-hs|\
om2p-hsv2|\
om2p-hsv3|\
om2p-hsv4|\
om2p-lc|\
om2pv2|\
om2pv4)
	ucidef_set_led_netdev "port1" "port1" "om2p:blue:wan" "eth0"
	ucidef_set_led_netdev "port2" "port2" "om2p:blue:lan" "eth1"
	ucidef_set_led_default "wlan-red" "WLAN (red)" "om2p:red:wifi" "0"
	ucidef_set_led_default "wlan-yellow" "WLAN (yellow)" "om2p:yellow:wifi" "0"
	ucidef_set_led_default "wlan-green" "WLAN (green)" "om2p:green:wifi" "0"
	;;
om5p|\
om5p-an)
	ucidef_set_led_netdev "port1" "port1" "om5p:blue:wan" "eth0"
	ucidef_set_led_netdev "port2" "port2" "om5p:blue:lan" "eth1"
	ucidef_set_led_default "wlan-red" "WLAN (red)" "om5p:red:wifi" "0"
	ucidef_set_led_default "wlan-yellow" "WLAN (yellow)" "om5p:yellow:wifi" "0"
	ucidef_set_led_default "wlan-green" "WLAN (green)" "om5p:green:wifi" "0"
	;;
om5p-ac)
	ucidef_set_led_netdev "port1" "port1" "om5pac:blue:lan" "eth0"
	ucidef_set_led_netdev "port2" "port2" "om5pac:blue:wan" "eth1"
	ucidef_set_led_default "wlan-red" "WLAN (red)" "om5pac:red:wifi" "0"
	ucidef_set_led_default "wlan-yellow" "WLAN (yellow)" "om5pac:yellow:wifi" "0"
	ucidef_set_led_default "wlan-green" "WLAN (green)" "om5pac:green:wifi" "0"
	;;
om5p-acv2)
	ucidef_set_led_default "wlan-red" "WLAN (red)" "om5pac:red:wifi" "0"
	ucidef_set_led_default "wlan-yellow" "WLAN (yellow)" "om5pac:yellow:wifi" "0"
	ucidef_set_led_default "wlan-green" "WLAN (green)" "om5pac:green:wifi" "0"
	;;
omy-g1)
	ucidef_set_led_wlan "wlan" "WLAN" "omy:green:wlan" "phy0tpt"
	ucidef_set_led_netdev "wan" "WAN" "omy:green:wan" "eth0"
	ucidef_set_led_netdev "lan" "LAN" "omy:green:lan" "eth1"
	;;
omy-x1)
	ucidef_set_led_default "power" "POWER" "omy:green:power" "1"
	ucidef_set_led_default "wan" "WAN" "omy:green:wan" "eth0"
	;;
pqi-air-pen)
	ucidef_set_led_wlan "wlan" "WLAN" "pqi-air-pen:blue:wlan" "phy0tpt"
	ucidef_set_led_default "wps" "WPS" "pqi-air-pen:blue:wps" "0"
	;;
qihoo-c301)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "qihoo:red:status" "phy1tpt"
	;;
r36a)
	ucidef_set_led_netdev "lan" "LAN" "$board:blue:lan" "eth0"
	ucidef_set_led_usbdev "usb" "USB" "$board:blue:usb" "1-1"
	ucidef_set_led_netdev "wan" "WAN" "$board:blue:wan" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:blue:wlan" "phy0tpt"
	;;
r602n|\
t830|\
zbt-we1526)
	ucidef_set_led_netdev "wan" "WAN" "$board:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "$board:green:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "$board:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "$board:green:lan3" "switch0" "0x04"
	ucidef_set_led_switch "lan4" "LAN4" "$board:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"

	case "$board" in
	t830)
		ucidef_set_led_usbdev "usb" "USB" "$board:green:usb" "1-1"
		;;
	esac
	;;
r6100)
	ucidef_set_led_netdev "wan" "WAN (green)" "netgear:green:wan" "eth0"
	ucidef_set_led_usbdev "usb" "USB" "netgear:blue:usb" "1-1"
	ucidef_set_led_wlan "wlan" "WLAN" "netgear:blue:wlan" "phy1tpt"
	;;
rb-750)
	ucidef_set_led_default "act" "act" "rb750:green:act" "1"
	ucidef_set_led_netdev "port1" "port1" "rb750:green:port1" "eth1"
	ucidef_set_led_switch "port2" "port2" "rb750:green:port2" "switch0" "0x10"
	ucidef_set_led_switch "port3" "port3" "rb750:green:port3" "switch0" "0x08"
	ucidef_set_led_switch "port4" "port4" "rb750:green:port4" "switch0" "0x04"
	ucidef_set_led_switch "port5" "port5" "rb750:green:port5" "switch0" "0x02"
	;;
rb-750-r2|\
rb-750p-pbr2|\
rb-750up-r2)
	ucidef_set_led_timer "user" "USER" "rb:green:user" "1000" "1000"
	ucidef_set_led_netdev "port1" "port1" "rb:green:port1" "eth0"
	ucidef_set_led_switch "port2" "port2" "rb:green:port2" "switch0" "0x10"
	ucidef_set_led_switch "port3" "port2" "rb:green:port3" "switch0" "0x08"
	ucidef_set_led_switch "port4" "port3" "rb:green:port4" "switch0" "0x04"
	ucidef_set_led_switch "port5" "port5" "rb:green:port5" "switch0" "0x02"
	;;
rb-911-2hn|\
rb-911-5hn)
	ucidef_set_led_netdev "eth" "ETH" "rb:green:eth" "eth0"
	;;
rb-941-2nd)
	ucidef_set_led_timer "user" "USR/ACT" "rb:green:user" "1000" "1000"
	;;
rb-951ui-2nd|\
rb-952ui-5ac2nd)
	ucidef_set_led_timer "user" "USER" "rb:green:user" "1000" "1000"
	ucidef_set_led_netdev "port1" "port1" "rb:green:port1" "eth0"
	ucidef_set_led_switch "port2" "port2" "rb:green:port2" "switch0" "0x10"
	ucidef_set_led_switch "port3" "port2" "rb:green:port3" "switch0" "0x08"
	ucidef_set_led_switch "port4" "port3" "rb:green:port4" "switch0" "0x04"
	ucidef_set_led_switch "port5" "port5" "rb:green:port5" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "rb:blue:wlan" "phy0tpt"
	;;
rb-962uigs-5hact2hnt)
	ucidef_set_led_timer "user" "USER/SFP" "rb:green:user" "1000" "1000"
	;;
rb-2011il|\
rb-2011ils|\
rb-2011l|\
rb-2011uas|\
rb-2011uas-2hnd|\
rb-2011uias|\
rb-2011uias-2hnd)
	ucidef_set_led_switch "eth6" "ETH6" "rb:green:eth6" "switch1" "0x20"
	ucidef_set_led_switch "eth7" "ETH7" "rb:green:eth7" "switch1" "0x10"
	ucidef_set_led_switch "eth8" "ETH8" "rb:green:eth8" "switch1" "0x08"
	ucidef_set_led_switch "eth9" "ETH9" "rb:green:eth9" "switch1" "0x04"
	ucidef_set_led_switch "eth10" "ETH10" "rb:green:eth10" "switch1" "0x02"
	;;
rb-lhg-5nd)
	ucidef_set_led_netdev "lan" "LAN" "rb:green:eth" "eth0"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "rb:green:rssi0" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "rb:green:rssi1" "wlan0" "20" "100" "-19" "13"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "rb:green:rssi2" "wlan0" "40" "100" "-39" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "rb:green:rssi3" "wlan0" "60" "100" "-59" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "rb:green:rssi4" "wlan0" "80" "100" "-79" "13"
	;;
rb-map-2nd)
	ucidef_set_led_switch "eth1" "WAN" "rb:green:eth1" "switch0" "0x02"
	ucidef_set_led_switch "eth2" "LAN" "rb:green:eth2" "switch0" "0x04"
	ucidef_set_led_gpio "poe" "POE" "rb:red:poe_out" "14" "0"
	ucidef_set_led_wlan "wlan" "WLAN" "rb:green:wlan" "phy0tpt"
	;;
rb-mapl-2nd)
	ucidef_set_led_default "power" "POWER" "rb:green:power" "1"
	ucidef_set_led_netdev "lan" "LAN" "rb:green:eth" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "rb:green:wlan" "phy0tpt"
	;;
rb-wap-2nd)
	ucidef_set_led_timer "user" "USER" "rb:green:user" "1000" "1000"
	ucidef_set_led_wlan "wlan" "WLAN" "rb:green:wlan" "phy0tpt"
	;;
re355|\
re450)
	ucidef_set_led_netdev "lan_data" "LAN Data" "$board:green:lan_data" "eth0" "tx rx"
	ucidef_set_led_netdev "lan_link" "LAN Link" "$board:green:lan_link" "eth0" "link"
	ucidef_set_led_wlan "wlan2g" "WLAN 2.4 GHz" "$board:blue:wlan2g" "phy1tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN 5 GHz" "$board:blue:wlan5g" "phy0tpt"
	;;
rme-eg200)
        ucidef_set_led_netdev "wan" "WAN" "eg200:red:eth0" "eth0"
        ucidef_set_led_wlan "wlan" "WLAN" "eg200:red:wlan" "phy0tpt"
        ucidef_set_led_oneshot "modbus" "Modbus" "eg200:red:modbus" "100" "33"
        ucidef_set_led_default "etactica" "etactica" "eg200:red:etactica" "ignore"
        ;;
rocket-m-ti)
	ucidef_set_led_rssi "rssiverylow" "RSSIVERYLOW" "ubnt:green:link1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "ubnt:green:link2" "wlan0" "26" "100" "-25" "13"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "ubnt:green:link3" "wlan0" "51" "100" "-50" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "ubnt:green:link4" "wlan0" "76" "100" "-75" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "ubnt:green:link5" "wlan0" "76" "100" "-75" "13"
	ucidef_set_led_rssi "rssiveryhigh" "RSSIVERYHIGH" "ubnt:green:link4" "wlan0" "76" "100" "-75" "13"
	;;
rut900)
	ucidef_set_led_netdev "wan" "WAN" "$board:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "$board:green:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "$board:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "$board:green:lan3" "switch0" "0x04"
	;;
smart-300)
	ucidef_set_led_netdev "wan" "WAN" "nc-link:green:wan" "eth0"
	ucidef_set_led_switch "lan1" "LAN1" "nc-link:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "nc-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "nc-link:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "nc-link:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "nc-link:green:wlan" "phy0tpt"
	;;
som9331)
	ucidef_set_led_netdev "wan" "WAN" "$board:orange:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "$board:orange:lan1" "switch0" "0x08"
	ucidef_set_led_switch "lan2" "LAN2" "$board:orange:lan2" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:red:wlan" "phy0tpt"
	ucidef_set_led_usbdev "usb" "USB" "$board:green:system" "1-1"
	;;
sr3200)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "$board:green:wlan2g" "phy1tpt"
	;;
tellstick-znet-lite)
	ucidef_set_led_netdev "lan_act" "LANACT" "tellstick:green:lan" "eth0" "tx rx"
	ucidef_set_led_netdev "lan_link" "LANLINK" "tellstick:orange:lan" "eth0" "link"
	;;
tew-712br)
	ucidef_set_led_netdev "wan" "WAN" "trendnet:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "trendnet:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "trendnet:green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "trendnet:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "trendnet:green:lan4" "switch0" "0x10"
	ucidef_set_led_wlan "wlan" "WLAN" "trendnet:green:wlan" "phy0tpt"
	;;
tew-732br)
	ucidef_set_led_netdev "wan" "WAN" "trendnet:green:wan" "eth1"
	;;
tew-823dru)
	ucidef_set_led_netdev "wan" "WAN" "trendnet:green:planet" "eth0"
	;;
tl-mr11u|\
tl-mr3020|\
tl-mr3040|\
tl-mr3040-v2)
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:3g" "1-1"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth0"
	;;
tl-mr3220|\
tl-mr3420)
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:3g" "1-1"
	;;
tl-mr3220-v2|\
tl-wr741nd-v4)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"

	case "$board" in
	tl-mr3220-v2)
		ucidef_set_led_usbdev "usb" "USB" "tp-link:green:3g" "1-1"
		;;
	esac
	;;
tl-mr3420-v2|\
tl-wr841n-v8|\
tl-wr842n-v2|\
tl-wr941nd-v5)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth0"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"

	case "$board" in
	tl-mr3420-v2|\
	tl-wr842n-v2)
		ucidef_set_led_usbdev "usb" "USB" "tp-link:green:3g" "1-1"
		;;
	esac
	;;
tl-mr6400)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:white:lan" "eth0"
	ucidef_set_led_netdev "wan" "WAN" "tp-link:white:wan" "eth1"
	ucidef_set_led_netdev "4g" "4G" "tp-link:white:4g" "usb0"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:white:wlan" "phy0tpt"
	;;
tl-wa7210n-v2)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth0"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "tp-link:green:signal1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "tp-link:green:signal2" "wlan0" "26" "100" "-25" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "tp-link:green:signal3" "wlan0" "51" "100" "-50" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "tp-link:green:signal4" "wlan0" "76" "100" "-75" "13"
	;;
tl-wa750re)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:orange:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:orange:wlan" "phy0tpt"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "tp-link:orange:signal1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "tp-link:orange:signal2" "wlan0" "20" "100" "-19" "13"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "tp-link:orange:signal3" "wlan0" "40" "100" "-39" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "tp-link:orange:signal4" "wlan0" "60" "100" "-59" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "tp-link:orange:signal5" "wlan0" "80" "100" "-79" "13"
	;;
tl-wa801nd-v3)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth1"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;
tl-wa850re|\
tl-wa850re-v2)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:blue:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:blue:wlan" "phy0tpt"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "tp-link:blue:signal1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "rssimediumlow" "RSSIMEDIUMLOW" "tp-link:blue:signal2" "wlan0" "20" "100" "-19" "13"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "tp-link:blue:signal3" "wlan0" "40" "100" "-39" "13"
	ucidef_set_led_rssi "rssimediumhigh" "RSSIMEDIUMHIGH" "tp-link:blue:signal4" "wlan0" "60" "100" "-59" "13"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "tp-link:blue:signal5" "wlan0" "80" "100" "-79" "13"
	;;
tl-wa701nd-v2|\
tl-wa801nd-v2|\
tl-wa830re-v2|\
tl-wa860re|\
tl-wa901nd-v3|\
tl-wa901nd-v4|\
tl-wa901nd-v5)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;
tl-wa901nd)
	ucidef_set_led_netdev "lan" "LAN" "tp-link:green:lan" "eth0"
	;;
tl-wa901nd-v2|\
tl-wr941nd|\
tl-wr1041n-v2)
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;
tl-wdr3320-v2)
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "tp-link:green:wlan5g" "phy0tpt"
	;;
tl-wdr3500)
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:usb" "1-1"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "tp-link:green:wlan2g" "phy0tpt"
	;;
tl-wdr4300)
	ucidef_set_led_usbdev "usb1" "USB1" "tp-link:green:usb1" "1-1.1"
	ucidef_set_led_usbdev "usb2" "USB2" "tp-link:green:usb2" "1-1.2"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "tp-link:blue:wlan2g" "phy0tpt"
	;;
tl-wdr4900-v2)
	ucidef_set_led_usbdev "usb1" "USB1" "tp-link:green:usb1" "1-1"
	ucidef_set_led_usbdev "usb2" "USB2" "tp-link:green:usb2" "2-1"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "tp-link:blue:wlan2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "tp-link:blue:wlan5g" "phy1tpt"
	;;
tl-wdr6500-v2|\
tl-wr741nd)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x10"
	;;
tl-wpa8630)
	ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth0"
	ucidef_set_led_netdev "wlan" "WLAN" "$board:green:wlan" "wlan1"
	ucidef_set_led_netdev "wlan5" "WLAN5" "$board:green:wlan5" "wlan0"
	;;
tl-wr740n-v6|\
tl-wr841n-v9|\
tl-wr841n-v11|\
tl-wr842n-v3)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x04"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"

	case "$board" in
	tl-wr842n-v3)
		ucidef_set_led_usbdev "usb" "USB" "tp-link:green:3g" "1-1"
		;;
	esac
	;;
tl-wr802n-v1)
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:blue:system" "phy0tpt"
	;;
tl-wr802n-v2)
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:system" "phy0tpt"
	;;
tl-wr902ac-v1)
	ucidef_set_led_netdev "lan" "LAN" "$board:green:lan" "eth0"
	ucidef_set_led_usbdev "usb" "USB" "$board:green:usb" "1-1"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "$board:green:wlan2g" "phy1tpt"
	;;
tl-wr940n-v4|\
tl-wr941nd-v6)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:blue:wan" "eth0"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:blue:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:blue:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:blue:lan3" "switch0" "0x04"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:blue:lan4" "switch0" "0x02"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:blue:wlan" "phy0tpt"
	;;
tl-wr840n-v2|\
tl-wr840n-v3)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:green:wan" "eth1"
	ucidef_set_led_switch "lan" "LAN" "tp-link:green:lan" "switch0" "0x1E"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;
tl-wr940n-v6)
	ucidef_set_led_netdev "wan" "WAN" "tp-link:blue:wan" "eth0"
	;;
tl-wr942n-v1)
	ucidef_set_led_switch "lan1" "LAN1" "$board:green:lan1" "switch0" "0x04"
	ucidef_set_led_switch "lan2" "LAN2" "$board:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "$board:green:lan3" "switch0" "0x10"
	ucidef_set_led_switch "lan4" "LAN4" "$board:green:lan4" "switch0" "0x02"
	ucidef_set_led_netdev "wan" "WAN" "$board:green:wan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:green:wlan" "phy0tpt"
	ucidef_set_led_usbdev "usb1" "USB1" "$board:green:usb1" "1-1.2"
	ucidef_set_led_usbdev "usb2" "USB2" "$board:green:usb2" "1-1.1"
	;;
tl-wr1043nd|\
tl-wr1043nd-v2)
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:usb" "1-1"
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	;;
tl-wr1043n-v5|\
tl-wr1043nd-v4)
	ucidef_set_led_wlan "wlan" "WLAN" "tp-link:green:wlan" "phy0tpt"
	ucidef_set_led_switch "wan" "WAN" "tp-link:green:wan" "switch0" "0x20"
	ucidef_set_led_switch "lan1" "LAN1" "tp-link:green:lan1" "switch0" "0x10"
	ucidef_set_led_switch "lan2" "LAN2" "tp-link:green:lan2" "switch0" "0x08"
	ucidef_set_led_switch "lan3" "LAN3" "tp-link:green:lan3" "switch0" "0x04"
	ucidef_set_led_switch "lan4" "LAN4" "tp-link:green:lan4" "switch0" "0x02"

	case "$board" in
	tl-wr1043nd-v4)
		ucidef_set_led_usbdev "usb" "USB" "tp-link:green:usb" "1-1"
		;;
	esac
	;;
tl-wr2543n)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "tp-link:green:wlan2g" "phy0tpt"
	ucidef_set_led_usbdev "usb" "USB" "tp-link:green:usb" "1-1"
	;;
tube2h)
	ucidef_set_led_netdev "lan" "LAN" "alfa:blue:lan" "eth0"
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "signal1" "SIGNAL1" "alfa:red:signal1" "wlan0" "1" "100" "0" "13"
	ucidef_set_led_rssi "signal2" "SIGNAL2" "alfa:orange:signal2" "wlan0" "26" "100" "-25" "13"
	ucidef_set_led_rssi "signal3" "SIGNAL3" "alfa:green:signal3" "wlan0" "51" "100" "-50" "13"
	ucidef_set_led_rssi "signal4" "SIGNAL4" "alfa:green:signal4" "wlan0" "76" "100" "-75" "13"
	;;
wam250)
	ucidef_set_led_netdev "lan" "LAN" "$board:white:lan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "$board:white:wlan" "phy0tpt"
	;;
wndap360)
	ucidef_set_led_power "power" "POWER GREEN" "netgear:green:power" "1"
	;;
wndr3700)
	ucidef_set_led_default "wan" "WAN LED (green)" "netgear:green:wan" "0"
	ucidef_set_led_usbdev "usb" "USB" "netgear:green:usb" "1-1"
	;;
wi2a-ac200i)
	ucidef_set_led_default "power" "Power (green)" "nokia:green:power" "1"
	ucidef_set_led_default "wan" "Ethernet LED (green)" "nokia:green:wan" "1"
	ucidef_set_led_wlan "wlan5g" "WLAN" "nokia:green:wlan-5g" "phy0tpt"
	ucidef_set_led_wlan "wlan2g" "WLAN" "nokia:green:wlan-2g" "phy1tpt"
	;;
wndr3700v4|\
wndr4300)
	ucidef_set_led_switch "wan-green" "WAN (green)" "netgear:green:wan" "switch0" "0x20" "0x08"
	ucidef_set_led_switch "wan-amber" "WAN (amber)" "netgear:amber:wan" "switch0" "0x20" "0x06"
	ucidef_set_led_usbdev "usb" "USB" "netgear:green:usb" "1-1"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "netgear:green:wlan2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "netgear:blue:wlan5g" "phy1tpt"
	;;
whr-g301n|\
whr-hp-g300n|\
whr-hp-gn)
	ucidef_set_led_netdev "wan" "WAN" "buffalo:green:wan" "eth1"
	ucidef_set_led_switch "lan1" "LAN1" "buffalo:green:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "buffalo:green:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "buffalo:green:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "buffalo:green:lan4" "switch0" "0x10"
	;;
wifi-pineapple-nano)
	ucidef_set_led_wlan "wlan0" "WLAN0" "$board:blue:system" "phy0tpt"
	;;
wlae-ag300n)
	ucidef_set_led_netdev "wireless" "WIRELESS" "buffalo:green:wireless" "wlan0"
	;;
wnr1000-v2|\
wnr2000-v3)
	ucidef_set_led_netdev "wan-amber" "WAN (amber)" "netgear:amber:wan" "eth0"
	ucidef_set_led_default "wan-green" "WAN (green)" "netgear:green:wan" "0"
	ucidef_set_led_wlan "wlan" "WLAN" "netgear:blue:wlan" "phy0tpt"
	ucidef_set_led_switch "lan1green" "LAN1 (green)" "netgear:green:lan1" "switch0" "0x02" "0x04"
	ucidef_set_led_switch "lan2green" "LAN2 (green)" "netgear:green:lan2" "switch0" "0x04" "0x04"
	ucidef_set_led_switch "lan3green" "LAN3 (green)" "netgear:green:lan3" "switch0" "0x08" "0x04"
	ucidef_set_led_switch "lan4green" "LAN4 (green)" "netgear:green:lan4" "switch0" "0x10" "0x04"
	ucidef_set_led_switch "lan1amber" "LAN1 (amber)" "netgear:amber:lan1" "switch0" "0x02" "0x02"
	ucidef_set_led_switch "lan2amber" "LAN2 (amber)" "netgear:amber:lan2" "switch0" "0x04" "0x02"
	ucidef_set_led_switch "lan3amber" "LAN3 (amber)" "netgear:amber:lan3" "switch0" "0x08" "0x02"
	ucidef_set_led_switch "lan4amber" "LAN4 (amber)" "netgear:amber:lan4" "switch0" "0x10" "0x02"
	;;
wnr2000-v4)
	ucidef_set_led_netdev "wan" "WAN" "netgear:green:wan" "eth0"
	ucidef_set_led_netdev "wlan" "WLAN" "netgear:blue:wlan" "wlan0"
	ucidef_set_led_switch "lan1" "LAN1" "netgear:amber:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2" "LAN2" "netgear:amber:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3" "LAN3" "netgear:amber:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4" "LAN4" "netgear:amber:lan4" "switch0" "0x10"
	ucidef_set_led_usbdev "usb" "USB" "netgear:amber:status" "1-1"
	;;
wnr2200)
	ucidef_set_led_netdev "wan-amber" "WAN (amber)" "netgear:amber:wan" "eth0"
	ucidef_set_led_default "wan-green" "WAN (green)" "netgear:green:wan" "0"
	ucidef_set_led_wlan "wlan" "WLAN" "netgear:blue:wlan" "phy0tpt"
	ucidef_set_led_switch "lan1green" "LAN1 (green)" "netgear:green:lan1" "switch0" "0x02" "0x04"
	ucidef_set_led_switch "lan2green" "LAN2 (green)" "netgear:green:lan2" "switch0" "0x04" "0x04"
	ucidef_set_led_switch "lan3green" "LAN3 (green)" "netgear:green:lan3" "switch0" "0x08" "0x04"
	ucidef_set_led_switch "lan4green" "LAN4 (green)" "netgear:green:lan4" "switch0" "0x10" "0x04"
	ucidef_set_led_switch "lan1amber" "LAN1 (amber)" "netgear:amber:lan1" "switch0" "0x02" "0x02"
	ucidef_set_led_switch "lan2amber" "LAN2 (amber)" "netgear:amber:lan2" "switch0" "0x04" "0x02"
	ucidef_set_led_switch "lan3amber" "LAN3 (amber)" "netgear:amber:lan3" "switch0" "0x08" "0x02"
	ucidef_set_led_switch "lan4amber" "LAN4 (amber)" "netgear:amber:lan4" "switch0" "0x10" "0x02"
	ucidef_set_led_usbdev "usb" "USB" "netgear:green:usb" "1-1"
	;;
wnr612-v2)
	ucidef_set_led_netdev "wan" "WAN" "netgear:green:wan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "netgear:green:wlan" "phy0tpt"
	ucidef_set_led_switch "lan1" "LAN1" "netgear:green:lan1" "switch0" "0x02" "0x0f"
	ucidef_set_led_switch "lan2" "LAN2" "netgear:green:lan2" "switch0" "0x04" "0x0f"
	;;
wpn824n)
	ucidef_set_led_netdev "wan-amber" "WAN (amber)" "netgear:amber:wan" "eth0"
	ucidef_set_led_wlan "wlan" "WLAN" "netgear:blue:wlan" "phy0tpt"
	ucidef_set_led_switch "lan1amber" "LAN1 (amber)" "netgear:amber:lan1" "switch0" "0x02"
	ucidef_set_led_switch "lan2amber" "LAN2 (amber)" "netgear:amber:lan2" "switch0" "0x04"
	ucidef_set_led_switch "lan3amber" "LAN3 (amber)" "netgear:amber:lan3" "switch0" "0x08"
	ucidef_set_led_switch "lan4amber" "LAN4 (amber)" "netgear:amber:lan4" "switch0" "0x10"
	ucidef_set_led_default "lan1green" "LAN1 (green)" "netgear:green:lan1" "0"
	ucidef_set_led_default "lan2green" "LAN2 (green)" "netgear:green:lan2" "0"
	ucidef_set_led_default "lan3green" "LAN3 (green)" "netgear:green:lan3" "0"
	ucidef_set_led_default "lan4green" "LAN4 (green)" "netgear:green:lan4" "0"
	ucidef_set_led_default "wan-green" "WAN (green)" "netgear:green:wan" "0"
	ucidef_set_led_default "wps1" "WPS1" "netgear:blue:wps1" "0"
	ucidef_set_led_default "wps2" "WPS2" "netgear:blue:wps2" "0"
	ucidef_set_led_default "status" "STATUS" "netgear:amber:status" "0"
	ucidef_set_led_default "test" "TEST" "netgear:amber:test" "0"
	;;
wzr-hp-ag300h)
	ucidef_set_led_default "diag" "DIAG" "buffalo:red:diag" "0"
	ucidef_set_led_netdev "router" "ROUTER" "buffalo:green:router" "eth1"
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "buffalo:amber:band2g" "phy0tpt"
	ucidef_set_led_wlan "wlan5g" "WLAN5G" "buffalo:amber:band5g" "phy1tpt"
	ucidef_set_led_usbdev "usb" "USB" "buffalo:green:usb" "1-1"
	;;
wzr-hp-g300nh)
	ucidef_set_led_wlan "wlan" "Wireless" "buffalo:green:wireless" "phy0tpt"
	ucidef_set_led_netdev "router" "Router" "buffalo:green:router" "eth1"
	ucidef_set_led_usbdev "usb" "USB" "buffalo:blue:usb" "1-1"
	;;
wzr-hp-g300nh2|\
wzr-hp-g450h)
	ucidef_set_led_wlan "wlan" "Wireless" "buffalo:green:wireless" "phy0tpt"
	;;
xd3200)
	ucidef_set_led_wlan "wlan2g" "WLAN2G" "$board:blue:wlan2g" "phy1tpt"
	;;
z1)
	ucidef_set_led_netdev "wlan1" "WLAN1" "$board:blue:tricolor0" "wlan1"
	;;
zcn-1523h-2)
	ucidef_set_led_netdev "lan1" "lan1" "zcn-1523h:green:lan1" "eth0"
	;;
zcn-1523h-5)
	ucidef_set_led_netdev "lan1" "lan1" "zcn-1523h:green:lan1" "eth0"
	ucidef_set_led_netdev "lan2" "lan2" "zcn-1523h:green:lan2" "eth1"
	;;
esac

board_config_flush

exit 0
