From 76a4707de5e18dc32d9cb4e990686140c5664a15 Mon Sep 17 00:00:00 2001
From: Brian Norris <computersforpeace@gmail.com>
Date: Fri, 29 Jan 2016 11:25:35 -0800
Subject: [PATCH] mtd: spi-nor: add SPI_NOR_HAS_LOCK flag

We can't determine this purely by manufacturer type (see commit
67b9bcd36906 ("mtd: spi-nor: fix Spansion regressions (aliased with
Winbond)")), and it's not autodetectable by anything like SFDP. So make
a new flag for it.

Signed-off-by: Brian Norris <computersforpeace@gmail.com>
Reviewed-by: Ezequiel Garcia <ezequiel@vanguardiasur.com.ar>
Tested-by: Ezequiel Garcia <ezequiel@vanguardiasur.com.ar>
---
 drivers/mtd/spi-nor/spi-nor.c | 7 +++++--
 1 file changed, 5 insertions(+), 2 deletions(-)

--- a/drivers/mtd/spi-nor/spi-nor.c
+++ b/drivers/mtd/spi-nor/spi-nor.c
@@ -68,6 +68,7 @@ struct flash_info {
 #define	SPI_NOR_DUAL_READ	0x20    /* Flash supports Dual Read */
 #define	SPI_NOR_QUAD_READ	0x40    /* Flash supports Quad Read */
 #define	USE_FSR			0x80	/* use flag status register */
+#define	SPI_NOR_HAS_LOCK	0x100	/* Flash supports lock/unlock via SR */
 };
 
 #define JEDEC_MFR(info)	((info)->id[0])
@@ -1163,7 +1164,8 @@ int spi_nor_scan(struct spi_nor *nor, co
 
 	if (JEDEC_MFR(info) == SNOR_MFR_ATMEL ||
 	    JEDEC_MFR(info) == SNOR_MFR_INTEL ||
-	    JEDEC_MFR(info) == SNOR_MFR_SST) {
+	    JEDEC_MFR(info) == SNOR_MFR_SST ||
+	    info->flags & SPI_NOR_HAS_LOCK) {
 		write_enable(nor);
 		write_sr(nor, 0);
 	}
@@ -1179,7 +1181,8 @@ int spi_nor_scan(struct spi_nor *nor, co
 	mtd->_read = spi_nor_read;
 
 	/* NOR protection support for STmicro/Micron chips and similar */
-	if (JEDEC_MFR(info) == SNOR_MFR_MICRON) {
+	if (JEDEC_MFR(info) == SNOR_MFR_MICRON ||
+		info->flags & SPI_NOR_HAS_LOCK) {
 		nor->flash_lock = stm_lock;
 		nor->flash_unlock = stm_unlock;
 		nor->flash_is_locked = stm_is_locked;
