#!/bin/sh

. /lib/functions/uci-defaults.sh
. /lib/ramips.sh

set_usb_led() {
	ucidef_set_led_usbdev "usb" "USB" "${1}" "${2:-1-1}"
}

set_wifi_led() {
	ucidef_set_led_netdev "wifi_led" "wifi" "${1}" "${2:-wlan0}"
}


board=$(ramips_board_name)

board_config_update

case $board in
11acnas|\
all0239-3g|\
hw550-3g|\
mofi3500-3gn|\
sap-g3200u3|\
sk-wb8|\
w2914nsv2|\
wf-2881)
	set_usb_led "$board:green:usb"
	;;
3g150b|\
3g300m)
	set_usb_led "$board:blue:3g"
	;;
3g-6200n)
	set_wifi_led "$board:amber:wlan"
	set_usb_led "$board:blue:3g"
	;;
3g-6200nl|\
wnce2001)
	set_wifi_led "$board:green:wlan"
	;;
br-6475nd|\
mzk-w300nh2)
	set_wifi_led "$board:amber:wlan"
	;;
a5-v11|\
cs-qr10)
	ucidef_set_led_default "power" "POWER" "$board:red:power" "1"
	;;
ai-br100)
	ucidef_set_led_netdev "wan" "wan" "$board:blue:wan" "eth0.2"
	set_wifi_led "$board:blue:wlan"
	;;
air3gii)
	set_wifi_led "$board:green:wlan"
	set_usb_led "$board:green:mobile"
	;;
all0256n)
	ucidef_set_rssimon "wlan0" "200000" "1"
	ucidef_set_led_rssi "rssilow" "RSSILOW" "$board:green:rssilow" "wlan0" "1" "40" "0" "6"
	ucidef_set_led_rssi "rssimedium" "RSSIMEDIUM" "$board:green:rssimed" "wlan0" "30" "80" "-29" "5"
	ucidef_set_led_rssi "rssihigh" "RSSIHIGH" "$board:green:rssihigh" "wlan0" "70" "100" "-69" "8"
	set_wifi_led "rt2800pci-phy0::radio"
	;;
ar670w|\
ar725w|\
awapn2403)
	set_wifi_led "rt2800soc-phy0::radio"
	;;
asl26555)
	ucidef_set_led_default "power" "POWER" "$board:green:power" "1"
	ucidef_set_led_netdev "eth" "ETH" "$board:green:eth" "eth0"
	set_wifi_led "$board:green:wlan"
	set_usb_led "$board:green:3g"
	;;
bc2)
	set_usb_led "$board:blue:usb"
	;;
br-6425)
	set_wifi_led "$board:orange:wlan"
	;;
broadway)
	set_usb_led "$board:red:diskmounted"
	set_wifi_led "$board:red:wps_active"
	;;
c20i)
	ucidef_set_led_switch "lan" "lan" "$board:blue:lan" "switch0" "0x1e"
	ucidef_set_led_switch "wan" "wan" "$board:blue:wan" "switch0" "0x01"
	set_usb_led "$board:blue:usb" "2-1"
	ucidef_set_led_wlan "wlan" "wlan" "$board:blue:wlan" "phy0radio"
	;;
c50)
	ucidef_set_led_switch "lan" "lan" "$board:green:lan" "switch0" "0x1e"
	ucidef_set_led_switch "wan" "wan" "$board:green:wan" "switch0" "0x01"
	set_usb_led "$board:green:usb"
	ucidef_set_led_netdev "wlan2g" "wlan2g" "$board:green:wlan2g" wlan1
	set_wifi_led "$board:green:wlan5g"
	;;
cf-wr800n)
	ucidef_set_led_netdev "lan" "lan" "$board:white:ethernet" eth0.1
	set_wifi_led "$board:white:wifi"
	;;
cy-swr1100)
	ucidef_set_led_default "wps" "WPS" "$board:blue:wps" "0"
	set_usb_led "$board:blue:usb"
	;;
d105)
	ucidef_set_led_default "power" "POWER" "$board:red:power" "1"
	set_usb_led "$board:green:usb"
	;;
d240)
	set_wifi_led "$board:blue:wifi"
	set_usb_led "$board:blue:usb"
	;;
db-wrt01)
	ucidef_set_led_default "power" "power" "$board:orange:power" "1"
	;;
dch-m225)
	ucidef_set_led_default "power" "POWER" "$board:geeen:power" "1"
	ucidef_set_led_default "status" "STATUS" "$board:red:status" "0"
	;;
dcs-930l-b1)
	ucidef_set_led_default "power" "POWER" "$board:red:power" "1"
	ucidef_set_led_netdev "wifi" "WiFi" "$board:blue:wps"
	;;
dir-300-b1|\
dir-600-b1|\
dir-620-a1)
	ucidef_set_led_default "wan" "WAN LED (amber)" "$board:amber:wan" "1"
	set_wifi_led "rt2800pci-phy0::radio"
	;;
dir-300-b7|\
dir-320-b1|\
dir-610-a1|\
esr-9753|\
hlk-rm04|\
sl-r7205|\
v11st-fe|\
w306r-v20|\
wt1520)
	set_wifi_led "rt2800pci-phy0::radio"
	;;
dir-615-d|\
dir-615-h1)
	ucidef_set_led_default "status" "Status LED (amber)" "$board:amber:status" "0"
	set_wifi_led "rt2800pci-phy0::radio"
	;;
dir-620-d1|\
mzk-ex300np)
	set_wifi_led "$board:green:wifi"
	;;
dir-810l|\
mzk-750dhp|\
mzk-dp150n|\
vr500)
	ucidef_set_led_default "power" "power" "$board:green:power" "1"
	;;
dir-860l-b1)
	ucidef_set_led_netdev "wan" "wan" "$board:green:net" "eth0.2"
	;;
ex2700|\
wn3000rpv3)
	ucidef_set_led_default "power_r" "POWER (red)" "$board:red:power" "0"
	set_wifi_led "$board:green:router"
	;;
f5d8235-v1)
	ucidef_set_led_default "lan" "lan" "$board:blue:wired" "0"
	set_usb_led "$board:blue:storage"
	set_wifi_led "$board:blue:wireless"
	;;
f5d8235-v2)
	set_usb_led "$board:blue:storage"
	;;
fonera20n)
	set_usb_led "$board:orange:usb"
	set_wifi_led "$board:orange:wifi"
	;;
gb-pc1)
	ucidef_set_led_switch "lan1" "lan1" "$board:green:lan1" "switch0" "0x01"
	ucidef_set_led_switch "lan2" "lan2" "$board:green:lan2" "switch0" "0x10"
	;;
gl-mt300a|\
gl-mt300n|\
gl-mt750)
	set_wifi_led "$board:wlan"
	;;
hc5661)
	ucidef_set_led_default "system" "system" "$board:blue:system" "1"
	ucidef_set_led_netdev "internet" "internet" "$board:blue:internet" "eth0.2"
	set_wifi_led "$board:blue:wlan2g"
	;;
hc5761)
	ucidef_set_led_default "system" "system" "$board:blue:system" "1"
	ucidef_set_led_netdev "internet" "internet" "$board:blue:internet" "eth0.2"
	set_wifi_led "$board:blue:wlan2g"
	ucidef_set_led_netdev "wifi5g" "wifi5g" "$board:blue:wlan5g" "rai0"
	;;
hc5861)
	ucidef_set_led_default "system" "system" "$board:blue:system" "1"
	ucidef_set_led_netdev "internet" "internet" "$board:blue:internet" "eth0.2"
	set_wifi_led "$board:blue:wlan2g"
	ucidef_set_led_netdev "wifi5g" "wifi5g" "$board:blue:wlan5g" "rai0"
	ucidef_set_led_default "turbo" "turbo" "$board:blue:turbo" "0"
	;;
hg255d)
	set_wifi_led "$board:green:wlan"
	set_usb_led "$board:green:usb"
	ucidef_set_led_netdev "internet" "internet" "$board:green:internet" "eth0.2"
	;;
hpm)
	ucidef_set_led_default "power" "POWER" "$board:orange:power" "1"
	ucidef_set_led_netdev "eth" "ETH" "$board:green:eth" "eth0"
	set_wifi_led "$board:green:wifi"
	;;
ht-tm02)
	ucidef_set_led_netdev "eth" "Ethernet" "$board:green:lan" "eth0"
	set_wifi_led "$board:blue:wlan"
	;;
kn_rc|\
kn_rf|\
kng_rc)
	set_usb_led "$board:green:usb"
	set_wifi_led "$board:green:wifi"
	;;
m2m)
	set_wifi_led "$board:blue:wifi"
	ucidef_set_led_netdev "eth" "Ethernet" "$board:green:wan" "eth0"
	;;
miniembplug)
	set_wifi_led "$board:red:wlan"
	set_usb_led "$board:green:mobile"
	;;
miwifi-mini)
	ucidef_set_led_default "power" "power" "$board:red:status" "1"
	;;
mlw221|\
mlwg2)
	set_wifi_led "$board:blue:wifi"
	ucidef_set_led_default "system" "system" "$board:blue:system" "1"
	;;
mpr-a1|\
mpr-a2)
	set_wifi_led "$board:blue:system"
	;;
mr-102n)
	set_wifi_led "$board:green:wlan"
	set_usb_led "$board:green:usb"
	;;
mr200)
	ucidef_set_led_default "power" "power" "$board:white:power" "1"
	ucidef_set_led_netdev "lan" "lan" "$board:white:lan" "eth0.1"
	ucidef_set_led_netdev "wan" "wan" "$board:white:wan" "usb0"
	set_wifi_led "$board:white:wlan"
	;;
mzk-ex750np)
	ucidef_set_led_default "power" "power" "$board:red:power" "1"
	set_wifi_led "$board:red:wifi"
	;;
na930)
	set_usb_led "$board:blue:status"
	;;
nbg-419n2)
	set_usb_led "$board:green:usb"
	set_wifi_led "rt2800pci-phy0::radio"
	;;
newifi-d1)
	set_usb_led "$board:red:status"
	;;
nw718)
	set_usb_led "$board:amber:usb"
	;;
oy-0001)
	ucidef_set_led_default "power" "power" "$board:green:power" "1"
	set_wifi_led "$board:green:wifi"
	;;
pbr-d1)
	set_usb_led "$board:orange:usb"
	;;
pbr-m1)
	ucidef_set_led_netdev "internet" "internet" "$board:blue:internet" "eth0.2"
	ucidef_set_led_default "power" "power" "$board:blue:power" "1"
	ucidef_set_led_default "sys" "sys" "$board:blue:sys" "1"
	;;
psg1208)
	set_wifi_led "$board:white:wlan2g"
	;;
psg1218)
	ucidef_set_led_netdev "Network" "Network" "$board:blue:status" "eth0"
	ucidef_set_led_default "status" "STATUS" "$board:yellow:status" "0"
	;;
px-4885)
	set_wifi_led "$board:orange:wifi"
	set_usb_led "$board:blue:storage"
	;;
re6500)
	ucidef_set_led_default "power" "power" "$board:white:power" "1"
	ucidef_set_led_default "wifi" "wifi" "$board:orange:wifi" "1"
	;;
rp-n53)
	ucidef_set_led_netdev "eth" "Network" "$board:white:back" "eth0"
	set_wifi_led "$board:blue:wifi"
	;;
rt-n14u)
	ucidef_set_led_default "power" "power" "$board:blue:power" "1"
	ucidef_set_led_netdev "lan" "lan" "$board:blue:lan" eth0.1
	ucidef_set_led_netdev "wan" "wan" "$board:blue:wan" eth0.2
	set_wifi_led "$board:blue:air"
	set_usb_led "$board:blue:usb"
	;;
tew-714tru)
	set_usb_led "$board:red:usb"
	set_wifi_led "$board:green:wifi"
	;;
tiny-ac)
	set_wifi_led "$board:orange:wifi"
	set_usb_led "$board:green:usb"
	;;
vocore)
	ucidef_set_led_netdev "eth" "ETH" "$board:orange:eth" "eth0"
	set_wifi_led "$board:green:status"
	;;
vocore2)
	set_wifi_led "$board:fuchsia:status"
	;;
w502u)
	set_usb_led "$board:blue:usb"
	set_wifi_led "rt2800pci-phy0::radio"
	;;
wcr-150gn)
	set_usb_led "$board:amber:user"
	;;
whr-1166d|\
whr-300hp2|\
whr-600d)
	ucidef_set_led_default "power" "power" "$board:green:power" "1"
	ucidef_set_led_default "router" "router" "$board:green:router" "1"
	;;
wl-wn575a3)
	ucidef_set_rssimon "wlan1" "200000" "1"
	ucidef_set_led_rssi "wifi-low" "wifi-low" "$board:green:wifi-low" "wlan1" "1" "49" "0" "1"
	ucidef_set_led_rssi "wifi-med" "wifi-med" "$board:green:wifi-med" "wlan1" "50" "84" "0" "1"
	ucidef_set_led_rssi "wifi-high" "wifi-high" "$board:green:wifi-high" "wlan1" "85" "100" "0" "1"
	;;
wrh-300cr)
	set_wifi_led "$board:green:wlan"
	ucidef_set_led_netdev "lan" "lan" "$board:green:ethernet" "eth0"
	;;
wndr3700v5)
	ucidef_set_led_default "power" "POWER" "$board:green:power" "0"
	;;
wt3020)
	ucidef_set_led_default "power" "power" "$board:blue:power" "0"
	;;
y1)
	set_usb_led "$board:blue:usb"
	ucidef_set_led_netdev "wifi" "WIFI" "$board:blue:wifi" "wlan1"
	ucidef_set_led_netdev "wifi5g" "WIFI5G" "$board:blue:wifi5g" "wlan0"
	ucidef_set_led_netdev "lan" "LAN" "$board:blue:lan" "eth0.1" "tx rx"
	ucidef_set_led_netdev "wan" "WAN" "$board:blue:internet" "eth0.2" "tx rx"
	;;
y1s)
	set_usb_led "$board:blue:usb"
	ucidef_set_led_netdev "wifi" "WIFI" "$board:yellow:wifi" "wlan1"
	ucidef_set_led_netdev "wifi5g" "WIFI5G" "$board:blue:wifi" "wlan0"
	ucidef_set_led_netdev "wan" "WAN" "$board:blue:internet" "eth0.2" "tx rx"
	;;
zbt-ape522ii)
	ucidef_set_led_netdev "wlan2g4" "wlan1-link" "$board:green:wlan2g4" "wlan1"
	ucidef_set_led_netdev "sys1" "wlan1" "$board:green:sys1" "wlan1" "tx rx"
	ucidef_set_led_netdev "sys2" "wlan0" "$board:green:sys2" "wlan0" "tx rx"
	;;
zbt-cpe102)
	ucidef_set_led_default "power" "power" "$board:green:4g-0" "0"
	;;
zbt-wa05)
	ucidef_set_led_default "power" "power" "$board:blue:power" "1"
	set_wifi_led "$board:blue:air"
	set_usb_led "$board:blue:usb"
	;;
zbt-we826)
	ucidef_set_led_default "power" "power" "$board:green:power" "1"
	set_wifi_led "$board:green:wifi"
	set_usb_led "$board:green:usb"
	;;
zbt-wr8305rt)
	ucidef_set_led_default "power" "power" "$board:green:sys" "1"
	set_usb_led "$board:green:usb"
	set_wifi_led "$board:green:wifi"
	;;
zte-q7)
	set_wifi_led "$board:blue:status"
	;;
youku-yk1)
	ucidef_set_led_default "power" "power" "$board:blue:power" "1"
	set_wifi_led "$board:blue:air"
	set_usb_led "$board:blue:usb"
	;;
esac

board_config_flush

exit 0
