There is a variant of MT7621 which contains only one CPU core instead of 2.
This is not reflected in the config register, so the kernel detects more
physical cores, which leads to a hang on SMP bringup.
Add a hack to detect missing cores.

Signed-off-by: Felix Fietkau <nbd@nbd.name>

--- a/arch/mips/kernel/smp-cps.c
+++ b/arch/mips/kernel/smp-cps.c
@@ -44,6 +44,11 @@ static unsigned core_vpe_count(unsigned
 	return (cfg >> CM_GCR_Cx_CONFIG_PVPE_SHF) + 1;
 }
 
+bool __weak plat_cpu_core_present(int core)
+{
+	return true;
+}
+
 static void __init cps_smp_setup(void)
 {
 	unsigned int ncores, nvpes, core_vpes;
@@ -53,6 +58,8 @@ static void __init cps_smp_setup(void)
 	ncores = mips_cm_numcores();
 	pr_info("VPE topology ");
 	for (c = nvpes = 0; c < ncores; c++) {
+		if (!plat_cpu_core_present(c))
+			continue;
 		core_vpes = core_vpe_count(c);
 		pr_cont("%c%u", c ? ',' : '{', core_vpes);
 
--- a/arch/mips/ralink/mt7621.c
+++ b/arch/mips/ralink/mt7621.c
@@ -20,6 +20,7 @@
 #include <asm/mips-cpc.h>
 #include <asm/mach-ralink/ralink_regs.h>
 #include <asm/mach-ralink/mt7621.h>
+#include <asm/mips-boards/launch.h>
 
 #include <pinmux.h>
 
@@ -163,6 +164,20 @@ void __init ralink_of_remap(void)
 		panic("Failed to remap core resources");
 }
 
+bool plat_cpu_core_present(int core)
+{
+	struct cpulaunch *launch = (struct cpulaunch *)CKSEG0ADDR(CPULAUNCH);
+
+	if (!core)
+		return true;
+	launch += core * 2; /* 2 VPEs per core */
+	if (!(launch->flags & LAUNCH_FREADY))
+		return false;
+	if (launch->flags & (LAUNCH_FGO | LAUNCH_FGONE))
+		return false;
+	return true;
+}
+
 void prom_soc_init(struct ralink_soc_info *soc_info)
 {
 	void __iomem *sysc = (void __iomem *) KSEG1ADDR(MT7621_SYSC_BASE);
